(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT60B2G8HB-48B_A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 52.07 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT60B2G8HB-48B_A"
				(at 52.07 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT60B2G8HB-48B_A"
				(at 52.07 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/3704816.pdf"
				(at 52.07 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DRAM, SDRAM, 16 Gbit, 2G x 8bit, FBGA, 82 Pins"
				(at 52.07 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Micron Technology"
				(at 52.07 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT60B2G8HB-48B:A"
				(at 52.07 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 52.07 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 52.07 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DRAM, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "BGA*10.0x14.5mm*P0.80x0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT60B2G8HB-48B_A_1_1"
				(pin no_connect line
					(at 34.29 -22.86 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "A1")
				)
				(pin input line
					(at 38.1 -55.88 180)
					(length 3.81)
					(name "LBDQ")
					(number "A2")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(name "VSS")
					(number "A3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VPP")
					(number "A4")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 3.81)
					(name "ZQ")
					(number "A8")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "A9")
				)
				(pin input line
					(at 38.1 -58.42 180)
					(length 3.81)
					(name "LBDQS")
					(number "A10")
				)
				(pin no_connect line
					(at 34.29 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "A11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "B2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDQ")
					(number "B3")
				)
				(pin bidirectional line
					(at 38.1 -30.48 180)
					(length 3.81)
					(name "DQ2")
					(number "B4")
				)
				(pin bidirectional line
					(at 38.1 -33.02 180)
					(length 3.81)
					(name "DQ3")
					(number "B8")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "B9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "B10")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C2")
				)
				(pin bidirectional line
					(at 38.1 -25.4 180)
					(length 3.81)
					(name "DQ0")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "DQS_T")
					(number "C4")
				)
				(pin output line
					(at 38.1 -48.26 180)
					(length 3.81)
					(name "TDQS_T")
					(number "C8")
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 3.81)
					(name "DQ1")
					(number "C9")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C10")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "D2")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "DQS_C")
					(number "D4")
				)
				(pin output line
					(at 38.1 -50.8 180)
					(length 3.81)
					(name "TDQS_C")
					(number "D8")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "D10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "E2")
				)
				(pin bidirectional line
					(at 38.1 -35.56 180)
					(length 3.81)
					(name "DQ4")
					(number "E3")
				)
				(pin bidirectional line
					(at 38.1 -40.64 180)
					(length 3.81)
					(name "DQ6")
					(number "E4")
				)
				(pin bidirectional line
					(at 38.1 -43.18 180)
					(length 3.81)
					(name "DQ7")
					(number "E8")
				)
				(pin bidirectional line
					(at 38.1 -38.1 180)
					(length 3.81)
					(name "DQ5")
					(number "E9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "E10")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "F3")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F4")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "F9")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F10")
				)
				(pin input line
					(at 38.1 -2.54 180)
					(length 3.81)
					(name "CA_ODT")
					(number "G2")
				)
				(pin input line
					(at 38.1 -10.16 180)
					(length 3.81)
					(name "MIR")
					(number "G3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "G4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "CK_T")
					(number "G8")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "G9")
				)
				(pin input line
					(at 38.1 -12.7 180)
					(length 3.81)
					(name "TEN")
					(number "G10")
				)
				(pin bidirectional line
					(at 38.1 -5.08 180)
					(length 3.81)
					(name "ALERT_N")
					(number "H2")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "CS_N")
					(number "H4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "CK_C")
					(number "H8")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "H10")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "J2")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "CA4")
					(number "J3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "CA0")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "CA1")
					(number "J8")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "CA5")
					(number "J9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "J10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "CA6")
					(number "K3")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "CA2")
					(number "K4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "CA3")
					(number "K8")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "CA7")
					(number "K9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "K10")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "L2")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "CA8")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "CA9")
					(number "L8")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDQ")
					(number "L10")
				)
				(pin input line
					(at 38.1 -7.62 180)
					(length 3.81)
					(name "CAI")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "CA10")
					(number "M3")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "CA12")
					(number "M4")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "CA13")
					(number "M8")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "CA11")
					(number "M9")
				)
				(pin input line
					(at 38.1 0 180)
					(length 3.81)
					(name "RESET_N")
					(number "M10")
				)
				(pin no_connect line
					(at 34.29 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "N1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N2")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "N8")
				)
				(pin passive line
					(at 38.1 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N10")
				)
				(pin no_connect line
					(at 34.29 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "N11")
				)
			)
			(embedded_fonts no)
		)
)
