(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT62F1G32D4DR-031"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 44.45 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT62F1G32D4DR-031"
				(at 44.45 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT62F1G32D4DR-031"
				(at 44.45 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.micron.com/search-results?searchRequest=%7B%22term%22%3A%22MT62F1G32D4DR-031%22%7D"
				(at 44.45 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DRAM LPDDR5 32G X32 TFBGA"
				(at 44.45 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Micron Technology"
				(at 44.45 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT62F1G32D4DR-031 WT:B"
				(at 44.45 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 44.45 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 44.45 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "BGA, DDR, MEMORY, DRAM"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT62F1G32D4DR-031_1_0"
				(pin no_connect line
					(at 29.21 -3.81 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A1")
				)
				(pin no_connect line
					(at 29.21 -17.78 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(name "VDDQ")
					(number "A3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(name "VSS")
					(number "A5")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(name "VDD2L")
					(number "A6")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(name "VDD2H")
					(number "A7")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "A8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "A9")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "A10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A11")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "A13")
				)
				(pin no_connect line
					(at 29.21 -19.05 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A14")
				)
				(pin no_connect line
					(at 29.21 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A15")
				)
				(pin no_connect line
					(at 29.21 -26.67 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA1")
				)
				(pin no_connect line
					(at 29.21 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA2")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "AA3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA5")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "AA6")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "AA7")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "AA8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "AA9")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "AA10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA11")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "AA13")
				)
				(pin no_connect line
					(at 29.21 -29.21 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA14")
				)
				(pin no_connect line
					(at 29.21 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA15")
				)
				(pin no_connect line
					(at 29.21 -21.59 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B1")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "B2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B4")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "B6")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "B7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "B9")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "B10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B12")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "B14")
				)
				(pin no_connect line
					(at 29.21 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "B15")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 5.08)
					(name "VDD1")
					(number "C1")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "C3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C5")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "C7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "C9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C11")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "C13")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "C15")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D2")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "D4")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D7")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "D8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D10")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "D12")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D14")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E1")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E3")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "E5")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "E7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "E9")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "E11")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E13")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E15")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F1")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F2")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F3")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F4")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "F6")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "F7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "F9")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "F10")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F12")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F13")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F14")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F15")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "G1")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "G2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G11")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G13")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "G14")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "G15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "RESET_n")
					(number "H1")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "H2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H4")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H12")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "H14")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(name "ZQ_A")
					(number "H15")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J1")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "J2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J3")
				)
				(pin no_connect line
					(at 29.21 -1.27 180)
					(length 5.08)
					(hide yes)
					(name "RFU")
					(number "J4")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "J5")
				)
				(pin no_connect line
					(at 29.21 0 180)
					(length 5.08)
					(hide yes)
					(name "RFU")
					(number "J6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J10")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "J11")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J12")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J13")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "J14")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J15")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K1")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K2")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K3")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K4")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K5")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K9")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K10")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K11")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K12")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K13")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K14")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "K15")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L1")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L4")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L5")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "L6")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "L7")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "L8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "L9")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "L10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L11")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L12")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L13")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L14")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L15")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M1")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M2")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M3")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M4")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M5")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M9")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M10")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M11")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M12")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M13")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M14")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "M15")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N1")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "N2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N4")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "N5")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N10")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "N11")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N12")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N13")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "N14")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N15")
				)
				(pin no_connect line
					(at 29.21 1.27 180)
					(length 5.08)
					(hide yes)
					(name "RFU")
					(number "P1")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "P2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P4")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P12")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P13")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "P14")
				)
				(pin no_connect line
					(at 29.21 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "RFU")
					(number "P15")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "R1")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "R2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R5")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R11")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R13")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "R14")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "R15")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "T1")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T2")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "T3")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "T4")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "T6")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "T7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "T9")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "T10")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "T12")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "T13")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T14")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "T15")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U1")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U3")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "U5")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "U7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "U9")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "U11")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U13")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U15")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V2")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "V4")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V7")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "V8")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V10")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "V12")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V14")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "W1")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "W3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W5")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "W7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "W9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W11")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "W13")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "W15")
				)
				(pin no_connect line
					(at 29.21 -24.13 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "Y1")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "Y2")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y4")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "Y6")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "Y7")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y8")
				)
				(pin passive line
					(at 34.29 -6.35 180)
					(length 5.08)
					(hide yes)
					(name "VDD2H")
					(number "Y9")
				)
				(pin passive line
					(at 34.29 -13.97 180)
					(length 5.08)
					(hide yes)
					(name "VDD2L")
					(number "Y10")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y12")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "Y14")
				)
				(pin no_connect line
					(at 29.21 -25.4 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "Y15")
				)
			)
			(symbol "MT62F1G32D4DR-031_1_1")
			(symbol "MT62F1G32D4DR-031_2_0"
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DMI0_A")
					(number "A4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DMI1_A")
					(number "A12")
				)
				(pin passive line
					(at 34.29 0 180)
					(length 5.08)
					(name "RDQS0_t_A")
					(number "B3")
				)
				(pin passive line
					(at 34.29 -25.4 180)
					(length 5.08)
					(name "DQ4_A")
					(number "B5")
				)
				(pin passive line
					(at 34.29 -45.72 180)
					(length 5.08)
					(name "DQ12_A")
					(number "B11")
				)
				(pin passive line
					(at 34.29 -7.62 180)
					(length 5.08)
					(name "RDQS1_t_A")
					(number "B13")
				)
				(pin passive line
					(at 34.29 -17.78 180)
					(length 5.08)
					(name "DQ1_A")
					(number "C2")
				)
				(pin passive line
					(at 34.29 -2.54 180)
					(length 5.08)
					(name "RDQS0_c_A")
					(number "C4")
				)
				(pin passive line
					(at 34.29 -27.94 180)
					(length 5.08)
					(name "DQ5_A")
					(number "C6")
				)
				(pin passive line
					(at 34.29 -48.26 180)
					(length 5.08)
					(name "DQ13_A")
					(number "C10")
				)
				(pin passive line
					(at 34.29 -10.16 180)
					(length 5.08)
					(name "RDQS1_c_A")
					(number "C12")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 5.08)
					(name "DQ9_A")
					(number "C14")
				)
				(pin passive line
					(at 34.29 -15.24 180)
					(length 5.08)
					(name "DQ0_A")
					(number "D1")
				)
				(pin passive line
					(at 34.29 -22.86 180)
					(length 5.08)
					(name "DQ3_A")
					(number "D3")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "WCK0_c_A")
					(number "D5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "WCK1_c_A")
					(number "D11")
				)
				(pin passive line
					(at 34.29 -43.18 180)
					(length 5.08)
					(name "DQ11_A")
					(number "D13")
				)
				(pin passive line
					(at 34.29 -35.56 180)
					(length 5.08)
					(name "DQ8_A")
					(number "D15")
				)
				(pin passive line
					(at 34.29 -20.32 180)
					(length 5.08)
					(name "DQ2_A")
					(number "E2")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "WCK0_t_A")
					(number "E4")
				)
				(pin passive line
					(at 34.29 -30.48 180)
					(length 5.08)
					(name "DQ6_A")
					(number "E6")
				)
				(pin passive line
					(at 34.29 -50.8 180)
					(length 5.08)
					(name "DQ14_A")
					(number "E10")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "WCK1_t_A")
					(number "E12")
				)
				(pin passive line
					(at 34.29 -40.64 180)
					(length 5.08)
					(name "DQ10_A")
					(number "E14")
				)
				(pin passive line
					(at 34.29 -33.02 180)
					(length 5.08)
					(name "DQ7_A")
					(number "F5")
				)
				(pin passive line
					(at 34.29 -53.34 180)
					(length 5.08)
					(name "DQ15_A")
					(number "F11")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "CA0_A")
					(number "G4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "CS1_A")
					(number "G6")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "CA2_A")
					(number "G8")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "CA4_A")
					(number "G10")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "CA6_A")
					(number "G12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "CA1_A")
					(number "H5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "CS0_A")
					(number "H7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "CK_t_A")
					(number "H9")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "CA3_A")
					(number "H11")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "CA5_A")
					(number "H13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "CK_c_A")
					(number "J9")
				)
			)
			(symbol "MT62F1G32D4DR-031_2_1")
			(symbol "MT62F1G32D4DR-031_3_0"
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DMI1_B")
					(number "AA4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DMI0_B")
					(number "AA12")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "CK_c_B")
					(number "N7")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "CA5_B")
					(number "P3")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "CA3_B")
					(number "P5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "CK_t_B")
					(number "P7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "CS0_B")
					(number "P9")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "CA1_B")
					(number "P11")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "CA6_B")
					(number "R4")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "CA4_B")
					(number "R6")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "CA2_B")
					(number "R8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "CS1_B")
					(number "R10")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "CA0_B")
					(number "R12")
				)
				(pin passive line
					(at 34.29 -53.34 180)
					(length 5.08)
					(name "DQ15_B")
					(number "T5")
				)
				(pin passive line
					(at 34.29 -33.02 180)
					(length 5.08)
					(name "DQ7_B")
					(number "T11")
				)
				(pin passive line
					(at 34.29 -40.64 180)
					(length 5.08)
					(name "DQ10_B")
					(number "U2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "WCK1_t_B")
					(number "U4")
				)
				(pin passive line
					(at 34.29 -50.8 180)
					(length 5.08)
					(name "DQ14_B")
					(number "U6")
				)
				(pin passive line
					(at 34.29 -30.48 180)
					(length 5.08)
					(name "DQ6_B")
					(number "U10")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "WCK0_t_B")
					(number "U12")
				)
				(pin passive line
					(at 34.29 -20.32 180)
					(length 5.08)
					(name "DQ2_B")
					(number "U14")
				)
				(pin passive line
					(at 34.29 -35.56 180)
					(length 5.08)
					(name "DQ8_B")
					(number "V1")
				)
				(pin passive line
					(at 34.29 -43.18 180)
					(length 5.08)
					(name "DQ11_B")
					(number "V3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "WCK1_c_B")
					(number "V5")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "WCK0_c_B")
					(number "V11")
				)
				(pin passive line
					(at 34.29 -22.86 180)
					(length 5.08)
					(name "DQ3_B")
					(number "V13")
				)
				(pin passive line
					(at 34.29 -15.24 180)
					(length 5.08)
					(name "DQ0_B")
					(number "V15")
				)
				(pin passive line
					(at 34.29 -38.1 180)
					(length 5.08)
					(name "DQ9_B")
					(number "W2")
				)
				(pin passive line
					(at 34.29 -10.16 180)
					(length 5.08)
					(name "RDQS1_c_B")
					(number "W4")
				)
				(pin passive line
					(at 34.29 -48.26 180)
					(length 5.08)
					(name "DQ13_B")
					(number "W6")
				)
				(pin passive line
					(at 34.29 -27.94 180)
					(length 5.08)
					(name "DQ5_B")
					(number "W10")
				)
				(pin passive line
					(at 34.29 -2.54 180)
					(length 5.08)
					(name "RDQS0_c_B")
					(number "W12")
				)
				(pin passive line
					(at 34.29 -17.78 180)
					(length 5.08)
					(name "DQ1_B")
					(number "W14")
				)
				(pin passive line
					(at 34.29 -7.62 180)
					(length 5.08)
					(name "RDQS1_t_B")
					(number "Y3")
				)
				(pin passive line
					(at 34.29 -45.72 180)
					(length 5.08)
					(name "DQ12_B")
					(number "Y5")
				)
				(pin passive line
					(at 34.29 -25.4 180)
					(length 5.08)
					(name "DQ4_B")
					(number "Y11")
				)
				(pin passive line
					(at 34.29 0 180)
					(length 5.08)
					(name "RDQS0_t_B")
					(number "Y13")
				)
			)
			(symbol "MT62F1G32D4DR-031_3_1")
			(embedded_fonts no)
		)
)
