(footprint "BGA-170-100_18x14mm_Layout17x10_P1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Uses depopulated JEDEC-MO-304B")
	(property "Reference" "REF**"
		(at 0 -9.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-170-100_18x14mm_Layout17x10_P1mm"
		(at 0 10.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -7.4 12.3 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -7.4 13.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -7.4 14.7 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -4.5 -8)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -3.5 -8)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 3.499 -8)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at 4.499 -8)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -4.5 -7)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 4.499 -7)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -3.5 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -2.5 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -1.5 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -0.5 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at 0.499 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at 1.499 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 2.499 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 3.499 -5)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -3.5 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -2.5 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -1.5 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -0.5 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at 0.499 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at 1.499 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 2.499 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 3.499 -4)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -3.5 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -2.5 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -1.5 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -0.5 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 0.499 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 1.499 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 2.499 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 3.499 -3)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -3.5 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -2.5 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -1.5 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at -0.5 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at 0.499 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 1.499 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 2.499 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 3.499 -2)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -3.5 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -2.5 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -1.5 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -0.5 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at 0.499 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 1.499 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 2.499 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 3.499 -1)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -3.5 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -2.5 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -1.5 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -0.5 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at 0.499 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at 1.499 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 2.499 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 3.499 0)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -3.5 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -2.5 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -1.5 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -0.5 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K6" smd circle
		(at 0.499 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at 1.499 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 2.499 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 3.499 0.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -3.5 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -2.5 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -1.5 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -0.5 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L6" smd circle
		(at 0.499 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at 1.499 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at 2.499 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at 3.499 1.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -3.5 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -2.5 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -1.5 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M5" smd circle
		(at -0.5 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M6" smd circle
		(at 0.499 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M7" smd circle
		(at 1.499 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at 2.499 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at 3.499 2.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -3.5 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -2.5 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -1.5 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N5" smd circle
		(at -0.5 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N6" smd circle
		(at 0.499 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N7" smd circle
		(at 1.499 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at 2.499 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at 3.499 3.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -3.5 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -2.5 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd circle
		(at -1.5 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P5" smd circle
		(at -0.5 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P6" smd circle
		(at 0.499 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P7" smd circle
		(at 1.499 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P8" smd circle
		(at 2.499 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P9" smd circle
		(at 3.499 4.999)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -4.5 6.998)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T10" smd circle
		(at 4.499 6.998)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -4.5 7.998)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -3.5 7.998)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U9" smd circle
		(at 3.499 7.998)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U10" smd circle
		(at 4.499 7.998)
		(size 0.37 0.37)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_mtfc16gapalna_ait.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
