(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MTFC16GAPALNA-AIT"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MTFC16GAPALNA-AIT"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MTFC16GAPALNA-AIT"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/671/micron_technology_mict-s-a0006806196-1-1759129.pdf"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Managed NAND Flash Serial e-MMC 3.3V 128G-bit 128G/32G/16G x 1/4-bit/8-bit Automotive AEC-Q100 100-Pin TBGA Tray"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Micron Technology"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MTFC16GAPALNA-AIT"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, FLASH, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MTFC16GAPALNA-AIT_0_0"
				(pin no_connect line
					(at 7.62 1.27 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A1")
				)
				(pin no_connect line
					(at 7.62 -1.27 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin no_connect line
					(at 7.62 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A9")
				)
				(pin no_connect line
					(at 7.62 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A10")
				)
				(pin no_connect line
					(at 7.62 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B1")
				)
				(pin no_connect line
					(at 7.62 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B10")
				)
				(pin no_connect line
					(at 12.7 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "VSF1")
					(number "D2")
				)
				(pin no_connect line
					(at 12.7 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "VSF2")
					(number "D3")
				)
				(pin no_connect line
					(at 12.7 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "VSF3")
					(number "D4")
				)
				(pin no_connect line
					(at 12.7 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "VSF4")
					(number "D5")
				)
				(pin no_connect line
					(at 12.7 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "VSF5")
					(number "D6")
				)
				(pin no_connect line
					(at 12.7 -21.59 0)
					(length 2.54)
					(hide yes)
					(name "VSF6")
					(number "D7")
				)
				(pin no_connect line
					(at 12.7 -24.13 0)
					(length 2.54)
					(hide yes)
					(name "VSF7")
					(number "D8")
				)
				(pin no_connect line
					(at 12.7 -26.67 0)
					(length 2.54)
					(hide yes)
					(name "VSF8")
					(number "D9")
				)
				(pin no_connect line
					(at 8.89 1.27 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E2")
				)
				(pin no_connect line
					(at 8.89 -1.27 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E3")
				)
				(pin power_in line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "VDDIM")
					(number "E4")
				)
				(pin no_connect line
					(at 8.89 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E5")
				)
				(pin no_connect line
					(at 8.89 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E6")
				)
				(pin no_connect line
					(at 8.89 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E7")
				)
				(pin no_connect line
					(at 8.89 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E8")
				)
				(pin no_connect line
					(at 8.89 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E9")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "VCC")
					(number "F2")
				)
				(pin power_in line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "VSSQ")
					(number "H2")
				)
				(pin power_in line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "VCCQ")
					(number "H3")
				)
				(pin no_connect line
					(at 8.89 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "H4")
				)
				(pin no_connect line
					(at 8.89 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "H5")
				)
				(pin no_connect line
					(at 8.89 -21.59 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "H6")
				)
				(pin no_connect line
					(at 8.89 -24.13 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "H7")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "H8")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "H9")
				)
				(pin no_connect line
					(at 8.89 -26.67 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "J2")
				)
				(pin no_connect line
					(at 10.16 1.27 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "J3")
				)
				(pin no_connect line
					(at 10.16 -1.27 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "J4")
				)
				(pin no_connect line
					(at 10.16 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "J6")
				)
				(pin no_connect line
					(at 10.16 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "J7")
				)
				(pin no_connect line
					(at 10.16 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "J8")
				)
				(pin no_connect line
					(at 10.16 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "J9")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DAT0")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DAT2")
					(number "K3")
				)
				(pin no_connect line
					(at 10.16 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "K4")
				)
				(pin output line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "DS")
					(number "K5")
				)
				(pin no_connect line
					(at 10.16 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "K6")
				)
				(pin no_connect line
					(at 10.16 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "K7")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DAT5")
					(number "K8")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DAT7")
					(number "K9")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "L2")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "L3")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "L4")
				)
				(pin no_connect line
					(at 10.16 -21.59 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "L5")
				)
				(pin no_connect line
					(at 10.16 -24.13 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "L6")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "L7")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "L8")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "L9")
				)
				(pin no_connect line
					(at 10.16 -26.67 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "M2")
				)
				(pin no_connect line
					(at 11.43 1.27 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "M3")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "M4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RST_N")
					(number "M5")
				)
				(pin no_connect line
					(at 11.43 -1.27 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "M6")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "M7")
				)
				(pin no_connect line
					(at 11.43 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "M8")
				)
				(pin no_connect line
					(at 11.43 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "M9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DAT1")
					(number "N2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DAT3")
					(number "N3")
				)
				(pin no_connect line
					(at 11.43 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "N4")
				)
				(pin no_connect line
					(at 11.43 -11.43 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "N5")
				)
				(pin no_connect line
					(at 11.43 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "N6")
				)
				(pin no_connect line
					(at 11.43 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "N7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DAT4")
					(number "N8")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DAT6")
					(number "N9")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "P2")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "P3")
				)
				(pin no_connect line
					(at 11.43 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "P4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CMD")
					(number "P5")
				)
				(pin input clock
					(at 0 0 0)
					(length 2.54)
					(name "CLK")
					(number "P6")
				)
				(pin no_connect line
					(at 11.43 -21.59 0)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "P7")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "P8")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "P9")
				)
				(pin no_connect line
					(at 7.62 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "T1")
				)
				(pin no_connect line
					(at 7.62 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "T10")
				)
				(pin no_connect line
					(at 7.62 -19.05 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "U1")
				)
				(pin no_connect line
					(at 7.62 -21.59 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "U2")
				)
				(pin no_connect line
					(at 7.62 -24.13 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "U9")
				)
				(pin no_connect line
					(at 7.62 -26.67 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "U10")
				)
			)
			(symbol "MTFC16GAPALNA-AIT_1_1"
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "F3")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "F4")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "F5")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "F6")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "F7")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "F8")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "F9")
				)
				(pin power_in line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "VSS")
					(number "G2")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G3")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G4")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G6")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G7")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G9")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "J5")
				)
			)
			(embedded_fonts no)
		)
)
