(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MX25L3233FM1I-08Q"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MX25L3233FM1I-08Q"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MX25L3233FM1I-08Q"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/819/MX25L3233F_2c_3V_2c_32Mb_2c_v1_7-3371049.pdf"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FLASH - NOR Memory IC 32Mbit SPI133 MHz 8-SOIC"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MX25L3233FM1I-08Q"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Macronix"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, FLASH, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MX25L3233FM1I-08Q_0_1")
			(symbol "MX25L3233FM1I-08Q_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SO/IO1")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{WP}/SIO2")
					(number "3")
				)
				(pin power_in line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "SI/IO0")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCLK")
					(number "6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{HOLD}/SIO3")
					(number "7")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
