(footprint "WLCSP-8_1.24x1.75mm_Layout3-2-3_P0.35x0.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "WLCSP-8_1.24x1.75mm_Layout3-2-3_P0.35x0.4mm"
		(at 0 2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -0.75 15.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -0.75 16.6 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -0.75 17.8 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.351 -0.402)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at 0.349 -0.402)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at 0 -0.202)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.351 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at 0.349 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at 0 0.2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -0.351 0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at 0.349 0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_mx25r8035fbdil0.glb"
		(offset
			(xyz 0 0 -0.02)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
