(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "N25Q032A13EF440F"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "N25Q032A13EF440F"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "N25Q032A13EF440F"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/Micron_Datasheet_N25Q032A_RevJ.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FLASH - NOR Memory IC 32Mbit SPI 108MHz 2.7V-3.6V VDFPN8"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "N25Q032A13EF440F "
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Alliance Memory"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, FLASH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "N25Q032A13EF440F_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{S}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DQ1")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{W}")
					(number "3")
					(alternate "DQ2" bidirectional line)
					(alternate "V_{PP}" power_in line)
				)
				(pin power_in line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "V_{SS}")
					(number "4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "DQ0")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "C")
					(number "6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{HOLD}")
					(number "7")
					(alternate "DQ3" bidirectional line)
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "V_{CC}")
					(number "8")
				)
				(pin power_in line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
