(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NB3L202KMN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NB3L202KMN"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NB3L202KMN"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/308/1/NB3L202K_D-2316569.pdf"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fanout Buffer, 2 Outputs, 2.97V to 3.63 V, QFN-16, -40°C to 85°C"
				(at 55.88 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NB3L202KMNTXG"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CLOCK, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "QFNN16_NB3L202_ONS QFNN16_NB3L202_ONS-M QFNN16_NB3L202_ONS-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NB3L202KMN_1_1"
				(pin power_in line
					(at 19.05 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "CLK_{IN}+")
					(number "2")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "CLK_{IN}-")
					(number "3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
				(pin passive line
					(at 19.05 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "GND_O")
					(number "5")
				)
				(pin output line
					(at 19.05 -8.89 180)
					(length 2.54)
					(name "DIF_{1}-")
					(number "6")
				)
				(pin output line
					(at 19.05 -6.35 180)
					(length 2.54)
					(name "DIF_{1}+")
					(number "7")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD_O")
					(number "8")
				)
				(pin passive line
					(at 19.05 -19.05 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin input line
					(at 19.05 -12.7 180)
					(length 2.54)
					(name "I_{REF}")
					(number "10")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{OE0}")
					(number "11")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "~{OE1}")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_O")
					(number "13")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "DIF_{0}+")
					(number "14")
				)
				(pin output line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "DIF_{0}-")
					(number "15")
				)
				(pin power_in line
					(at 19.05 -21.59 180)
					(length 2.54)
					(name "GND_O")
					(number "16")
				)
				(pin power_in line
					(at 19.05 -16.51 180)
					(length 2.54)
					(name "EPAD")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
