(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NRF24L01P-T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NRF24L01P-T"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NRF24L01P-T"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/297/nRF24L01P-1187709.pdf"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver IC, Single Chip 2.4GHz Transceiver"
				(at 38.1 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nordic Semiconductor"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NRF24L01P-T"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RF, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NRF24L01P-T_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CE")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CSN")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCK")
					(number "3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "MOSI")
					(number "4")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "MISO")
					(number "5")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "IRQ")
					(number "6")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "7")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "8")
				)
				(pin output line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "XC2")
					(number "9")
				)
				(pin input line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "XC1")
					(number "10")
				)
				(pin power_out line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "VDD_PA")
					(number "11")
				)
				(pin output line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "ANT1")
					(number "12")
				)
				(pin output line
					(at 22.86 0 180)
					(length 2.54)
					(name "ANT2")
					(number "13")
				)
				(pin power_in line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "VSS")
					(number "14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "15")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "IREF")
					(number "16")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "17")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "18")
				)
				(pin power_out line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DVDD")
					(number "19")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "20")
				)
				(pin no_connect line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "EP")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
