(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NRF52832-QFAA-G-R7"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NRF52832-QFAA-G-R7"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NRF52832-QFAA-G-R7"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/nRF52832_PS_v1.9/resource/nRF52832_PS_v1.9.pdf"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF Transceiver, 2.36GHz to 2.5GHz, FSK, 2Mbps, 4dBm out, -89dBm in, 1.7V to 3.6V, QFN-48"
				(at 53.34 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nordic Semiconductor"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NRF52832-QFAA-G-R7"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, RF, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NRF52832-QFAA-G-R7_1_1"
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DEC1")
					(number "1")
				)
				(pin passive line
					(at 40.64 -3.81 180)
					(length 2.54)
					(name "P0.00")
					(number "2")
					(alternate "XL1" passive line)
				)
				(pin passive line
					(at 40.64 -6.35 180)
					(length 2.54)
					(name "P0.01")
					(number "3")
					(alternate "XL2" passive line)
				)
				(pin passive line
					(at 40.64 -8.89 180)
					(length 2.54)
					(name "P0.02")
					(number "4")
					(alternate "AIN0" passive line)
				)
				(pin passive line
					(at 40.64 -11.43 180)
					(length 2.54)
					(name "P0.03")
					(number "5")
					(alternate "AIN1" passive line)
				)
				(pin passive line
					(at 40.64 -13.97 180)
					(length 2.54)
					(name "P0.04")
					(number "6")
					(alternate "AIN2" passive line)
				)
				(pin passive line
					(at 40.64 -16.51 180)
					(length 2.54)
					(name "P0.05")
					(number "7")
					(alternate "AIN3" passive line)
				)
				(pin passive line
					(at 40.64 -19.05 180)
					(length 2.54)
					(name "P0.06")
					(number "8")
				)
				(pin passive line
					(at 40.64 -21.59 180)
					(length 2.54)
					(name "P0.07")
					(number "9")
				)
				(pin passive line
					(at 40.64 -24.13 180)
					(length 2.54)
					(name "P0.08")
					(number "10")
				)
				(pin passive line
					(at 40.64 -26.67 180)
					(length 2.54)
					(name "NFC1/P0.09")
					(number "11")
					(alternate "P0.09" passive line)
				)
				(pin passive line
					(at 40.64 -29.21 180)
					(length 2.54)
					(name "NFC2/P0.10")
					(number "12")
					(alternate "P0.10" passive line)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "13")
				)
				(pin passive line
					(at 40.64 -31.75 180)
					(length 2.54)
					(name "P0.11")
					(number "14")
				)
				(pin passive line
					(at 40.64 -34.29 180)
					(length 2.54)
					(name "P0.12")
					(number "15")
				)
				(pin passive line
					(at 40.64 -36.83 180)
					(length 2.54)
					(name "P0.13")
					(number "16")
				)
				(pin passive line
					(at 40.64 -39.37 180)
					(length 2.54)
					(name "P0.14")
					(number "17")
					(alternate "TRACEDATA[3]" passive line)
				)
				(pin passive line
					(at 40.64 -41.91 180)
					(length 2.54)
					(name "P0.15")
					(number "18")
					(alternate "TRACEDATA[2]" passive line)
				)
				(pin passive line
					(at 40.64 -44.45 180)
					(length 2.54)
					(name "P0.16")
					(number "19")
					(alternate "TRACEDATA[1]" passive line)
				)
				(pin passive line
					(at 40.64 -46.99 180)
					(length 2.54)
					(name "P0.17")
					(number "20")
				)
				(pin passive line
					(at 40.64 -49.53 180)
					(length 2.54)
					(name "P0.18")
					(number "21")
					(alternate "SWO" passive line)
					(alternate "TRACEDATA[0]" passive line)
				)
				(pin passive line
					(at 40.64 -52.07 180)
					(length 2.54)
					(name "P0.19")
					(number "22")
				)
				(pin passive line
					(at 40.64 -54.61 180)
					(length 2.54)
					(name "P0.20")
					(number "23")
					(alternate "TRACECLK" passive line)
				)
				(pin passive line
					(at 40.64 -57.15 180)
					(length 2.54)
					(name "P0.21")
					(number "24")
					(alternate "NRESET" passive line)
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "SWDCLK")
					(number "25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "SWDIO")
					(number "26")
				)
				(pin passive line
					(at 40.64 -59.69 180)
					(length 2.54)
					(name "P0.22")
					(number "27")
				)
				(pin passive line
					(at 40.64 -62.23 180)
					(length 2.54)
					(name "P0.23")
					(number "28")
				)
				(pin passive line
					(at 40.64 -64.77 180)
					(length 2.54)
					(name "P0.24")
					(number "29")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 2.54)
					(name "ANT")
					(number "30")
				)
				(pin power_in line
					(at 0 -80.01 0)
					(length 2.54)
					(name "VSS")
					(number "31")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DEC2")
					(number "32")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DEC3")
					(number "33")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "XC1")
					(number "34")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "XC2")
					(number "35")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "36")
				)
				(pin passive line
					(at 40.64 -67.31 180)
					(length 2.54)
					(name "P0.25")
					(number "37")
				)
				(pin passive line
					(at 40.64 -69.85 180)
					(length 2.54)
					(name "P0.26")
					(number "38")
				)
				(pin passive line
					(at 40.64 -72.39 180)
					(length 2.54)
					(name "P0.27")
					(number "39")
				)
				(pin passive line
					(at 40.64 -74.93 180)
					(length 2.54)
					(name "P0.28")
					(number "40")
					(alternate "AIN4" passive line)
				)
				(pin passive line
					(at 40.64 -77.47 180)
					(length 2.54)
					(name "P0.29")
					(number "41")
					(alternate "AIN5" passive line)
				)
				(pin passive line
					(at 40.64 -80.01 180)
					(length 2.54)
					(name "P0.30")
					(number "42")
					(alternate "AIN6" passive line)
				)
				(pin passive line
					(at 40.64 -82.55 180)
					(length 2.54)
					(name "P0.31")
					(number "43")
					(alternate "AIN7" passive line)
				)
				(pin no_connect line
					(at 2.54 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "44")
				)
				(pin passive line
					(at 0 -80.01 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "45")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DEC4")
					(number "46")
				)
				(pin power_out line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DCC")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 2.54)
					(name "EP")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
