(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NRF52832-QFAA-R"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NRF52832-QFAA-R"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NRF52832-QFAA-R"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://infocenter.nordicsemi.com/pdf/nRF52832_PS_v1.4.pdf"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF Transceiver, 2.5 GHz, 2 MBPS, QFN-48, -40 °C to 85 °C"
				(at 53.34 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nordic Semiconductor"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NRF52832-QFAA-R"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NRF52832-QFAA-R_1_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DEC1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 2.54)
					(name "P0.00/XL1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 2.54)
					(name "P0.01/XL2")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 2.54)
					(name "P0.02/AIN0")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 2.54)
					(name "P0.03/AIN1")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 2.54)
					(name "P0.04/AIN2")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 2.54)
					(name "P0.05/AIN3")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 2.54)
					(name "P0.06")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 2.54)
					(name "P0.07")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 2.54)
					(name "P0.08")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "NFC1/P0.09")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "NFC2/P0.10")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "P0.11")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "P0.12")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "P0.13")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "P0.14/TRACEDATA_3")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "P0.15/TRACEDATA_2")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "P0.16/TRACEDATA_1")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "P0.17")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "P0.18/TRACEDATA_0/SWO")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "P0.19")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "P0.20")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "P0.21/nRESET")
					(number "24")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SWDCLK")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SWDIO")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "P0.22")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "P0.23")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "P0.24")
					(number "29")
				)
				(pin bidirectional line
					(at 38.1 0 180)
					(length 2.54)
					(name "ANT")
					(number "30")
				)
				(pin power_in line
					(at 38.1 -104.14 180)
					(length 2.54)
					(name "VSS")
					(number "31")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DEC2")
					(number "32")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DEC3")
					(number "33")
				)
				(pin input line
					(at 38.1 -86.36 180)
					(length 2.54)
					(name "XC1")
					(number "34")
				)
				(pin input line
					(at 38.1 -93.98 180)
					(length 2.54)
					(name "XC2")
					(number "35")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "P0.25")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "P0.26")
					(number "38")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "P0.27")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "P0.28/AIN4")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "P0.29/AIN5")
					(number "41")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "P0.30/AIN6")
					(number "42")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "P0.31/AIN7")
					(number "43")
				)
				(pin no_connect line
					(at 35.56 -83.82 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "44")
				)
				(pin passive line
					(at 38.1 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "45")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DEC4")
					(number "46")
				)
				(pin power_out line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DCC")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin power_in line
					(at 38.1 -101.6 180)
					(length 2.54)
					(name "VSS/PAD")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
