(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nRF52833-QIAA-R"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "nRF52833-QIAA-R"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "nRF52833-QIAA-R"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/297/nRF52833_SoC_Product_Brief-1815256.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF System on Chip, Bluetooth, Zigbee, NFC,  2.4 GHz, 2 MBPS, aQFN-73"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nordic Semiconductor"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "nRF52833-QIAA-R"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RF, ARM, SMT, SOC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "nRF52833-QIAA-R_1_1"
				(pin power_in line
					(at 0 -80.01 0)
					(length 5.08)
					(name "VSS")
					(number "74")
				)
				(pin bidirectional line
					(at 43.18 -82.55 180)
					(length 5.08)
					(name "P0.31")
					(number "A8")
					(alternate "AIN7" passive line)
				)
				(pin bidirectional line
					(at 43.18 -77.47 180)
					(length 5.08)
					(name "P0.29")
					(number "A10")
					(alternate "AIN5" passive line)
				)
				(pin bidirectional line
					(at 43.18 -8.89 180)
					(length 5.08)
					(name "P0.02")
					(number "A12")
					(alternate "AIN0" passive line)
				)
				(pin bidirectional line
					(at 43.18 -52.07 180)
					(length 5.08)
					(name "P0.19")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "P1.05")
					(number "A16")
				)
				(pin bidirectional line
					(at 43.18 -67.31 180)
					(length 5.08)
					(name "P0.25")
					(number "A20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD")
					(number "A22")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 5.08)
					(name "XC2")
					(number "A23")
				)
				(pin input clock
					(at 0 -33.02 0)
					(length 5.08)
					(name "SWDCLK")
					(number "AA24")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "DECUSB")
					(number "AC5")
				)
				(pin bidirectional line
					(at 43.18 -39.37 180)
					(length 5.08)
					(name "P0.14")
					(number "AC9")
				)
				(pin bidirectional line
					(at 43.18 -44.45 180)
					(length 5.08)
					(name "P0.16")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -49.53 180)
					(length 5.08)
					(name "P0.18")
					(number "AC13")
					(alternate "NRESET" passive line)
				)
				(pin bidirectional line
					(at 43.18 -57.15 180)
					(length 5.08)
					(name "P0.21")
					(number "AC17")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "SWDIO")
					(number "AC24")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VBUS")
					(number "AD2")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "D-")
					(number "AD4")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "D+")
					(number "AD6")
				)
				(pin bidirectional line
					(at 43.18 -36.83 180)
					(length 5.08)
					(name "P0.13")
					(number "AD8")
				)
				(pin bidirectional line
					(at 43.18 -41.91 180)
					(length 5.08)
					(name "P0.15")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -46.99 180)
					(length 5.08)
					(name "P0.17")
					(number "AD12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -54.61 180)
					(length 5.08)
					(name "P0.20")
					(number "AD16")
				)
				(pin bidirectional line
					(at 43.18 -59.69 180)
					(length 5.08)
					(name "P0.22")
					(number "AD18")
				)
				(pin bidirectional line
					(at 43.18 -64.77 180)
					(length 5.08)
					(name "P0.24")
					(number "AD20")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "P1.00")
					(number "AD22")
					(alternate "TRACEDATA0" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "AD23")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "B1")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "DCC")
					(number "B3")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "DEC4")
					(number "B5")
				)
				(pin passive line
					(at 0 -80.01 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B7")
				)
				(pin bidirectional line
					(at 43.18 -80.01 180)
					(length 5.08)
					(name "P0.30")
					(number "B9")
					(alternate "AIN6" passive line)
				)
				(pin bidirectional line
					(at 43.18 -74.93 180)
					(length 5.08)
					(name "P0.28")
					(number "B11")
					(alternate "AIN4" passive line)
				)
				(pin bidirectional line
					(at 43.18 -11.43 180)
					(length 5.08)
					(name "P0.03")
					(number "B13")
					(alternate "AIN1" passive line)
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "P1.03")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -62.23 180)
					(length 5.08)
					(name "P0.23")
					(number "B17")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 5.08)
					(name "XC1")
					(number "B24")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DEC1")
					(number "C1")
				)
				(pin bidirectional line
					(at 43.18 -3.81 180)
					(length 5.08)
					(name "P0.00")
					(number "D2")
					(alternate "XL1" passive line)
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DEC3")
					(number "D23")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 5.08)
					(name "DEC6")
					(number "E24")
				)
				(pin bidirectional line
					(at 43.18 -6.35 180)
					(length 5.08)
					(name "P0.01")
					(number "F2")
					(alternate "XL2" passive line)
				)
				(pin power_in line
					(at 0 -82.55 0)
					(length 5.08)
					(name "VSS_PA")
					(number "F23")
				)
				(pin bidirectional line
					(at 43.18 -69.85 180)
					(length 5.08)
					(name "P0.26")
					(number "G1")
				)
				(pin bidirectional line
					(at 43.18 -72.39 180)
					(length 5.08)
					(name "P0.27")
					(number "H2")
				)
				(pin bidirectional line
					(at 43.18 0 180)
					(length 5.08)
					(name "ANT")
					(number "H23")
				)
				(pin bidirectional line
					(at 43.18 -13.97 180)
					(length 5.08)
					(name "P0.04")
					(number "J1")
					(alternate "AIN2" passive line)
				)
				(pin bidirectional line
					(at 43.18 -29.21 180)
					(length 5.08)
					(name "P0.10")
					(number "J24")
					(alternate "NFC2" passive line)
				)
				(pin bidirectional line
					(at 43.18 -16.51 180)
					(length 5.08)
					(name "P0.05")
					(number "K2")
					(alternate "AIN3" passive line)
				)
				(pin bidirectional line
					(at 43.18 -19.05 180)
					(length 5.08)
					(name "P0.06")
					(number "L1")
				)
				(pin bidirectional line
					(at 43.18 -26.67 180)
					(length 5.08)
					(name "P0.09")
					(number "L24")
					(alternate "NFC1" passive line)
				)
				(pin bidirectional line
					(at 43.18 -21.59 180)
					(length 5.08)
					(name "P0.07")
					(number "M2")
					(alternate "TRACECLK" passive line)
				)
				(pin bidirectional line
					(at 43.18 -24.13 180)
					(length 5.08)
					(name "P0.08")
					(number "N1")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "DEC5")
					(number "N24")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "P1.08")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "P1.07")
					(number "P23")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "P1.09")
					(number "R1")
					(alternate "TRACEDATA3" passive line)
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "P1.06")
					(number "R24")
				)
				(pin bidirectional line
					(at 43.18 -31.75 180)
					(length 5.08)
					(name "P0.11")
					(number "T2")
					(alternate "TRACEDATA2" passive line)
				)
				(pin bidirectional line
					(at 43.18 -34.29 180)
					(length 5.08)
					(name "P0.12")
					(number "U1")
					(alternate "TRACEDATA1" passive line)
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "P1.04")
					(number "U24")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "P1.02")
					(number "W24")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDDH")
					(number "Y2")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "P1.01")
					(number "Y23")
				)
			)
			(embedded_fonts no)
		)
)
