(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NRF8001-R2Q32-T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NRF8001-R2Q32-T"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NRF8001-R2Q32-T"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/297/NRSAS00035_1-2559952.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver IC, Single-chip Bluetooth® low energy solution"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nordic Semiconductor"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NRF8001-R2Q32-T"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SOC, IC, BLUETOOTH, RF, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NRF8001-R2Q32-T_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DEC1")
					(number "2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DEC2")
					(number "3")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "XL2")
					(number "4")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "XL1")
					(number "5")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 2.54)
					(name "ACTIVE")
					(number "6")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 2.54)
					(name "TXD")
					(number "7")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "9")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "RXD")
					(number "10")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SCK")
					(number "11")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "~{REQN}")
					(number "12")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "MOSI")
					(number "13")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "MISO")
					(number "14")
				)
				(pin no_connect line
					(at 27.94 -35.56 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "~{RDYN}")
					(number "16")
				)
				(pin power_in line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "VSS")
					(number "17")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "18")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{RESET}")
					(number "19")
				)
				(pin power_out line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "VDD_PA")
					(number "20")
				)
				(pin input line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "ANT1")
					(number "21")
				)
				(pin input line
					(at 30.48 0 180)
					(length 2.54)
					(name "ANT2")
					(number "22")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "23")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDD")
					(number "24")
				)
				(pin passive line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "IREF")
					(number "25")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "26")
				)
				(pin output line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "XC2")
					(number "27")
				)
				(pin input line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "XC1")
					(number "28")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "29")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "30")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "31")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DCC")
					(number "32")
				)
				(pin power_in line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "EP_GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
