(footprint "X2SON8_1.4x1x0.32mm_P0.35mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "X2SON8_1.4x1x0.32mm_P0.35mm"
		(at 0 1.929 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -0.95 3.929 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -0.95 5.129 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -0.95 6.329 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.43 -0.526 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.43 -0.175 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.43 0.175 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.43 0.526 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.43 0.526 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.43 0.175 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.43 -0.175 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.43 -0.526 270)
		(size 0.17 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_nts0302jkz.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
