(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "NVT2008BQ,115"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "NVT2008BQ,115"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "NVT2008BQ,115"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/NVT2008_NVT2010.pdf"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Bidirectional Voltage Level Translator, 8 Inputs, 1.5ns, 1.8V to 5.5V, DHVQFN-20"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "NVT2008BQ,115"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LEVEL-SHIFTER, IC, LOGIC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "NVT2008BQ,115_0_1")
			(symbol "NVT2008BQ,115_1_1"
				(pin power_in line
					(at 0 -31.75 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VREFA")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A1")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A2")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A3")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A4")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A5")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A6")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A7")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "A8")
					(number "10")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "B8")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "B7")
					(number "12")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "B6")
					(number "13")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "B5")
					(number "14")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "B4")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "B3")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "B2")
					(number "17")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "B1")
					(number "18")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "VREFB")
					(number "19")
				)
				(pin input line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "EN")
					(number "20")
				)
				(pin power_in line
					(at 0 -29.21 0)
					(length 2.54)
					(name "EP")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
