(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "OPA4H199-SEP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "OPA4H199-SEP"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "OPA4H199-SEP"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/opa4h199-sep.pdf"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation Hardened, Rail-to-Rail Input/Output, Low Offset Voltage, Low Noise Op Amp in Space Enhanced Plastic"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "OPA4H199MDYYTSEP"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, AMP, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "OPA4H199-SEP_1_1"
				(text "+"
					(at 2.54 -1.016 0)
				)
				(text "-"
					(at 2.54 -3.302 0)
				)
				(pin output line
					(at 10.16 -1.27 180)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "3")
				)
			)
			(symbol "OPA4H199-SEP_2_1"
				(text "+"
					(at 2.54 -1.016 0)
				)
				(text "-"
					(at 2.54 -3.302 0)
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin output line
					(at 10.16 -1.27 180)
					(length 2.54)
					(name "")
					(number "7")
				)
			)
			(symbol "OPA4H199-SEP_3_1"
				(text "+"
					(at 2.54 -1.016 0)
				)
				(text "-"
					(at 2.54 -3.302 0)
				)
				(pin output line
					(at 10.16 -1.27 180)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "10")
				)
			)
			(symbol "OPA4H199-SEP_4_1"
				(text "+"
					(at 2.54 -1.016 0)
				)
				(text "-"
					(at 2.54 -3.302 0)
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "12")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin output line
					(at 10.16 -1.27 180)
					(length 2.54)
					(name "")
					(number "14")
				)
			)
			(symbol "OPA4H199-SEP_5_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V-")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
