(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "P3S0210BQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "P3S0210BQ"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "P3S0210BQ"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/P3S0210BQ.pdf"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I3C Multiplexer, 2 Channels, 1:2, 2:1, 0.72 V to 3.63 V, DHVQFN14"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "P3S0210BQAZ"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MUX, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "P3S0210BQ_1_1"
				(pin power_in line
					(at 20.32 -3.81 180)
					(length 2.54)
					(name "VCCP1")
					(number "1")
				)
				(pin bidirectional line
					(at 20.32 -6.35 180)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin bidirectional line
					(at 20.32 -8.89 180)
					(length 2.54)
					(name "B1")
					(number "3")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "A2")
					(number "4")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "B2")
					(number "5")
				)
				(pin passive line
					(at 20.32 -21.59 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin power_in line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "VCCP2")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VCCE")
					(number "8")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SEL")
					(number "9")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "OE")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "B")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "A")
					(number "12")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 2.54)
					(name "VCCS")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCR")
					(number "14")
				)
				(pin power_in line
					(at 20.32 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "15")
				)
			)
			(embedded_fonts no)
		)
)
