(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCA6408A_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCA6408A_TSSOP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCA6408A_TSSOP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/302/PCA6408A-1127604.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I/O Expander, 8 bit, I2C, SMBus, 1.65-5.5 V, TSSOP, 16 Pins"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PCA6408APW"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCA6408A_TSSOP_1_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD(I2C)")
					(number "1")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ADDR")
					(number "2")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "P0")
					(number "4")
				)
				(pin bidirectional line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "P1")
					(number "5")
				)
				(pin bidirectional line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "P2")
					(number "6")
				)
				(pin bidirectional line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "P3")
					(number "7")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "P4")
					(number "9")
				)
				(pin bidirectional line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "P5")
					(number "10")
				)
				(pin bidirectional line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "P6")
					(number "11")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "P7")
					(number "12")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{INT}")
					(number "13")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCL")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDA")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD(P)")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
