(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCA9517A_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCA9517A_TSSOP"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCA9517A_TSSOP"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/308/1/ONSM_S_A0009688870_1-2560458.pdf"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Buffer, ReDriver 2 Channel 8-MSOP"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PCA9517ADMR2G"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, LEVEL-SHIFTER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCA9517A_TSSOP_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VREF_{1}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SCL_{1}")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SDA_{1}")
					(number "3")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "EN")
					(number "5")
				)
				(pin bidirectional line
					(at 19.05 -8.89 180)
					(length 2.54)
					(name "SDA_{2}")
					(number "6")
				)
				(pin bidirectional line
					(at 19.05 -6.35 180)
					(length 2.54)
					(name "SCL_{2}")
					(number "7")
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "VREF_{2}")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
