(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCA9517ATP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCA9517ATP"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCA9517ATP"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9517A.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Level Translating I2C-Bus Repeater, 2 Inputs, 0.9 V to 5.5 V Supply, 50 mA Out, HWSON-8"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PCA9517ATP"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LEVEL-SHIFTER, IC, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCA9517ATP_1_1"
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SDA_{(A)}")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin passive line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "SDA_{(B)}")
					(number "4")
				)
				(pin passive line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "SCL_{(B)}")
					(number "5")
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "V_{CC(B)}")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC(A)}")
					(number "7")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCL_{(A)}")
					(number "8")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
