(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCA9539AHF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 36.83 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCA9539AHF"
				(at 36.83 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCA9539AHF"
				(at 36.83 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9539A.pdf"
				(at 36.83 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I/O Expanders 16bit I2C IO Port"
				(at 36.83 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PCA9539AHF,128"
				(at 36.83 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 36.83 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.83 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "VFQFN-16-1EP_3x3mm"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCA9539AHF_1_1"
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "IO0_0")
					(number "1")
				)
				(pin bidirectional line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "IO0_1")
					(number "2")
				)
				(pin bidirectional line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "IO0_2")
					(number "3")
				)
				(pin bidirectional line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "IO0_3")
					(number "4")
				)
				(pin bidirectional line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "IO0_4")
					(number "5")
				)
				(pin bidirectional line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "IO0_5")
					(number "6")
				)
				(pin bidirectional line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "IO0_6")
					(number "7")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "IO0_7")
					(number "8")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin bidirectional line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "IO1_0")
					(number "10")
				)
				(pin bidirectional line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "IO1_1")
					(number "11")
				)
				(pin bidirectional line
					(at 22.86 -27.94 180)
					(length 2.54)
					(name "IO1_2")
					(number "12")
				)
				(pin bidirectional line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "IO1_3")
					(number "13")
				)
				(pin bidirectional line
					(at 22.86 -33.02 180)
					(length 2.54)
					(name "IO1_4")
					(number "14")
				)
				(pin bidirectional line
					(at 22.86 -35.56 180)
					(length 2.54)
					(name "IO1_5")
					(number "15")
				)
				(pin bidirectional line
					(at 22.86 -38.1 180)
					(length 2.54)
					(name "IO1_6")
					(number "16")
				)
				(pin bidirectional line
					(at 22.86 -40.64 180)
					(length 2.54)
					(name "IO1_7")
					(number "17")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "A0")
					(number "18")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SCL")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDA")
					(number "20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "21")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{INT}")
					(number "22")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "A1")
					(number "23")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "~{RESET}")
					(number "24")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
