(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCA9698DGG_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCA9698DGG_TSSOP"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCA9698DGG_TSSOP"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/1090575.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I/O Expander, 40 bit, I2C, 2.3-5.5 V, TSSOP, 56 Pins"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PCA9698DGG,518"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCA9698DGG_TSSOP_1_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDA")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SCL")
					(number "2")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 2.54)
					(name "IO0_0")
					(number "3")
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "IO0_1")
					(number "4")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "IO0_2")
					(number "5")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "6")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "IO0_3")
					(number "7")
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "IO0_4")
					(number "8")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "IO0_5")
					(number "9")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "IO0_6")
					(number "10")
				)
				(pin power_in line
					(at 0 -109.22 0)
					(length 2.54)
					(name "VSS")
					(number "11")
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "IO0_7")
					(number "12")
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "IO1_0")
					(number "13")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "IO1_1")
					(number "14")
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "IO1_2")
					(number "15")
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "IO1_3")
					(number "16")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "IO1_4")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "18")
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "IO1_5")
					(number "19")
				)
				(pin bidirectional line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "IO1_6")
					(number "20")
				)
				(pin bidirectional line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "IO1_7")
					(number "21")
				)
				(pin bidirectional line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "IO2_0")
					(number "22")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "23")
				)
				(pin bidirectional line
					(at 30.48 -48.26 180)
					(length 2.54)
					(name "IO2_1")
					(number "24")
				)
				(pin bidirectional line
					(at 30.48 -50.8 180)
					(length 2.54)
					(name "IO2_2")
					(number "25")
				)
				(pin bidirectional line
					(at 30.48 -53.34 180)
					(length 2.54)
					(name "IO2_3")
					(number "26")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 2.54)
					(name "AD0")
					(number "27")
				)
				(pin input line
					(at 0 -101.6 0)
					(length 2.54)
					(name "AD1")
					(number "28")
				)
				(pin input line
					(at 0 -104.14 0)
					(length 2.54)
					(name "AD2")
					(number "29")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "~{OE}")
					(number "30")
				)
				(pin bidirectional line
					(at 30.48 -55.88 180)
					(length 2.54)
					(name "IO2_4")
					(number "31")
				)
				(pin bidirectional line
					(at 30.48 -58.42 180)
					(length 2.54)
					(name "IO2_5")
					(number "32")
				)
				(pin bidirectional line
					(at 30.48 -60.96 180)
					(length 2.54)
					(name "IO2_6")
					(number "33")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "34")
				)
				(pin bidirectional line
					(at 30.48 -63.5 180)
					(length 2.54)
					(name "IO2_7")
					(number "35")
				)
				(pin bidirectional line
					(at 30.48 -68.58 180)
					(length 2.54)
					(name "IO3_0")
					(number "36")
				)
				(pin bidirectional line
					(at 30.48 -71.12 180)
					(length 2.54)
					(name "IO3_1")
					(number "37")
				)
				(pin bidirectional line
					(at 30.48 -73.66 180)
					(length 2.54)
					(name "IO3_2")
					(number "38")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "39")
				)
				(pin bidirectional line
					(at 30.48 -76.2 180)
					(length 2.54)
					(name "IO3_3")
					(number "40")
				)
				(pin bidirectional line
					(at 30.48 -78.74 180)
					(length 2.54)
					(name "IO3_4")
					(number "41")
				)
				(pin bidirectional line
					(at 30.48 -81.28 180)
					(length 2.54)
					(name "IO3_5")
					(number "42")
				)
				(pin bidirectional line
					(at 30.48 -83.82 180)
					(length 2.54)
					(name "IO3_6")
					(number "43")
				)
				(pin bidirectional line
					(at 30.48 -86.36 180)
					(length 2.54)
					(name "IO3_7")
					(number "44")
				)
				(pin bidirectional line
					(at 30.48 -91.44 180)
					(length 2.54)
					(name "IO4_0")
					(number "45")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "46")
				)
				(pin bidirectional line
					(at 30.48 -93.98 180)
					(length 2.54)
					(name "IO4_1")
					(number "47")
				)
				(pin bidirectional line
					(at 30.48 -96.52 180)
					(length 2.54)
					(name "IO4_2")
					(number "48")
				)
				(pin bidirectional line
					(at 30.48 -99.06 180)
					(length 2.54)
					(name "IO4_3")
					(number "49")
				)
				(pin bidirectional line
					(at 30.48 -101.6 180)
					(length 2.54)
					(name "IO4_4")
					(number "50")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "51")
				)
				(pin bidirectional line
					(at 30.48 -104.14 180)
					(length 2.54)
					(name "IO4_5")
					(number "52")
				)
				(pin bidirectional line
					(at 30.48 -106.68 180)
					(length 2.54)
					(name "IO4_6")
					(number "53")
				)
				(pin bidirectional line
					(at 30.48 -109.22 180)
					(length 2.54)
					(name "IO4_7")
					(number "54")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{INT/SMBALERT}")
					(number "55")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{RESET}")
					(number "56")
				)
			)
			(embedded_fonts no)
		)
)
