(footprint "SON-6_1.3X2.0mm_P0.65mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "SON-6_1.3X2.0mm_P0.65mm"
		(at 0 2.25 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "."
		(at -1 -0.9 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -1 3.25 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1 4.5 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1 5.7 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.6 -0.661 90)
		(size 0.41 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.6 0 90)
		(size 0.41 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.6 0.66 90)
		(size 0.41 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.599 0.66 90)
		(size 0.41 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.599 0 90)
		(size 0.41 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.599 -0.661 90)
		(size 0.41 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_pd0922j5050s2hf.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
