(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PI3EQX1204-C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PI3EQX1204-C"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PI3EQX1204-C"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PI3EQX1204-C.pdf"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "12.5Gbps 4-Channel, SAS3, 10GbE ReDriver with Linear Equalization"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PI3EQX1204-CZHEX"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PI3EQX1204-C_1_1"
				(pin input line
					(at 0 -53.34 0)
					(length 2.54)
					(name "SW1")
					(number "1")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "SW0")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A0RX+")
					(number "4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A0RX-")
					(number "5")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "6")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A1RX+")
					(number "7")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A1RX-")
					(number "8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "9")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A2RX+")
					(number "10")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A2RX-")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "12")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A3RX+")
					(number "13")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A3RX-")
					(number "14")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "15")
				)
				(pin no_connect line
					(at 20.32 -41.91 180)
					(length 2.54)
					(name "DNC")
					(number "16")
				)
				(pin no_connect line
					(at 20.32 -38.1 180)
					(length 2.54)
					(name "DNC")
					(number "17")
				)
				(pin open_collector line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SDA")
					(number "18")
				)
				(pin open_collector line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SCL")
					(number "19")
				)
				(pin input line
					(at 22.86 -35.56 180)
					(length 2.54)
					(name "~{PRSNT}")
					(number "20")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "EN_{I2C}")
					(number "21")
				)
				(pin no_connect line
					(at 20.32 -40.64 180)
					(length 2.54)
					(name "DNC")
					(number "22")
				)
				(pin no_connect line
					(at 20.32 -39.37 180)
					(length 2.54)
					(name "DNC")
					(number "23")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "24")
				)
				(pin output line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "A3TX-")
					(number "25")
				)
				(pin input line
					(at 22.86 -27.94 180)
					(length 2.54)
					(name "A3TX+")
					(number "26")
				)
				(pin power_in line
					(at 22.86 -58.42 180)
					(length 2.54)
					(name "GND")
					(number "26")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "27")
				)
				(pin output line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "A2TX-")
					(number "28")
				)
				(pin input line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "A2TX+")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "30")
				)
				(pin output line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "A1TX-")
					(number "31")
				)
				(pin input line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "A1TX+")
					(number "32")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "33")
				)
				(pin output line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "A0TX-")
					(number "34")
				)
				(pin input line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "A0TX+")
					(number "35")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "36")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "FG0")
					(number "37")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "FG1/~{I2C_{RESET}}")
					(number "38")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 2.54)
					(name "EQ0/AD0")
					(number "39")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 2.54)
					(name "EQ1/AD1")
					(number "40")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 2.54)
					(name "EQ2/AD2")
					(number "41")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 2.54)
					(name "EQ3/AD3")
					(number "42")
				)
			)
			(embedded_fonts no)
		)
)
