(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PI3HDX412BDZBEX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PI3HDX412BDZBEX"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PI3HDX412BDZBEX"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PI3HDX412BD.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "HDMI Active Splitter, 2 Channels, 1:2, TQFN"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PI3HDX412BD"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MUX, IC, HDMI, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PI3HDX412BDZBEX_1_1"
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "MS")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "2")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "D2P")
					(number "4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "D2N")
					(number "5")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D1P")
					(number "7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D1N")
					(number "8")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D0P")
					(number "9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D0N")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "11")
				)
				(pin passive clock
					(at 0 -27.94 0)
					(length 2.54)
					(name "CLKP")
					(number "12")
				)
				(pin passive clock
					(at 0 -25.4 0)
					(length 2.54)
					(name "CLKN")
					(number "13")
				)
				(pin power_in line
					(at 0 -71.12 0)
					(length 2.54)
					(name "GND")
					(number "14")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "15")
				)
				(pin passive line
					(at 40.64 -5.08 180)
					(length 2.54)
					(name "SEL_OUT")
					(number "16")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "ROUT_SEL")
					(number "17")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD18")
					(number "18")
				)
				(pin passive clock
					(at 0 -48.26 0)
					(length 2.54)
					(name "EQ2/SCL_CTL")
					(number "19")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "EQ1/SDA_CTL")
					(number "20")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "22")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "24")
				)
				(pin passive clock
					(at 40.64 -33.02 180)
					(length 2.54)
					(name "CLKN2")
					(number "25")
				)
				(pin passive clock
					(at 40.64 -35.56 180)
					(length 2.54)
					(name "CLKP2")
					(number "26")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin passive line
					(at 40.64 -38.1 180)
					(length 2.54)
					(name "D0N2")
					(number "28")
				)
				(pin passive line
					(at 40.64 -40.64 180)
					(length 2.54)
					(name "D0P2")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "30")
				)
				(pin passive line
					(at 40.64 -43.18 180)
					(length 2.54)
					(name "D1N2")
					(number "31")
				)
				(pin passive line
					(at 40.64 -45.72 180)
					(length 2.54)
					(name "D1P2")
					(number "32")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin passive line
					(at 40.64 -48.26 180)
					(length 2.54)
					(name "D2N2")
					(number "34")
				)
				(pin passive line
					(at 40.64 -50.8 180)
					(length 2.54)
					(name "D2P2")
					(number "35")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "36")
				)
				(pin passive clock
					(at 40.64 -10.16 180)
					(length 2.54)
					(name "CLKN1")
					(number "37")
				)
				(pin passive clock
					(at 40.64 -12.7 180)
					(length 2.54)
					(name "CLKP1")
					(number "38")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin passive line
					(at 40.64 -15.24 180)
					(length 2.54)
					(name "D0N1")
					(number "40")
				)
				(pin passive line
					(at 40.64 -17.78 180)
					(length 2.54)
					(name "D0P1")
					(number "41")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "42")
				)
				(pin passive line
					(at 40.64 -20.32 180)
					(length 2.54)
					(name "D1N1")
					(number "43")
				)
				(pin passive line
					(at 40.64 -22.86 180)
					(length 2.54)
					(name "D1P1")
					(number "44")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin passive line
					(at 40.64 -25.4 180)
					(length 2.54)
					(name "D2N1")
					(number "46")
				)
				(pin passive line
					(at 40.64 -27.94 180)
					(length 2.54)
					(name "D2P1")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SW1/I2C_ADR0")
					(number "49")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SW2/I2C_ADR1")
					(number "50")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "EMP1/I2C_ADR2")
					(number "51")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "EMP2/I2C_ADR3")
					(number "52")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "53")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "DR")
					(number "54")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "SEL1")
					(number "55")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "OE")
					(number "56")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
)
