(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PIC18F8585-I_PT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PIC18F8585-I_PT"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PIC18F8585-I_PT"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30491D.pdf"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MCU 48K Flash 3328 RAM ECAN TQFP80"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PIC18F8585-I/PT"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, MEMORY, FLASH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PIC18F8585-I_PT_1_1"
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RG5/~{MCLR}/VPP")
					(number "9")
				)
				(pin power_in line
					(at 0 -39.37 0)
					(length 2.54)
					(name "VSS")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDD")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "AVSS")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RA3/AN3/VREF+")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RA2/AN2/VREF-")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "RA1/AN1")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RA0/AN0")
					(number "30")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "31")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RA5/AN4/LVDIN")
					(number "33")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "RA4/T0CKI")
					(number "34")
				)
				(pin bidirectional line
					(at 39.37 -24.13 180)
					(length 2.54)
					(name "RC1/T1OSI/CCP2")
					(number "35")
				)
				(pin bidirectional line
					(at 39.37 -21.59 180)
					(length 2.54)
					(name "RC0/T1OSO/T13CKI")
					(number "36")
				)
				(pin bidirectional line
					(at 39.37 -36.83 180)
					(length 2.54)
					(name "RC6/TX/CK")
					(number "37")
				)
				(pin bidirectional line
					(at 39.37 -39.37 180)
					(length 2.54)
					(name "RC7/RX/DT")
					(number "38")
				)
				(pin bidirectional line
					(at 39.37 -26.67 180)
					(length 2.54)
					(name "RC2/CCP1/P1A")
					(number "43")
				)
				(pin bidirectional line
					(at 39.37 -29.21 180)
					(length 2.54)
					(name "RC3/SCK/SCL")
					(number "44")
				)
				(pin bidirectional line
					(at 39.37 -31.75 180)
					(length 2.54)
					(name "RC4/SDI/SDA")
					(number "45")
				)
				(pin bidirectional line
					(at 39.37 -34.29 180)
					(length 2.54)
					(name "RC5/SDO")
					(number "46")
				)
				(pin bidirectional line
					(at 39.37 -17.78 180)
					(length 2.54)
					(name "RB7/KBI3/PGD")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "OSC1/CLKI")
					(number "49")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "OSC2/CLKO/RA6")
					(number "50")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "51")
				)
				(pin bidirectional line
					(at 39.37 -15.24 180)
					(length 2.54)
					(name "RB6/KBI2/PGC")
					(number "52")
				)
				(pin bidirectional line
					(at 39.37 -12.7 180)
					(length 2.54)
					(name "RB5/KBI1/PGM")
					(number "53")
				)
				(pin bidirectional line
					(at 39.37 -10.16 180)
					(length 2.54)
					(name "RB4/KBI0")
					(number "54")
				)
				(pin bidirectional line
					(at 39.37 -7.62 180)
					(length 2.54)
					(name "RB3/INT3/CCP2")
					(number "55")
				)
				(pin bidirectional line
					(at 39.37 -5.08 180)
					(length 2.54)
					(name "RB2/INT2")
					(number "56")
				)
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 2.54)
					(name "RB1/INT1")
					(number "57")
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 2.54)
					(name "RB0/INT0")
					(number "58")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "70")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "71")
				)
			)
			(symbol "PIC18F8585-I_PT_2_1"
				(pin bidirectional line
					(at 39.37 -19.05 180)
					(length 2.54)
					(name "RH2/A18")
					(number "1")
				)
				(pin bidirectional line
					(at 39.37 -21.59 180)
					(length 2.54)
					(name "RH3/A19")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "RE1/~{WR}/AD9")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "RE0/~{RD}/AD8")
					(number "4")
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 2.54)
					(name "RG0/CANTX1")
					(number "5")
				)
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 2.54)
					(name "RG1/CANTX2")
					(number "6")
				)
				(pin bidirectional line
					(at 39.37 -5.08 180)
					(length 2.54)
					(name "RG2/CANRX")
					(number "7")
				)
				(pin bidirectional line
					(at 39.37 -7.62 180)
					(length 2.54)
					(name "RG3")
					(number "8")
				)
				(pin bidirectional line
					(at 39.37 -10.16 180)
					(length 2.54)
					(name "RG4/P1D")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "RF7/~{SS}")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "RF6/AN11/C1IN-")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "RF5/AN10/C1IN+/CVREF")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "RF4/AN9/C2IN-")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "RF3/AN8/C2IN+")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "RF2/AN7/C1OUT")
					(number "18")
				)
				(pin bidirectional line
					(at 39.37 -31.75 180)
					(length 2.54)
					(name "RH7/AN15/P1B")
					(number "19")
				)
				(pin bidirectional line
					(at 39.37 -29.21 180)
					(length 2.54)
					(name "RH6/AN14/P1C")
					(number "20")
				)
				(pin bidirectional line
					(at 39.37 -26.67 180)
					(length 2.54)
					(name "RH5/AN13")
					(number "21")
				)
				(pin bidirectional line
					(at 39.37 -24.13 180)
					(length 2.54)
					(name "RH4/AN12")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "RF1/AN6/C2OUT")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "RF0/AN5")
					(number "24")
				)
				(pin bidirectional line
					(at 39.37 -45.72 180)
					(length 2.54)
					(name "RJ4/BA0")
					(number "39")
				)
				(pin bidirectional line
					(at 39.37 -48.26 180)
					(length 2.54)
					(name "RJ5/~{CE}")
					(number "40")
				)
				(pin bidirectional line
					(at 39.37 -50.8 180)
					(length 2.54)
					(name "RJ6/~{LB}")
					(number "41")
				)
				(pin bidirectional line
					(at 39.37 -53.34 180)
					(length 2.54)
					(name "RJ7/~{UB}")
					(number "42")
				)
				(pin bidirectional line
					(at 39.37 -43.18 180)
					(length 2.54)
					(name "RJ3/~{WRH}")
					(number "59")
				)
				(pin bidirectional line
					(at 39.37 -40.64 180)
					(length 2.54)
					(name "RJ2/~{WRL}")
					(number "60")
				)
				(pin bidirectional line
					(at 39.37 -38.1 180)
					(length 2.54)
					(name "RJ1/~{OE}")
					(number "61")
				)
				(pin bidirectional line
					(at 39.37 -35.56 180)
					(length 2.54)
					(name "RJ0/ALE")
					(number "62")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RD7/PSP7/AD7")
					(number "63")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RD6/PSP6/AD6")
					(number "64")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RD5/PSP5/AD5")
					(number "65")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RD4/PSP4/AD4")
					(number "66")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RD3/PSP3/AD3")
					(number "67")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RD2/PSP2/AD2")
					(number "68")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RD1/PSP1/AD1")
					(number "69")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "RD0/PSP0/AD0")
					(number "72")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "RE7/CCP2/AD15")
					(number "73")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "RE6/AD14/P1B")
					(number "74")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "RE5/AD13/P1C")
					(number "75")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 2.54)
					(name "RE4/AD12")
					(number "76")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "RE3/AD11")
					(number "77")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 2.54)
					(name "RE2/~{CS}/AD10")
					(number "78")
				)
				(pin bidirectional line
					(at 39.37 -13.97 180)
					(length 2.54)
					(name "RH0/A16")
					(number "79")
				)
				(pin bidirectional line
					(at 39.37 -16.51 180)
					(length 2.54)
					(name "RH1/A17")
					(number "80")
				)
			)
			(embedded_fonts no)
		)
)
