(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PN7160A1_HVQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 44.45 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PN7160A1_HVQFN"
				(at 44.45 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PN7160A1_HVQFN"
				(at 44.45 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PN7160_PN7161.pdf"
				(at 44.45 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Near Field Communication (NFC) controller"
				(at 44.45 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PN7160A1HN/C100E"
				(at 44.45 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 44.45 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 44.45 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 44.45 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "NFC, IC, RF, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "QFN40_PN7160_NXP QFN40_PN7160_NXP-M QFN40_PN7160_NXP-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PN7160A1_HVQFN_1_1"
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "I2C_ADR0")
					(number "1")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "DWL_REQ")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "I2C_ADR1")
					(number "3")
				)
				(pin power_out line
					(at 0 -60.96 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "I2C_SDA")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD(PAD)}")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "I2C_SCL")
					(number "7")
				)
				(pin output line
					(at 0 -19.05 0)
					(length 2.54)
					(name "IRQ")
					(number "8")
				)
				(pin power_out line
					(at 0 -60.96 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "9")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "VEN/~{RST}")
					(number "10")
				)
				(pin no_connect line
					(at 27.94 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "IC")
					(number "11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "V_{BAT}")
					(number "12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{DD(UP)}")
					(number "13")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "V_{DD(TX)}")
					(number "14")
				)
				(pin input line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "RXN")
					(number "15")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "RXP")
					(number "16")
				)
				(pin power_in line
					(at 0 -57.15 0)
					(length 2.54)
					(name "V_{DD(VMID)}")
					(number "17")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "TVDD_IN")
					(number "18")
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "TX2")
					(number "19")
				)
				(pin power_out line
					(at 0 -60.96 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "20")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "TX1")
					(number "21")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 2.54)
					(name "TVDD_IN2")
					(number "22")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 2.54)
					(name "ANT1")
					(number "23")
				)
				(pin bidirectional line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "ANT2")
					(number "24")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 2.54)
					(name "V_{DD(HF)}")
					(number "25")
				)
				(pin power_in line
					(at 0 -39.37 0)
					(length 2.54)
					(name "V_{DD(A)}")
					(number "26")
				)
				(pin power_in line
					(at 0 -44.45 0)
					(length 2.54)
					(name "V_{DD}")
					(number "27")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "V_{BAT}")
					(number "28")
				)
				(pin output line
					(at 30.48 -60.96 180)
					(length 2.54)
					(name "XTAL2")
					(number "29")
				)
				(pin input line
					(at 30.48 -58.42 180)
					(length 2.54)
					(name "CLK_XTAL1")
					(number "30")
				)
				(pin power_in line
					(at 0 -41.91 0)
					(length 2.54)
					(name "V_{DD(D)}")
					(number "31")
				)
				(pin no_connect line
					(at 27.94 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "32")
				)
				(pin no_connect line
					(at 27.94 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at 27.94 -24.13 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "34")
				)
				(pin no_connect line
					(at 27.94 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at 27.94 -26.67 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "36")
				)
				(pin output line
					(at 0 -11.43 0)
					(length 2.54)
					(name "DCDC_EN")
					(number "37")
				)
				(pin no_connect line
					(at 27.94 -19.05 180)
					(length 2.54)
					(hide yes)
					(name "IC")
					(number "38")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "WKUP_REQ")
					(number "39")
				)
				(pin output line
					(at 0 -16.51 0)
					(length 2.54)
					(name "CLK_REQ")
					(number "40")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "VSS")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
