(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PTN3363BSMP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PTN3363BSMP"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PTN3363BSMP"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PTN3363.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Low power HDMI/DVI level shifter with active DDC buffer"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PTN3363BSMP"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP Semiconductors"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, BUFFER, HDMI, LEVEL-SHIFTER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PTN3363BSMP_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 2.54)
					(name "EQ1")
					(number "2")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "DDET")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "REXT")
					(number "4")
				)
				(pin output line
					(at 31.75 -39.37 180)
					(length 2.54)
					(name "HPD_SOURCE")
					(number "5")
				)
				(pin bidirectional line
					(at 31.75 -36.83 180)
					(length 2.54)
					(name "SDA_SOURCE")
					(number "6")
				)
				(pin bidirectional line
					(at 31.75 -34.29 180)
					(length 2.54)
					(name "SCL_SOURCE")
					(number "7")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(name "EQ0")
					(number "8")
				)
				(pin output line
					(at 31.75 -25.4 180)
					(length 2.54)
					(name "OUT_D4+")
					(number "9")
				)
				(pin output line
					(at 31.75 -22.86 180)
					(length 2.54)
					(name "OUT_D4−")
					(number "10")
				)
				(pin output line
					(at 31.75 -20.32 180)
					(length 2.54)
					(name "OUT_D3+")
					(number "11")
				)
				(pin output line
					(at 31.75 -17.78 180)
					(length 2.54)
					(name "OUT_D3−")
					(number "12")
				)
				(pin output line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "OUT_D2+")
					(number "13")
				)
				(pin output line
					(at 31.75 -12.7 180)
					(length 2.54)
					(name "OUT_D2−")
					(number "14")
				)
				(pin output line
					(at 31.75 -10.16 180)
					(length 2.54)
					(name "OUT_D1+")
					(number "15")
				)
				(pin output line
					(at 31.75 -7.62 180)
					(length 2.54)
					(name "OUT_D1−")
					(number "16")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 2.54)
					(name "OE_N")
					(number "17")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "SCL_SINK")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "SDA_SINK")
					(number "20")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "HPD_SINK")
					(number "21")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "DDC_EN")
					(number "22")
				)
				(pin no_connect line
					(at 29.21 -67.31 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "23")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 2.54)
					(name "HIZ_EN")
					(number "24")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "IN_D1−")
					(number "25")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "IN_D1+")
					(number "26")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "IN_D2−")
					(number "27")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "IN_D2+")
					(number "28")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "IN_D3−")
					(number "29")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "IN_D3+")
					(number "30")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "IN_D4−")
					(number "31")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "IN_D4+")
					(number "32")
				)
				(pin power_in line
					(at 31.75 -69.85 180)
					(length 2.54)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
