(footprint "LCC-18_7.3x9mm_Layout4x5_P1.27mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Layout according to C-LCC-18-950")
	(property "Reference" "REF**"
		(at 0 -5.27 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "LCC-18_7.3x9mm_Layout4x5_P1.27mm"
		(at -4.2 6.09 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd allow_soldermask_bridges)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -4.2 7.23 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.2 8.43 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.18 9.66 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0.87 6.14 0)
		(unlocked yes)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0.87 7.64 0)
		(unlocked yes)
		(layer "User.9")
	)
	(pad "1" smd roundrect
		(at -0.635 -3.2 90)
		(size 2.94 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at -1.905 -3.965 90)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -3.14 -2.54 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -3.14 -1.27 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -3.14 1.27 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "7" smd roundrect
		(at -3.14 2.54 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at -1.905 3.965 90)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at -0.635 3.965 90)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "11" smd roundrect
		(at 1.905 3.965 90)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "12" smd roundrect
		(at 3.14 2.54 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "13" smd roundrect
		(at 3.14 1.27 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "14" smd roundrect
		(at 3.14 0 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "15" smd roundrect
		(at 3.14 -1.27 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "16" smd roundrect
		(at 3.14 -2.54 180)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "17" smd roundrect
		(at 1.905 -3.965 90)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "18" smd roundrect
		(at 0.635 -3.965 90)
		(size 1.41 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "antmicro_ric7s113e4.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
