(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RIC7S113E4"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RIC7S113E4"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RIC7S113E4"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-RIC7S113-DataSheet-v05_00-EN.pdf?fileId=8ac78c8c84f2c0670184f4d9c8d20a0b"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation hardened high and low side gate driver"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Infineon"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RIC7S113E4"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONTROLLER, DRIVER, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RIC7S113E4_1_1"
				(pin passive line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "LO")
					(number "1")
				)
				(pin passive line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "COM")
					(number "2")
				)
				(pin no_connect line
					(at 2.54 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin power_in line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "VCC")
					(number "4")
				)
				(pin passive line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "VS")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin power_in line
					(at 17.78 0 180)
					(length 2.54)
					(name "VB")
					(number "8")
				)
				(pin passive line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "HO")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "11")
				)
				(pin no_connect line
					(at 2.54 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "HIN")
					(number "13")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SD")
					(number "14")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "LIN")
					(number "15")
				)
				(pin no_connect line
					(at 2.54 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VSS")
					(number "17")
				)
				(pin no_connect line
					(at 2.54 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "18")
				)
			)
			(embedded_fonts no)
		)
)
