(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RK3399"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 68.58 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RK3399"
				(at 68.58 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RK3399"
				(at 68.58 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.rockchip.fr/RK3399%20datasheet%20V1.8.pdf"
				(at 68.58 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RK3399 ROCK Pi 4 Model A 2GB - ARM® Cortex®-A53, Cortex®-A72 MPU Embedded Evaluation Board"
				(at 68.58 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Rockchip"
				(at 68.58 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RK3399"
				(at 68.58 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 68.58 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 68.58 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, MCU, BGA, MICROPROCESSOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RK3399_1_1"
				(pin power_in line
					(at 0 -26.67 0)
					(length 5.08)
					(name "VSS")
					(number "A1")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A27")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A31")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA5")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA10")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 5.08)
					(name "AVSS")
					(number "AA11")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AA12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA13")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AA14")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AA15")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AA23")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AA26")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AA29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB9")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AB10")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AB11")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AB13")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AB15")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AB16")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AB17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB19")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AB23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC3")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC11")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC13")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC15")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC16")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC22")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC23")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC25")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC26")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AC29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD5")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD10")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AD13")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AD17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD22")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AD26")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AD29")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AE11")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AE12")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AE14")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AE17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE23")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AE27")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF9")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AF17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF20")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AF23")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AF24")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AF29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG2")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AG29")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AH29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ5")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ6")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ8")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ9")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ11")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ12")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ14")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ15")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ17")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ24")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ26")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ27")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ28")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "AJ29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AL1")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AL31")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B5")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 5.08)
					(name "EDP_AVSS")
					(number "B31")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C11")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C14")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C24")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C26")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "EDP_AVSS")
					(number "C28")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "EDP_AVSS")
					(number "C29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "EDP_AVSS")
					(number "D29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E2")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E7")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E24")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E31")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G27")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H10")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H11")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H13")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H16")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H18")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "EDP_AVSS")
					(number "H19")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H26")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J6")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J7")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J10")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "EDP_AVSS")
					(number "J21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K10")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K14")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K16")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K18")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "BIGCPU_VDD")
					(number "K19")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K20")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "K21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K22")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L6")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L11")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L13")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L14")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L16")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "LOGIC_VDD")
					(number "L17")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "L18")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "L19")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L20")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "L21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L22")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "L23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L27")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "CENTERLOGIC_VDD")
					(number "M11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "M12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "M13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "M14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "M15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M16")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "M17")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "M18")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "M19")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "M20")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "M21")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "M22")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "N11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "N12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N13")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N14")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N16")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N17")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "BIGCPU_VDD_COM")
					(number "N18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N19")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "N20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N21")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "BIGCPU_VDD")
					(number "N22")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P6")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P7")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P10")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P11")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "P13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "P14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "CENTERLOGIC_VDD")
					(number "P15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P16")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PLL_AVSS")
					(number "P17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P19")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "LITCPU_VDD")
					(number "P20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P21")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "LITCPU_VDD")
					(number "P22")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R5")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R6")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPU_VDD")
					(number "R11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "R12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "R13")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R14")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R16")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R18")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "LITCPU_VDD")
					(number "R19")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "LITCPU_VDD")
					(number "R20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R21")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "LITCPU_VDD")
					(number "R22")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "T11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "T12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "T13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "T14")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPU_VDD_COM")
					(number "T15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T16")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "T17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T19")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "LITCPU_VDD")
					(number "T20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T21")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "LITCPU_VDD")
					(number "T22")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U11")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "U13")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U14")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U16")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "U17")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "U18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U19")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "U20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U22")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "U23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U29")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V5")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "V11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "V12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "V13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "V14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "V15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "V16")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V17")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "V18")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "V19")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "V20")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "V21")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "V22")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "V23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "W10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "W11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "W12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "W14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "W15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "GPU_VDD")
					(number "W16")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W18")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W19")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "LOGIC_VDD")
					(number "W20")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W21")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W22")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "W23")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W30")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y3")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y9")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y10")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y11")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y12")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y13")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y14")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y15")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y16")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y17")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y20")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "Y23")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "Y29")
				)
			)
			(symbol "RK3399_2_1"
				(pin output line
					(at 50.8 -22.86 180)
					(length 5.08)
					(name "PCIE_TX2_P")
					(number "AA27")
				)
				(pin output line
					(at 50.8 -25.4 180)
					(length 5.08)
					(name "PCIE_TX2_N")
					(number "AA28")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PCIE_RX2_P")
					(number "AC27")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PCIE_RX2_N")
					(number "AC28")
				)
				(pin output line
					(at 50.8 -30.48 180)
					(length 5.08)
					(name "PCIE_TX3_P")
					(number "AD27")
				)
				(pin output line
					(at 50.8 -33.02 180)
					(length 5.08)
					(name "PCIE_TX3_N")
					(number "AD28")
				)
				(pin output line
					(at 50.8 -40.64 180)
					(length 5.08)
					(name "PCIE_RCLK_100M_N")
					(number "AD30")
				)
				(pin output line
					(at 50.8 -38.1 180)
					(length 5.08)
					(name "PCIE_RCLK_100M_P")
					(number "AD31")
				)
				(pin input clock
					(at 0 -30.48 0)
					(length 5.08)
					(name "GPIO4_D0")
					(number "AE6")
					(alternate "PCIE_CLKREQNB" passive line)
				)
				(pin output line
					(at 50.8 -7.62 180)
					(length 5.08)
					(name "PCIE_TX0_P")
					(number "AE30")
				)
				(pin output line
					(at 50.8 -10.16 180)
					(length 5.08)
					(name "PCIE_TX0_N")
					(number "AE31")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PCIE_RX3_P")
					(number "AF27")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PCIE_RX3_N")
					(number "AF28")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "PCIE_RX0_P")
					(number "AF30")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PCIE_RX0_N")
					(number "AF31")
				)
				(pin output line
					(at 50.8 -15.24 180)
					(length 5.08)
					(name "PCIE_TX1_P")
					(number "AG30")
				)
				(pin output line
					(at 50.8 -17.78 180)
					(length 5.08)
					(name "PCIE_TX1_N")
					(number "AG31")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PCIE_RX1_P")
					(number "AH30")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PCIE_RX1_N")
					(number "AH31")
				)
				(pin power_in line
					(at 50.8 0 180)
					(length 5.08)
					(name "PCIE_AVDD_0V9")
					(number "W24")
				)
				(pin power_in line
					(at 50.8 -2.54 180)
					(length 5.08)
					(name "PCIE_AVDD_1V8")
					(number "Y24")
				)
			)
			(symbol "RK3399_3_1"
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "DDR0_DQ3")
					(number "AA1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "DDR0_DQ2")
					(number "AA2")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "DDR0_DQS0N")
					(number "AA4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "DDR0_DQ1")
					(number "AB1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "DDR0_DQ0")
					(number "AB2")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "DDR0_DQ14")
					(number "AC1")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "DDR0_DQ15")
					(number "AC2")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "DDR0_DQS1P")
					(number "AC4")
				)
				(pin output line
					(at 50.8 -20.32 180)
					(length 5.08)
					(name "DDR0_DM1")
					(number "AC5")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "DDR0_DQ13")
					(number "AD1")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "DDR0_DQ11")
					(number "AD2")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "DDR0_DQS1N")
					(number "AD4")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "DDR0_DQ12")
					(number "AE1")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DDR0_DQ9")
					(number "AE2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DDR0_DQ10")
					(number "AF1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "DDR0_DQ8")
					(number "AF2")
				)
				(pin output line
					(at 50.8 -31.75 180)
					(length 5.08)
					(name "DDR0_CSN1")
					(number "B1")
				)
				(pin output line
					(at 50.8 -69.85 180)
					(length 5.08)
					(name "DDR0_A12")
					(number "C1")
				)
				(pin output line
					(at 50.8 -36.83 180)
					(length 5.08)
					(name "DDR0_CSN3")
					(number "C2")
				)
				(pin output line
					(at 50.8 -87.63 180)
					(length 5.08)
					(name "DDR0_BA0")
					(number "C3")
				)
				(pin output line
					(at 50.8 -64.77 180)
					(length 5.08)
					(name "DDR0_A10")
					(number "D1")
				)
				(pin output line
					(at 50.8 -72.39 180)
					(length 5.08)
					(name "DDR0_A13")
					(number "D2")
				)
				(pin output line
					(at 50.8 -74.93 180)
					(length 5.08)
					(name "DDR0_A14")
					(number "D3")
				)
				(pin output line
					(at 50.8 -113.03 180)
					(length 5.08)
					(name "DDR0_CKE0")
					(number "E1")
				)
				(pin output line
					(at 50.8 -67.31 180)
					(length 5.08)
					(name "DDR0_A11")
					(number "E3")
				)
				(pin output line
					(at 50.8 -41.91 180)
					(length 5.08)
					(name "DDR0_A1")
					(number "F1")
				)
				(pin output line
					(at 50.8 -39.37 180)
					(length 5.08)
					(name "DDR0_A0")
					(number "F2")
				)
				(pin output line
					(at 50.8 -11.43 180)
					(length 5.08)
					(name "DDR0_RASN")
					(number "F3")
				)
				(pin output line
					(at 50.8 -90.17 180)
					(length 5.08)
					(name "DDR0_BA1")
					(number "F4")
				)
				(pin output line
					(at 50.8 -115.57 180)
					(length 5.08)
					(name "DDR0_CKE1")
					(number "F5")
				)
				(pin output line
					(at 50.8 -44.45 180)
					(length 5.08)
					(name "DDR0_A2")
					(number "G1")
				)
				(pin output line
					(at 50.8 -46.99 180)
					(length 5.08)
					(name "DDR0_A3")
					(number "G2")
				)
				(pin output line
					(at 50.8 -109.22 180)
					(length 5.08)
					(name "DDR0_WEN")
					(number "G6")
				)
				(pin output line
					(at 50.8 -52.07 180)
					(length 5.08)
					(name "DDR0_A5")
					(number "H1")
				)
				(pin output line
					(at 50.8 -49.53 180)
					(length 5.08)
					(name "DDR0_A4")
					(number "H2")
				)
				(pin output line
					(at 50.8 0 180)
					(length 5.08)
					(name "DDR0_CLK0P")
					(number "H4")
				)
				(pin output line
					(at 50.8 -5.08 180)
					(length 5.08)
					(name "DDR0_CLK1P")
					(number "H5")
				)
				(pin output line
					(at 50.8 -13.97 180)
					(length 5.08)
					(name "DDR0_CASN")
					(number "H6")
				)
				(pin output line
					(at 50.8 -77.47 180)
					(length 5.08)
					(name "DDR0_A15")
					(number "H7")
				)
				(pin output line
					(at 50.8 -54.61 180)
					(length 5.08)
					(name "DDR0_A6")
					(number "J1")
				)
				(pin output line
					(at 50.8 -57.15 180)
					(length 5.08)
					(name "DDR0_A7")
					(number "J2")
				)
				(pin output line
					(at 50.8 -2.54 180)
					(length 5.08)
					(name "DDR0_CLK0N")
					(number "J4")
				)
				(pin output line
					(at 50.8 -7.62 180)
					(length 5.08)
					(name "DDR0_CLK1N")
					(number "J5")
				)
				(pin output line
					(at 50.8 -62.23 180)
					(length 5.08)
					(name "DDR0_A9")
					(number "K1")
				)
				(pin output line
					(at 50.8 -59.69 180)
					(length 5.08)
					(name "DDR0_A8")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "DDR0_DQ29")
					(number "L1")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "DDR0_DQ31")
					(number "L2")
				)
				(pin output line
					(at 50.8 -96.52 180)
					(length 5.08)
					(name "DDR0_ODT0")
					(number "L4")
				)
				(pin output line
					(at 50.8 -99.06 180)
					(length 5.08)
					(name "DDR0_ODT1")
					(number "L5")
				)
				(pin output line
					(at 0 -8.89 0)
					(length 5.08)
					(name "DDR0_RESETN")
					(number "L7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "L9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "DDR0_VDD")
					(number "L10")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "DDR0_DQ27")
					(number "M1")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "DDR0_DQ30")
					(number "M2")
				)
				(pin output line
					(at 50.8 -92.71 180)
					(length 5.08)
					(name "DDR0_BA2")
					(number "M4")
				)
				(pin output line
					(at 50.8 -34.29 180)
					(length 5.08)
					(name "DDR0_CSN2")
					(number "M5")
				)
				(pin output line
					(at 50.8 -29.21 180)
					(length 5.08)
					(name "DDR0_CSN0")
					(number "M6")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "DDR0_CLK_VDD")
					(number "M7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "M9")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "DDR0_DQ26")
					(number "N1")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "DDR0_DQ28")
					(number "N2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "N9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "N10")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "DDR0_DQ24")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "DDR0_DQ25")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "DDR0_DQS3P")
					(number "P4")
				)
				(pin output line
					(at 50.8 -25.4 180)
					(length 5.08)
					(name "DDR0_DM3")
					(number "P5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "P9")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "DDR0_DQ23")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "DDR0_DQ22")
					(number "R2")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 5.08)
					(name "DDR0_DQS3N")
					(number "R4")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "DDR0_PZQ")
					(number "R7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "DDR0PLL_AVDD_0V9")
					(number "R8")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "R9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "R10")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "DDR0_DQ20")
					(number "T1")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "DDR0_DQ21")
					(number "T2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "T9")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "DDR0_DQ18")
					(number "U1")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "DDR0_DQ19")
					(number "U2")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "DDR0_DQS2P")
					(number "U4")
				)
				(pin output line
					(at 50.8 -22.86 180)
					(length 5.08)
					(name "DDR0_DM2")
					(number "U5")
				)
				(pin output line
					(at 50.8 -81.28 180)
					(length 5.08)
					(name "DDR0_ATB0")
					(number "U6")
				)
				(pin output line
					(at 50.8 -83.82 180)
					(length 5.08)
					(name "DDR0_ATB1")
					(number "U7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "U9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "U10")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "DDR0_DQ16")
					(number "V1")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "DDR0_DQ17")
					(number "V2")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "DDR0_DQS2N")
					(number "V4")
				)
				(pin output line
					(at 50.8 -102.87 180)
					(length 5.08)
					(name "DDR0_PLL_TESTOUT_P")
					(number "V6")
				)
				(pin output line
					(at 50.8 -105.41 180)
					(length 5.08)
					(name "DDR0_PLL_TESTOUT_N")
					(number "V7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR0_VDD")
					(number "V9")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "DDR0_DQ6")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "DDR0_DQ7")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "DDR0_DQ5")
					(number "Y1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "DDR0_DQ4")
					(number "Y2")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "DDR0_DQS0P")
					(number "Y4")
				)
				(pin output line
					(at 50.8 -17.78 180)
					(length 5.08)
					(name "DDR0_DM0")
					(number "Y5")
				)
			)
			(symbol "RK3399_4_1"
				(pin output line
					(at 50.8 -2.54 180)
					(length 5.08)
					(name "DDR1_CSN1")
					(number "A2")
				)
				(pin output line
					(at 50.8 -52.07 180)
					(length 5.08)
					(name "DDR1_A12")
					(number "A3")
				)
				(pin output line
					(at 50.8 -46.99 180)
					(length 5.08)
					(name "DDR1_A10")
					(number "A4")
				)
				(pin output line
					(at 50.8 -114.3 180)
					(length 5.08)
					(name "DDR1_CKE0")
					(number "A5")
				)
				(pin output line
					(at 50.8 -44.45 180)
					(length 5.08)
					(name "DDR1_A9")
					(number "A6")
				)
				(pin output line
					(at 50.8 -39.37 180)
					(length 5.08)
					(name "DDR1_A7")
					(number "A7")
				)
				(pin output line
					(at 50.8 -34.29 180)
					(length 5.08)
					(name "DDR1_A5")
					(number "A8")
				)
				(pin output line
					(at 50.8 -29.21 180)
					(length 5.08)
					(name "DDR1_A3")
					(number "A9")
				)
				(pin output line
					(at 50.8 -24.13 180)
					(length 5.08)
					(name "DDR1_A1")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "DDR1_DQ10")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "DDR1_DQ12")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "DDR1_DQ13")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "DDR1_DQ14")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "DDR1_DQ1")
					(number "A15")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "DDR1_DQ3")
					(number "A16")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "DDR1_DQ5")
					(number "A17")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "DDR1_DQ6")
					(number "A18")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "DDR1_DQ16")
					(number "A19")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "DDR1_DQ18")
					(number "A20")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "DDR1_DQ20")
					(number "A21")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "DDR1_DQ23")
					(number "A22")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "DDR1_DQ24")
					(number "A23")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "DDR1_DQ26")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "DDR1_DQ27")
					(number "A25")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "DDR1_DQ29")
					(number "A26")
				)
				(pin output line
					(at 50.8 -69.85 180)
					(length 5.08)
					(name "DDR1_BA0")
					(number "B2")
				)
				(pin output line
					(at 50.8 -7.62 180)
					(length 5.08)
					(name "DDR1_CSN3")
					(number "B3")
				)
				(pin output line
					(at 50.8 -54.61 180)
					(length 5.08)
					(name "DDR1_A13")
					(number "B4")
				)
				(pin output line
					(at 50.8 -41.91 180)
					(length 5.08)
					(name "DDR1_A8")
					(number "B6")
				)
				(pin output line
					(at 50.8 -36.83 180)
					(length 5.08)
					(name "DDR1_A6")
					(number "B7")
				)
				(pin output line
					(at 50.8 -31.75 180)
					(length 5.08)
					(name "DDR1_A4")
					(number "B8")
				)
				(pin output line
					(at 50.8 -26.67 180)
					(length 5.08)
					(name "DDR1_A2")
					(number "B9")
				)
				(pin output line
					(at 50.8 -21.59 180)
					(length 5.08)
					(name "DDR1_A0")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "DDR1_DQ8")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "DDR1_DQ9")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "DDR1_DQ11")
					(number "B13")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "DDR1_DQ15")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "DDR1_DQ0")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "DDR1_DQ2")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "DDR1_DQ4")
					(number "B17")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "DDR1_DQ7")
					(number "B18")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "DDR1_DQ17")
					(number "B19")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "DDR1_DQ19")
					(number "B20")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "DDR1_DQ21")
					(number "B21")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "DDR1_DQ22")
					(number "B22")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "DDR1_DQ25")
					(number "B23")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "DDR1_DQ28")
					(number "B24")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "DDR1_DQ30")
					(number "B25")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "DDR1_DQ31")
					(number "B26")
				)
				(pin output line
					(at 50.8 -57.15 180)
					(length 5.08)
					(name "DDR1_A14")
					(number "C4")
				)
				(pin output line
					(at 50.8 -49.53 180)
					(length 5.08)
					(name "DDR1_A11")
					(number "C5")
				)
				(pin output line
					(at 50.8 -85.09 180)
					(length 5.08)
					(name "DDR1_RASN")
					(number "C6")
				)
				(pin output line
					(at 50.8 -72.39 180)
					(length 5.08)
					(name "DDR1_BA1")
					(number "D6")
				)
				(pin output line
					(at 50.8 -78.74 180)
					(length 5.08)
					(name "DDR1_CLK0N")
					(number "D8")
				)
				(pin output line
					(at 50.8 -91.44 180)
					(length 5.08)
					(name "DDR1_CLK0P")
					(number "D9")
				)
				(pin output line
					(at 50.8 -104.14 180)
					(length 5.08)
					(name "DDR1_ODT0")
					(number "D11")
				)
				(pin output line
					(at 50.8 -74.93 180)
					(length 5.08)
					(name "DDR1_BA2")
					(number "D12")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "DDR1_DQS1N")
					(number "D14")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "DDR1_DQS1P")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "DDR1_DQS0N")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "DDR1_DQS0P")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "DDR1_DQS2N")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "DDR1_DQS2P")
					(number "D21")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "DDR1_DQS3N")
					(number "D23")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "DDR1_DQS3P")
					(number "D24")
				)
				(pin output line
					(at 50.8 -116.84 180)
					(length 5.08)
					(name "DDR1_CKE1")
					(number "E6")
				)
				(pin output line
					(at 50.8 -81.28 180)
					(length 5.08)
					(name "DDR1_CLK1N")
					(number "E8")
				)
				(pin output line
					(at 50.8 -93.98 180)
					(length 5.08)
					(name "DDR1_CLK1P")
					(number "E9")
				)
				(pin output line
					(at 50.8 -106.68 180)
					(length 5.08)
					(name "DDR1_ODT1")
					(number "E11")
				)
				(pin output line
					(at 50.8 -13.97 180)
					(length 5.08)
					(name "DDR1_DM1")
					(number "E14")
				)
				(pin output line
					(at 50.8 -11.43 180)
					(length 5.08)
					(name "DDR1_DM0")
					(number "E17")
				)
				(pin output line
					(at 50.8 -16.51 180)
					(length 5.08)
					(name "DDR1_DM2")
					(number "E20")
				)
				(pin output line
					(at 50.8 -19.05 180)
					(length 5.08)
					(name "DDR1_DM3")
					(number "E23")
				)
				(pin output line
					(at 50.8 -110.49 180)
					(length 5.08)
					(name "DDR1_WEN")
					(number "F7")
				)
				(pin output line
					(at 50.8 -87.63 180)
					(length 5.08)
					(name "DDR1_CASN")
					(number "F9")
				)
				(pin output line
					(at 50.8 -5.08 180)
					(length 5.08)
					(name "DDR1_CSN2")
					(number "F11")
				)
				(pin output line
					(at 50.8 0 180)
					(length 5.08)
					(name "DDR1_CSN0")
					(number "F12")
				)
				(pin output line
					(at 50.8 -97.79 180)
					(length 5.08)
					(name "DDR1_PLL_TESTOUT_P")
					(number "F14")
				)
				(pin output line
					(at 50.8 -63.5 180)
					(length 5.08)
					(name "DDR1_ATB0")
					(number "F17")
				)
				(pin output line
					(at 50.8 -59.69 180)
					(length 5.08)
					(name "DDR1_A15")
					(number "G8")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DDR1_RESETN")
					(number "G11")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "DDR1_CLK_VDD")
					(number "G12")
				)
				(pin output line
					(at 50.8 -100.33 180)
					(length 5.08)
					(name "DDR1_PLL_TESTOUT_N")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "DDR1_PZQ")
					(number "G15")
				)
				(pin output line
					(at 50.8 -66.04 180)
					(length 5.08)
					(name "DDR1_ATB1")
					(number "G17")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "DDR1PLL_AVDD_0V9")
					(number "H14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "DDR1_VDD")
					(number "J11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "J12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "J13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "J14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "J15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "J16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "J17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "J18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "K11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "K13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "K15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DDR1_VDD")
					(number "K17")
				)
			)
			(symbol "RK3399_5_1"
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA19")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA20")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AA22")
				)
				(pin bidirectional line
					(at 40.64 -3.81 180)
					(length 5.08)
					(name "DFTJTAG_TMS")
					(number "AA24")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB20")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AB22")
				)
				(pin bidirectional line
					(at 40.64 -6.35 180)
					(length 5.08)
					(name "DFTJTAG_TRSTN")
					(number "AB24")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC12")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC14")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AD11")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AD12")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AD14")
				)
				(pin no_connect line
					(at 5.08 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AD15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "EFUSE")
					(number "AD23")
				)
				(pin power_in line
					(at 0 -31.75 0)
					(length 5.08)
					(name "USIC_AVDD_1V2")
					(number "AD24")
				)
				(pin power_in line
					(at 0 -34.29 0)
					(length 5.08)
					(name "USIC_AVDD_0V9")
					(number "AD25")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GPIO4_D6")
					(number "AG4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO4_D2")
					(number "AH3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO4_D4")
					(number "AH5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO4_D5")
					(number "AJ3")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "USIC_STROBE")
					(number "AJ30")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "USIC_DATA")
					(number "AJ31")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GPIO4_C5")
					(number "AK1")
					(alternate "SPDIF_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO4_D3")
					(number "AK3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO4_D1")
					(number "AK4")
					(alternate "DP_HOTPLUG" passive line)
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "GPIO1_C6")
					(number "L25")
					(alternate "TCPD_VBUS_SOURCE0" passive line)
				)
				(pin bidirectional line
					(at 40.64 -20.32 180)
					(length 5.08)
					(name "GPIO1_D0")
					(number "L26")
					(alternate "TCPD_VBUS_SOURCE2" passive line)
				)
				(pin bidirectional line
					(at 40.64 -12.7 180)
					(length 5.08)
					(name "GPIO1_B5")
					(number "M24")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "GPIO1_C7")
					(number "M31")
					(alternate "TCPD_VBUS_SOURCE1" passive line)
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "GPIO0_A2")
					(number "N24")
					(alternate "WIFI_26MHZ" passive line)
				)
				(pin bidirectional line
					(at 40.64 -34.29 180)
					(length 5.08)
					(name "GPIO0_B5")
					(number "P24")
					(alternate "TCPD_VBUS_FDIS" passive line)
					(alternate "TCPD_VBUS_SOURCE3" passive line)
				)
				(pin bidirectional line
					(at 40.64 -40.64 180)
					(length 5.08)
					(name "GPIO0_A1")
					(number "R29")
					(alternate "DDRIO_PWROFF" passive line)
					(alternate "TCPD_CCDB_EN" passive line)
				)
				(pin output line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "GPIO1_A5")
					(number "R30")
					(alternate "AP_PWROFF" passive line)
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "NPOR")
					(number "T30")
				)
				(pin bidirectional line
					(at 40.64 -29.21 180)
					(length 5.08)
					(name "GPIO0_B3")
					(number "U30")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "GPIO0_A0")
					(number "U31")
					(alternate "CLK32K_IN" passive line)
					(alternate "TEST_CLKOUT0" passive line)
				)
				(pin bidirectional line
					(at 40.64 -31.75 180)
					(length 5.08)
					(name "GPIO0_B4")
					(number "V26")
					(alternate "TCPD_VBUS_BDIS" passive line)
				)
				(pin bidirectional line
					(at 40.64 -24.13 180)
					(length 5.08)
					(name "GPIO0_B1")
					(number "V30")
					(alternate "PMUIO2_VOLSEL" passive line)
				)
				(pin bidirectional line
					(at 40.64 -26.67 180)
					(length 5.08)
					(name "GPIO0_B2")
					(number "W31")
				)
				(pin output line
					(at 40.64 0 180)
					(length 5.08)
					(name "XOUT_OSC")
					(number "Y30")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "XIN_OSC")
					(number "Y31")
				)
			)
			(symbol "RK3399_6_1"
				(pin power_in line
					(at 38.1 0 180)
					(length 5.08)
					(name "SDMMC0_VDD")
					(number "T23")
				)
				(pin output line
					(at 38.1 -10.16 180)
					(length 5.08)
					(name "SDMMC0_VDDPST")
					(number "U26")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO4_B3")
					(number "U27")
					(alternate "APJTAG_TMS" passive line)
					(alternate "SDMMC0_D3" passive line)
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO0_B0")
					(number "U28")
					(alternate "SDMMC0_WRPT" passive line)
					(alternate "TEST_CLKOUT2" passive line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO4_B5")
					(number "V25")
					(alternate "MCUJTAG_TMS" passive line)
					(alternate "SDMMC0_CMD" passive line)
				)
				(pin input line
					(at 38.1 -15.24 180)
					(length 5.08)
					(name "GPIO0_A7")
					(number "V28")
					(alternate "SDMMC0_DET" passive line)
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO4_B4")
					(number "V29")
					(alternate "MUCJTAG_TCK" passive line)
					(alternate "SDMMC0_CLKOUT" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO4_B1")
					(number "Y26")
					(alternate "SDMMC0_D1" passive line)
					(alternate "UART2A_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO4_B0")
					(number "Y27")
					(alternate "SDMMC0_D0" passive line)
					(alternate "UART2A_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO4_B2")
					(number "Y28")
					(alternate "APJTAG_TCK" passive line)
					(alternate "SDMMC0_D2" passive line)
				)
			)
			(symbol "RK3399_7_1"
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "GPIO0_A4")
					(number "AA25")
					(alternate "SDIO0_INTN" passive line)
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 5.08)
					(name "GPIO2_C4")
					(number "AD8")
					(alternate "SDIO0_D0" passive line)
					(alternate "SPI5_RXD" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO2_D3")
					(number "AD9")
					(alternate "SDIO0_PWREN" passive line)
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GPIO2_C7")
					(number "AE8")
					(alternate "SDIO0_D3" passive line)
					(alternate "SPI5_CSN0" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO2_D1")
					(number "AF7")
					(alternate "SDIO0_CLKOUT" passive line)
					(alternate "TEST_CLKOUT1" passive line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO2_D4")
					(number "AF8")
					(alternate "SDIO0_BKPWR" passive line)
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GPIO2_C6")
					(number "AG7")
					(alternate "SDIO0_D2" passive line)
					(alternate "SPI5_CLK" passive line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO2_D0")
					(number "AH6")
					(alternate "SDIO0_CMD" passive line)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GPIO2_C5")
					(number "AK5")
					(alternate "SDIO0_D1" passive line)
					(alternate "SPI5_TXD" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO2_D2")
					(number "AL4")
					(alternate "PCIE_CLKREQN" passive line)
					(alternate "SDIO0_DETN" passive line)
				)
				(pin bidirectional line
					(at 35.56 -11.43 180)
					(length 5.08)
					(name "GPIO1_A0")
					(number "R25")
					(alternate "ISP0_SHUTTER_EN" passive line)
					(alternate "ISP1_SHUTTER_EN" passive line)
					(alternate "TCPD_VBUS_SINK_EN" passive line)
				)
				(pin bidirectional line
					(at 35.56 -16.51 180)
					(length 5.08)
					(name "GPIO1_A2")
					(number "R26")
					(alternate "ISP0_FLASHTRIGIN" passive line)
					(alternate "ISP1_FLASHTRIGIN" passive line)
					(alternate "TCPD_CC1_VCONN_EN" passive line)
				)
				(pin bidirectional line
					(at 35.56 -19.05 180)
					(length 5.08)
					(name "GPIO1_A3")
					(number "R27")
					(alternate "ISP0_FLASHTRIGOUT" passive line)
					(alternate "ISP1_FLASHTRIGOUT" passive line)
				)
				(pin bidirectional line
					(at 35.56 -21.59 180)
					(length 5.08)
					(name "GPIO1_A4")
					(number "R28")
					(alternate "ISP0_PRELIGHT_TRIG" passive line)
					(alternate "ISP1_PRELIGHT_TRIG" passive line)
				)
				(pin bidirectional line
					(at 35.56 -13.97 180)
					(length 5.08)
					(name "GPIO1_A1")
					(number "T31")
					(alternate "ISP0_SHUTTER_TRIG" passive line)
					(alternate "ISP1_SHUTTER_TRIG" passive line)
					(alternate "TCPD_CC0_VCONN_EN" passive line)
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "GPIO0_A3")
					(number "V31")
					(alternate "SDIO0_WRPT" passive line)
				)
			)
			(symbol "RK3399_8_1"
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "EMMC_D3")
					(number "J25")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "EMMC_D4")
					(number "J26")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "EMMC_D5")
					(number "J27")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "EMMC_D0")
					(number "J28")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "EMMC_D1")
					(number "J29")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "EMMC_D2")
					(number "J30")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "EMMC_CMD")
					(number "J31")
				)
				(pin power_in line
					(at 44.45 0 180)
					(length 5.08)
					(name "EMMC_VDD_1V8")
					(number "K24")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "EMMC_D7")
					(number "K30")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "EMMC_STRB")
					(number "K31")
				)
				(pin power_in line
					(at 44.45 -2.54 180)
					(length 5.08)
					(name "EMMC_COREDLL_0V9")
					(number "L24")
				)
				(pin output line
					(at 44.45 -7.62 180)
					(length 5.08)
					(name "EMMC_CLK")
					(number "L28")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "EMMC_CALIO")
					(number "L29")
				)
				(pin output line
					(at 44.45 -10.16 180)
					(length 5.08)
					(name "EMMC_TP")
					(number "L30")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "EMMC_D6")
					(number "L31")
				)
				(pin bidirectional line
					(at 44.45 -15.24 180)
					(length 5.08)
					(name "GPIO0_A5")
					(number "V27")
					(alternate "EMMC_PWRON" passive line)
				)
			)
			(symbol "RK3399_9_1"
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "USB1_DP")
					(number "AA30")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "USB1_DN")
					(number "AA31")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "USB0_DP")
					(number "AB30")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "USB0_DN")
					(number "AB31")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "USB1_RBIAS")
					(number "AC30")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "USB0_RBIAS")
					(number "AC31")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "USB_AVDD_1V8")
					(number "U24")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "USB_AVDD_0V9")
					(number "V24")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "USB_AVDD_3V3")
					(number "Y25")
				)
			)
			(symbol "RK3399_10_1"
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "EDP_AUXN")
					(number "A28")
				)
				(pin output line
					(at 38.1 -2.54 180)
					(length 5.08)
					(name "EDP_TX0N")
					(number "A29")
				)
				(pin output line
					(at 38.1 -7.62 180)
					(length 5.08)
					(name "EDP_TX1N")
					(number "A30")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "GPIO4_C7")
					(number "AD7")
					(alternate "EDP_HOTPLUG" passive line)
					(alternate "HDMI_CECINOUT" passive line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "EDP_AUXP")
					(number "B28")
				)
				(pin output line
					(at 38.1 0 180)
					(length 5.08)
					(name "EDP_TX0P")
					(number "B29")
				)
				(pin output line
					(at 38.1 -5.08 180)
					(length 5.08)
					(name "EDP_TX1P")
					(number "B30")
				)
				(pin output line
					(at 38.1 -10.16 180)
					(length 5.08)
					(name "EDP_TX2P")
					(number "C30")
				)
				(pin output line
					(at 38.1 -12.7 180)
					(length 5.08)
					(name "EDP_TX2N")
					(number "C31")
				)
				(pin output line
					(at 38.1 -15.24 180)
					(length 5.08)
					(name "EDP_TX3P")
					(number "D30")
				)
				(pin output line
					(at 38.1 -17.78 180)
					(length 5.08)
					(name "EDP_TX3N")
					(number "D31")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "EDP_DC_TP")
					(number "G20")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 5.08)
					(name "EDP_REXT")
					(number "G21")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "EDP_AVDD_0V9")
					(number "H20")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 5.08)
					(name "EDP_CLK24M_IN")
					(number "H21")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "EDP_AVDD_1V8")
					(number "J19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "EDP_AVDD_1V8")
					(number "J20")
				)
			)
			(symbol "RK3399_11_1"
				(pin power_in line
					(at 53.34 0 180)
					(length 5.08)
					(name "TYPEC0_AVDD_1V8")
					(number "AA18")
				)
				(pin power_in line
					(at 53.34 -2.54 180)
					(length 5.08)
					(name "TYPEC1_AVDD_1V8")
					(number "AA21")
				)
				(pin power_in line
					(at 53.34 -5.08 180)
					(length 5.08)
					(name "TYPEC0_AVDD_3V3")
					(number "AB18")
				)
				(pin power_in line
					(at 53.34 -7.62 180)
					(length 5.08)
					(name "TYPEC1_AVDD_3V3")
					(number "AB21")
				)
				(pin input line
					(at 53.34 -19.05 180)
					(length 5.08)
					(name "TYPEC1_U3VBUSDET")
					(number "AC19")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 5.08)
					(name "TYPEC0_RCLKM")
					(number "AD18")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "TYPEC0_U3VBUSDET")
					(number "AD19")
				)
				(pin output line
					(at 0 -68.58 0)
					(length 5.08)
					(name "TYPEC1_RCLKM")
					(number "AD20")
				)
				(pin output line
					(at 0 -58.42 0)
					(length 5.08)
					(name "TYPEC0_RCLKP")
					(number "AE18")
				)
				(pin output line
					(at 0 -71.12 0)
					(length 5.08)
					(name "TYPEC1_RCLKP")
					(number "AE20")
				)
				(pin input line
					(at 53.34 -21.59 180)
					(length 5.08)
					(name "TYPEC1_REXT")
					(number "AE21")
				)
				(pin bidirectional line
					(at 53.34 -66.04 180)
					(length 5.08)
					(name "TYPEC1_AUXP_PD_PU")
					(number "AE24")
				)
				(pin input line
					(at 53.34 -16.51 180)
					(length 5.08)
					(name "TYPEC1_ID")
					(number "AE26")
				)
				(pin bidirectional line
					(at 53.34 -36.83 180)
					(length 5.08)
					(name "TYPEC1_CC2")
					(number "AF21")
				)
				(pin bidirectional line
					(at 53.34 -63.5 180)
					(length 5.08)
					(name "TYPEC1_AUXM_PU_PD")
					(number "AF25")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "TYPEC0_AUXM_PU_PD")
					(number "AG17")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "TYPEC0_REXT")
					(number "AG18")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "TYPEC0_REXT_CC")
					(number "AG20")
				)
				(pin input line
					(at 53.34 -24.13 180)
					(length 5.08)
					(name "TYPEC1_REXT_CC")
					(number "AG21")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "TYPEC0_DP")
					(number "AG23")
				)
				(pin bidirectional line
					(at 53.34 -27.94 180)
					(length 5.08)
					(name "TYPEC1_DP")
					(number "AG24")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "TYPEC0_AUXP_PD_PU")
					(number "AH17")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "TYPEC0_CC1")
					(number "AH18")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "TYPEC0_CC2")
					(number "AH20")
				)
				(pin bidirectional line
					(at 53.34 -34.29 180)
					(length 5.08)
					(name "TYPEC1_CC1")
					(number "AH21")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "TYPEC0_DN")
					(number "AH23")
				)
				(pin bidirectional line
					(at 53.34 -30.48 180)
					(length 5.08)
					(name "TYPEC1_DN")
					(number "AH24")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "TYPEC0_AUXP")
					(number "AK20")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "TYPEC0_RX1P")
					(number "AK21")
				)
				(pin output line
					(at 0 -26.67 0)
					(length 5.08)
					(name "TYPEC0_TX1M")
					(number "AK22")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "TYPEC0_RX2P")
					(number "AK23")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 5.08)
					(name "TYPEC0_TX2M")
					(number "AK24")
				)
				(pin bidirectional line
					(at 53.34 -45.72 180)
					(length 5.08)
					(name "TYPEC1_RX1P")
					(number "AK25")
				)
				(pin output line
					(at 53.34 -43.18 180)
					(length 5.08)
					(name "TYPEC1_TX1M")
					(number "AK26")
				)
				(pin bidirectional line
					(at 53.34 -57.15 180)
					(length 5.08)
					(name "TYPEC1_RX2P")
					(number "AK27")
				)
				(pin output line
					(at 53.34 -54.61 180)
					(length 5.08)
					(name "TYPEC1_TX2M")
					(number "AK28")
				)
				(pin bidirectional line
					(at 53.34 -68.58 180)
					(length 5.08)
					(name "TYPEC1_AUXP")
					(number "AK29")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "TYPEC0_U2VBUSDET")
					(number "AK30")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "TYPEC1_U2VBUSDET")
					(number "AK31")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "TYPEC0_AUXM")
					(number "AL20")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "TYPEC0_RX1M")
					(number "AL21")
				)
				(pin output line
					(at 0 -24.13 0)
					(length 5.08)
					(name "TYPEC0_TX1P")
					(number "AL22")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "TYPEC0_RX2M")
					(number "AL23")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 5.08)
					(name "TYPEC0_TX2P")
					(number "AL24")
				)
				(pin bidirectional line
					(at 53.34 -48.26 180)
					(length 5.08)
					(name "TYPEC1_RX1M")
					(number "AL25")
				)
				(pin output line
					(at 53.34 -40.64 180)
					(length 5.08)
					(name "TYPEC1_TX1P")
					(number "AL26")
				)
				(pin bidirectional line
					(at 53.34 -59.69 180)
					(length 5.08)
					(name "TYPEC1_RX2M")
					(number "AL27")
				)
				(pin output line
					(at 53.34 -52.07 180)
					(length 5.08)
					(name "TYPEC1_TX2P")
					(number "AL28")
				)
				(pin bidirectional line
					(at 53.34 -71.12 180)
					(length 5.08)
					(name "TYPEC1_AUXM")
					(number "AL29")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "TYPEC0_ID")
					(number "AL30")
				)
				(pin power_in line
					(at 53.34 -10.16 180)
					(length 5.08)
					(name "TYPEC0_AVDD_0V9")
					(number "Y18")
				)
				(pin passive line
					(at 53.34 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "TYPEC0_AVDD_0V9")
					(number "Y19")
				)
				(pin power_in line
					(at 53.34 -12.7 180)
					(length 5.08)
					(name "TYPEC1_AVDD_0V9")
					(number "Y21")
				)
				(pin passive line
					(at 53.34 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "TYPEC1_AVDD_0V9")
					(number "Y22")
				)
			)
			(symbol "RK3399_12_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "HDMI_AVDD_0V9")
					(number "AA16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "HDMI_AVDD_0V9")
					(number "AA17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "HDMI_AVDD_1V8")
					(number "AD16")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "HDMI_HPD")
					(number "AE15")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "HDMI_REXT")
					(number "AF15")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "HDMI_TCP")
					(number "AK16")
				)
				(pin output line
					(at 38.1 0 180)
					(length 5.08)
					(name "HDMI_TX0P")
					(number "AK17")
				)
				(pin output line
					(at 38.1 -5.08 180)
					(length 5.08)
					(name "HDMI_TX1P")
					(number "AK18")
				)
				(pin output line
					(at 38.1 -10.16 180)
					(length 5.08)
					(name "HDMI_TX2P")
					(number "AK19")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "HDMI_TCN")
					(number "AL16")
				)
				(pin output line
					(at 38.1 -2.54 180)
					(length 5.08)
					(name "HDMI_TX0N")
					(number "AL17")
				)
				(pin output line
					(at 38.1 -7.62 180)
					(length 5.08)
					(name "HDMI_TX1N")
					(number "AL18")
				)
				(pin output line
					(at 38.1 -12.7 180)
					(length 5.08)
					(name "HDMI_TX2N")
					(number "AL19")
				)
			)
			(symbol "RK3399_13_1"
				(pin power_in line
					(at 44.45 0 180)
					(length 5.08)
					(name "MIPI_RX0_AVDD_1V8")
					(number "AB14")
				)
				(pin bidirectional line
					(at 44.45 -8.89 180)
					(length 5.08)
					(name "MIPI_RX0_REXT")
					(number "AF14")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MIPI_RX0_D3P")
					(number "AK11")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MIPI_RX0_D2P")
					(number "AK12")
				)
				(pin bidirectional line
					(at 44.45 -3.81 180)
					(length 5.08)
					(name "MIPI_RX0_CLKP")
					(number "AK13")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MIPI_RX0_D1P")
					(number "AK14")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MIPI_RX0_D0P")
					(number "AK15")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MIPI_RX0_D3N")
					(number "AL11")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MIPI_RX0_D2N")
					(number "AL12")
				)
				(pin bidirectional line
					(at 44.45 -6.35 180)
					(length 5.08)
					(name "MIPI_RX0_CLKN")
					(number "AL13")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MIPI_RX0_D1N")
					(number "AL14")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MIPI_RX0_D0N")
					(number "AL15")
				)
			)
			(symbol "RK3399_14_1"
				(pin power_in line
					(at 44.45 0 180)
					(length 5.08)
					(name "MIPI_TX0_AVDD_1V8")
					(number "AB12")
				)
				(pin bidirectional line
					(at 44.45 -8.89 180)
					(length 5.08)
					(name "MIPI_TX0_REXT")
					(number "AF12")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MIPI_TX0_D3P")
					(number "AG9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MIPI_TX0_D2P")
					(number "AG11")
				)
				(pin bidirectional line
					(at 44.45 -3.81 180)
					(length 5.08)
					(name "MIPI_TX0_CLKP")
					(number "AG12")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MIPI_TX0_D1P")
					(number "AG14")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MIPI_TX0_D0P")
					(number "AG15")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MIPI_TX0_D3N")
					(number "AH9")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MIPI_TX0_D2N")
					(number "AH11")
				)
				(pin bidirectional line
					(at 44.45 -6.35 180)
					(length 5.08)
					(name "MIPI_TX0_CLKN")
					(number "AH12")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MIPI_TX0_D1N")
					(number "AH14")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MIPI_TX0_D0N")
					(number "AH15")
				)
			)
			(symbol "RK3399_15_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "MIPI_TX1_RX1_AVDD_1V8")
					(number "AC10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MIPI_TX1_RX1_REXT")
					(number "AF11")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D0P")
					(number "AK6")
				)
				(pin passive line
					(at 54.61 -5.08 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D1P")
					(number "AK7")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 5.08)
					(name "MIPI_TX1_RX1_CLKP")
					(number "AK8")
				)
				(pin passive line
					(at 54.61 -10.16 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D2P")
					(number "AK9")
				)
				(pin passive line
					(at 54.61 -15.24 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D3P")
					(number "AK10")
				)
				(pin passive line
					(at 54.61 -2.54 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D0N")
					(number "AL6")
				)
				(pin passive line
					(at 54.61 -7.62 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D1N")
					(number "AL7")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(name "MIPI_TX1_RX1_CLKN")
					(number "AL8")
				)
				(pin passive line
					(at 54.61 -12.7 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D2N")
					(number "AL9")
				)
				(pin passive line
					(at 54.61 -17.78 180)
					(length 5.08)
					(name "MIPI_TX1_RX1_D3N")
					(number "AL10")
				)
			)
			(symbol "RK3399_16_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "ADC_AVDD")
					(number "AC24")
				)
				(pin input line
					(at 29.21 0 180)
					(length 5.08)
					(name "ADC_IN2")
					(number "AG25")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 5.08)
					(name "ADC_IN0")
					(number "AG26")
				)
				(pin input line
					(at 29.21 -2.54 180)
					(length 5.08)
					(name "ADC_IN3")
					(number "AG28")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 5.08)
					(name "ADC_IN1")
					(number "AH26")
				)
				(pin input line
					(at 29.21 -5.08 180)
					(length 5.08)
					(name "ADC_IN4")
					(number "AH27")
				)
				(pin bidirectional line
					(at 29.21 -7.62 180)
					(length 5.08)
					(name "GPIO1_A6")
					(number "P26")
					(alternate "TSADC_INT" passive line)
				)
			)
			(symbol "RK3399_17_1"
				(pin bidirectional line
					(at 31.75 -2.54 180)
					(length 5.08)
					(name "GPIO3_B1")
					(number "C27")
					(alternate "MAC_RXDV" passive line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO3_A4")
					(number "D26")
					(alternate "MAC_TXD0" passive line)
					(alternate "SPI0_RXD" passive line)
				)
				(pin bidirectional line
					(at 31.75 -19.05 180)
					(length 5.08)
					(name "GPIO3_C0")
					(number "D27")
					(alternate "MAC_COL" passive line)
					(alternate "SPDIF_TX" passive line)
					(alternate "UART3_CTSN" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO3_A3")
					(number "E25")
					(alternate "MAC_RXD3" passive line)
					(alternate "SPI4_CSN0" passive line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO3_A6")
					(number "E26")
					(alternate "MAC_RXD0" passive line)
					(alternate "SPI0_CLK" passive line)
				)
				(pin bidirectional line
					(at 31.75 -21.59 180)
					(length 5.08)
					(name "GPIO3_C1")
					(number "E28")
					(alternate "MAC_TXCLK" passive line)
					(alternate "UART3_RTSN" passive line)
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 5.08)
					(name "GPIO3_B0")
					(number "E29")
					(alternate "MAC_MDC" passive line)
					(alternate "SPI0_CSN1" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO3_A2")
					(number "E30")
					(alternate "MAC_RXD2" passive line)
					(alternate "SPI4_CLK" passive line)
				)
				(pin bidirectional line
					(at 31.75 -5.08 180)
					(length 5.08)
					(name "GPIO3_B2")
					(number "F23")
					(alternate "I2C5_SDA" passive line)
					(alternate "MAC_RXER" passive line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO3_A0")
					(number "F24")
					(alternate "MAC_TXD2" passive line)
					(alternate "SPI4_RXD" passive line)
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 5.08)
					(name "GPIO3_B6")
					(number "F25")
					(alternate "MAC_RXCLK" passive line)
					(alternate "UART3_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO3_A7")
					(number "F27")
					(alternate "MAC_RXD1" passive line)
					(alternate "SPI0_CSN0" passive line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO3_A5")
					(number "G23")
					(alternate "MAC_TXD1" passive line)
					(alternate "SPI0_TXD" passive line)
				)
				(pin bidirectional clock
					(at 31.75 -7.62 180)
					(length 5.08)
					(name "GPIO3_B3")
					(number "G24")
					(alternate "I2C5_SCL" passive line)
					(alternate "MAC_CLK" passive line)
				)
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 5.08)
					(name "GPIO3_B5")
					(number "G26")
					(alternate "MAC_MDIO" passive line)
					(alternate "UART1_TX" passive line)
				)
				(pin bidirectional line
					(at 31.75 -10.16 180)
					(length 5.08)
					(name "GPIO3_B4")
					(number "H22")
					(alternate "MAC_TXEN" passive line)
					(alternate "UART1_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO3_A1")
					(number "H23")
					(alternate "MAC_TXD3" passive line)
					(alternate "SPI4_TXD" passive line)
				)
			)
			(symbol "RK3399_18_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO2_C0")
					(number "AE9")
					(alternate "UART0_RX" passive line)
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 5.08)
					(name "GPIO4_C0")
					(number "AG6")
					(alternate "I2C3_SDA" passive line)
					(alternate "UART2B_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO2_C2")
					(number "AG8")
					(alternate "UART0_CTSN" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO2_C1")
					(number "AH8")
					(alternate "UART0_TX" passive line)
				)
				(pin bidirectional line
					(at 31.75 -7.62 180)
					(length 5.08)
					(name "GPIO4_C4")
					(number "AJ4")
					(alternate "UART2C_TX" passive line)
				)
				(pin bidirectional line
					(at 31.75 -5.08 180)
					(length 5.08)
					(name "GPIO4_C3")
					(number "AK2")
					(alternate "UART2C_RX" passive line)
				)
				(pin bidirectional line
					(at 31.75 -2.54 180)
					(length 5.08)
					(name "GPIO4_C1")
					(number "AL2")
					(alternate "I2C3_SCL" passive line)
					(alternate "UART2B_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO2_C3")
					(number "AL5")
					(alternate "UART0_RTSN" passive line)
				)
			)
			(symbol "RK3399_19_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO4_A1")
					(number "AG1")
					(alternate "I2C1_SDA" passive line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO1_C4")
					(number "M29")
					(alternate "I2C8_SDA" passive line)
				)
				(pin bidirectional clock
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO1_C5")
					(number "M30")
					(alternate "I2C8_SCL" passive line)
				)
				(pin bidirectional clock
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO1_B4")
					(number "P30")
					(alternate "I2C4_SCL" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO1_B3")
					(number "P31")
					(alternate "I2C4_SDA" passive line)
				)
				(pin bidirectional clock
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO4_A2")
					(number "Y6")
					(alternate "I2C1_SCL" passive line)
				)
			)
			(symbol "RK3399_20_1"
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO4_C2")
					(number "AF5")
					(alternate "PWM0" passive line)
					(alternate "VOP0_PWM" passive line)
					(alternate "VOP1_PWM" passive line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO4_C6")
					(number "AL3")
					(alternate "PWM1" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO1_B6")
					(number "M25")
					(alternate "PWM3B_IR" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO1_C3")
					(number "M28")
					(alternate "PWM2" passive line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO0_A6")
					(number "P25")
					(alternate "PWM3A_IR" passive line)
				)
			)
			(symbol "RK3399_21_1"
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 5.08)
					(name "GPIO3_B7")
					(number "B27")
					(alternate "CIF_CLKOUTB" passive line)
					(alternate "MAC_CRS" passive line)
					(alternate "UART3_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO2_A3")
					(number "F28")
					(alternate "CIF_D3" passive line)
					(alternate "VOP_D3" passive line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO2_A5")
					(number "F29")
					(alternate "CIF_D5" passive line)
					(alternate "VOP_D5" passive line)
				)
				(pin bidirectional line
					(at 31.75 -2.54 180)
					(length 5.08)
					(name "GPIO2_B1")
					(number "F30")
					(alternate "CIF_HREF" passive line)
					(alternate "I2C6_SDA" passive line)
					(alternate "SPI2_RXD" passive line)
				)
				(pin bidirectional line
					(at 31.75 -10.16 180)
					(length 5.08)
					(name "GPIO2_B4")
					(number "F31")
					(alternate "SPI2_CSN0" passive line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO2_A7")
					(number "G30")
					(alternate "CIF_D7" passive line)
					(alternate "I2C7_SDA" passive line)
					(alternate "VOP_D7" passive line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO2_A0")
					(number "G31")
					(alternate "CIF_D0" passive line)
					(alternate "I2C2_SDA" passive line)
					(alternate "VOP_D0" passive line)
				)
				(pin bidirectional line
					(at 31.75 -5.08 180)
					(length 5.08)
					(name "GPIO2_B2")
					(number "H24")
					(alternate "CIF_CLKIN" passive line)
					(alternate "I2C6_SCL" passive line)
					(alternate "SPI2_TXD" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO2_A1")
					(number "H25")
					(alternate "CIF_D1" passive line)
					(alternate "I2C2_SCL" passive line)
					(alternate "VOP_D1" passive line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO2_A6")
					(number "H27")
					(alternate "CIF_D6" passive line)
					(alternate "VOP_D6" passive line)
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 5.08)
					(name "GPIO2_B0")
					(number "H28")
					(alternate "CIF_VSYNC" passive line)
					(alternate "I2C7_SCL" passive line)
					(alternate "VOP_CLK" passive line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO2_A4")
					(number "H29")
					(alternate "CIF_D4" passive line)
					(alternate "VOP_D4" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO2_A2")
					(number "H30")
					(alternate "CIF_D2" passive line)
					(alternate "VOP_D2" passive line)
				)
				(pin bidirectional line
					(at 31.75 -7.62 180)
					(length 5.08)
					(name "GPIO2_B3")
					(number "H31")
					(alternate "CIF_CLKOUTA" passive line)
					(alternate "SPI2_CLK" passive line)
					(alternate "VOP_DEN" passive line)
				)
			)
			(symbol "RK3399_22_1"
				(pin power_in line
					(at 0 -17.78 0)
					(length 5.08)
					(name "APIO5_VDDPST")
					(number "AA8")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "APIO3_VDD_1V8")
					(number "AB8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "APIO4_VDDPST")
					(number "AC8")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "APIO4_VDD")
					(number "AC9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "APIO1_VDDPST")
					(number "J22")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "APIO1_VDD")
					(number "J23")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "APIO2_VDDPST")
					(number "J24")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "APIO2_VDD")
					(number "K23")
				)
				(pin power_in line
					(at 41.91 -7.62 180)
					(length 5.08)
					(name "PMUIO2_VDDPST")
					(number "N23")
				)
				(pin power_in line
					(at 41.91 -15.24 180)
					(length 5.08)
					(name "PLL_AVDD_1V8")
					(number "P18")
				)
				(pin power_in line
					(at 41.91 -10.16 180)
					(length 5.08)
					(name "PMUIO2_VDD")
					(number "P23")
				)
				(pin power_in line
					(at 41.91 -12.7 180)
					(length 5.08)
					(name "PLL_AVDD_0V9")
					(number "R17")
				)
				(pin power_in line
					(at 41.91 -5.08 180)
					(length 5.08)
					(name "PMUIO1_VDD_1V8")
					(number "R24")
				)
				(pin power_in line
					(at 41.91 -2.54 180)
					(length 5.08)
					(name "PMU_VDD_0V9")
					(number "T24")
				)
				(pin power_in line
					(at 41.91 0 180)
					(length 5.08)
					(name "PMU_VDD_1V8")
					(number "U25")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "APIO5_VDD")
					(number "Y8")
				)
			)
			(symbol "RK3399_23_1"
				(pin output line
					(at 0 -19.05 0)
					(length 5.08)
					(name "GPIO1_B7")
					(number "M26")
					(alternate "I2C0_SDA" passive line)
					(alternate "SPI3_RXD" passive line)
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "GPIO1_C1")
					(number "M27")
					(alternate "SPI3_CLK" passive line)
				)
				(pin input line
					(at 0 -16.51 0)
					(length 5.08)
					(name "GPIO1_C0")
					(number "N30")
					(alternate "I2C0_SCL" passive line)
					(alternate "SPI3_TXD" passive line)
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "GPIO1_C2")
					(number "N31")
					(alternate "SPI3_CSN0" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO1_A7")
					(number "P27")
					(alternate "SPI1_RXD" passive line)
					(alternate "UART4_RX" passive line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO1_B1")
					(number "P28")
					(alternate "PMCU_JTAG_TCK" passive line)
					(alternate "SPI1_CLK" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO1_B2")
					(number "P29")
					(alternate "PMCU_JTAG_TMS" passive line)
					(alternate "SPI1_CSN0" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO1_B0")
					(number "R31")
					(alternate "SPI1_TXD" passive line)
					(alternate "UART4_TX" passive line)
				)
			)
			(symbol "RK3399_24_1"
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO3_D5")
					(number "AA6")
					(alternate "I2S0_SDI2SDO2" passive line)
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 5.08)
					(name "GPIO4_A4")
					(number "AA7")
					(alternate "I2S1_LRCK_RX" passive line)
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 5.08)
					(name "GPIO4_A7")
					(number "AC6")
					(alternate "I2S1_SDO0" passive line)
				)
				(pin bidirectional clock
					(at 33.02 0 180)
					(length 5.08)
					(name "GPIO4_A0")
					(number "AC7")
					(alternate "I2S_CLK" passive line)
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 5.08)
					(name "GPIO4_A6")
					(number "AD6")
					(alternate "I2S1_SDI0" passive line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO3_D4")
					(number "AE5")
					(alternate "I2S0_SDI1SDO3" passive line)
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 5.08)
					(name "GPIO4_A3")
					(number "AF3")
					(alternate "I2S1_SCLK" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO3_D1")
					(number "AF4")
					(alternate "I2S0_LRCK_RX" passive line)
				)
				(pin bidirectional clock
					(at 0 0 0)
					(length 5.08)
					(name "GPIO3_D0")
					(number "AG3")
					(alternate "I2S0_SCLK" passive line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO3_D7")
					(number "AH1")
					(alternate "I2S0_SDO0" passive line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO3_D6")
					(number "AH2")
					(alternate "I2S0_SDI3SDO1" passive line)
				)
				(pin bidirectional line
					(at 33.02 -7.62 180)
					(length 5.08)
					(name "GPIO4_A5")
					(number "AJ1")
					(alternate "I2S1_LRCK_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO3_D2")
					(number "AJ2")
					(alternate "I2S0_LRCK_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO3_D3")
					(number "Y7")
					(alternate "I2S0_SDI0" passive line)
				)
			)
			(embedded_fonts no)
		)
)
