(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RP2350A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RP2350A"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RP2350A"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://datasheets.raspberrypi.com/rp2350/rp2350-datasheet.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "The dual-architecture MCU has a dual-core Hazard3 RISC-V CPU and dual-core ARM Cortex-M33, selectable at boot time in software or in one-time programmable memory, Raspberry Pi , 32 bit, 150MHz system clock, 520 KB SRAM, 60 pin"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RP2350A"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Raspberry Pi"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RP2350A_1_1"
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "IOVDD")
					(number "1")
				)
				(pin bidirectional line
					(at 31.75 -7.62 180)
					(length 2.54)
					(name "GPIO0")
					(number "2")
				)
				(pin bidirectional line
					(at 31.75 -10.16 180)
					(length 2.54)
					(name "GPIO1")
					(number "3")
				)
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 2.54)
					(name "GPIO2")
					(number "4")
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "GPIO3")
					(number "5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "6")
				)
				(pin bidirectional line
					(at 31.75 -17.78 180)
					(length 2.54)
					(name "GPIO4")
					(number "7")
				)
				(pin bidirectional line
					(at 31.75 -20.32 180)
					(length 2.54)
					(name "GPIO5")
					(number "8")
				)
				(pin bidirectional line
					(at 31.75 -22.86 180)
					(length 2.54)
					(name "GPIO6")
					(number "9")
				)
				(pin bidirectional line
					(at 31.75 -25.4 180)
					(length 2.54)
					(name "GPIO7")
					(number "10")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "IOVDD")
					(number "11")
				)
				(pin bidirectional line
					(at 31.75 -27.94 180)
					(length 2.54)
					(name "GPIO8")
					(number "12")
				)
				(pin bidirectional line
					(at 31.75 -30.48 180)
					(length 2.54)
					(name "GPIO9")
					(number "13")
				)
				(pin bidirectional line
					(at 31.75 -33.02 180)
					(length 2.54)
					(name "GPIO10")
					(number "14")
				)
				(pin bidirectional line
					(at 31.75 -35.56 180)
					(length 2.54)
					(name "GPIO11")
					(number "15")
				)
				(pin bidirectional line
					(at 31.75 -38.1 180)
					(length 2.54)
					(name "GPIO12")
					(number "16")
				)
				(pin bidirectional line
					(at 31.75 -40.64 180)
					(length 2.54)
					(name "GPIO13")
					(number "17")
				)
				(pin bidirectional line
					(at 31.75 -43.18 180)
					(length 2.54)
					(name "GPIO14")
					(number "18")
				)
				(pin bidirectional line
					(at 31.75 -45.72 180)
					(length 2.54)
					(name "GPIO15")
					(number "19")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "IOVDD")
					(number "20")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(name "XIN")
					(number "21")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(name "XOUT")
					(number "22")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DVDD")
					(number "23")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SWCLK")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SWDIO")
					(number "25")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RUN")
					(number "26")
				)
				(pin bidirectional line
					(at 31.75 -48.26 180)
					(length 2.54)
					(name "GPIO16")
					(number "27")
				)
				(pin bidirectional line
					(at 31.75 -50.8 180)
					(length 2.54)
					(name "GPIO17")
					(number "28")
				)
				(pin bidirectional line
					(at 31.75 -53.34 180)
					(length 2.54)
					(name "GPIO18")
					(number "29")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "IOVDD")
					(number "30")
				)
				(pin bidirectional line
					(at 31.75 -55.88 180)
					(length 2.54)
					(name "GPIO19")
					(number "31")
				)
				(pin bidirectional line
					(at 31.75 -58.42 180)
					(length 2.54)
					(name "GPIO20")
					(number "32")
				)
				(pin bidirectional line
					(at 31.75 -60.96 180)
					(length 2.54)
					(name "GPIO21")
					(number "33")
				)
				(pin bidirectional line
					(at 31.75 -63.5 180)
					(length 2.54)
					(name "GPIO22")
					(number "34")
				)
				(pin bidirectional line
					(at 31.75 -66.04 180)
					(length 2.54)
					(name "GPIO23")
					(number "35")
				)
				(pin bidirectional line
					(at 31.75 -68.58 180)
					(length 2.54)
					(name "GPIO24")
					(number "36")
				)
				(pin bidirectional line
					(at 31.75 -71.12 180)
					(length 2.54)
					(name "GPIO25")
					(number "37")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "IOVDD")
					(number "38")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "39")
				)
				(pin bidirectional line
					(at 31.75 -73.66 180)
					(length 2.54)
					(name "GPIO26_ADC0")
					(number "40")
				)
				(pin bidirectional line
					(at 31.75 -76.2 180)
					(length 2.54)
					(name "GPIO27_ADC1")
					(number "41")
				)
				(pin bidirectional line
					(at 31.75 -78.74 180)
					(length 2.54)
					(name "GPIO28_ADC2")
					(number "42")
				)
				(pin bidirectional line
					(at 31.75 -81.28 180)
					(length 2.54)
					(name "GPIO29_ADC3")
					(number "43")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ADC_AVDD")
					(number "44")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "IOVDD")
					(number "45")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VREG_AVDD")
					(number "46")
				)
				(pin power_in line
					(at 0 -78.74 0)
					(length 2.54)
					(name "VREG_PGND")
					(number "47")
				)
				(pin passive line
					(at 31.75 0 180)
					(length 2.54)
					(name "VREG_LX")
					(number "48")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VREG_VIN")
					(number "49")
				)
				(pin passive line
					(at 31.75 -2.54 180)
					(length 2.54)
					(name "VREG_FB")
					(number "50")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "USB_DM")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "USB_DP")
					(number "52")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "USB_OTP_VDD")
					(number "53")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "QSPI_IOVDD")
					(number "54")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "QSPI_SD3")
					(number "55")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "QSPI_SCLK")
					(number "56")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "QSPI_SD0")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "QSPI_SD2")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "QSPI_SD1")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "QSPI_SS")
					(number "60")
				)
				(pin power_in line
					(at 0 -81.28 0)
					(length 2.54)
					(name "GND")
					(number "61")
				)
			)
			(embedded_fonts no)
		)
)
