(footprint "QFN-80_EP_10x10_Pitch0.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -5.39 -5.49 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-80_EP_10x10_Pitch0.4mm"
		(at -5.21 6.37 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -5.48 8.37 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.48 9.57 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -5.48 10.77 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -4.91 -3.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -4.91 -3.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -4.91 -3 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -4.91 -2.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -4.91 -2.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -4.91 -1.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -4.91 -1.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -4.91 -1 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -4.91 -0.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -4.91 -0.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -4.91 0.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -4.91 0.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -4.91 1 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at -4.91 1.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -4.91 1.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -4.91 2.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at -4.91 2.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at -4.91 3 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at -4.91 3.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at -4.91 3.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at -3.8 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at -3.4 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at -3 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at -2.6 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at -2.2 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at -1.8 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at -1.4 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at -1 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at -0.6 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at -0.2 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 0.2 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 0.6 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 1 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 1.4 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 1.8 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 2.2 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 2.6 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 3 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 3.4 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 3.8 4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 4.91 3.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 4.91 3.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at 4.91 3 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at 4.91 2.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at 4.91 2.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at 4.91 1.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at 4.91 1.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at 4.91 1 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd oval
		(at 4.91 0.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd oval
		(at 4.91 0.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd oval
		(at 4.91 -0.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd oval
		(at 4.91 -0.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd oval
		(at 4.91 -1 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd oval
		(at 4.91 -1.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd oval
		(at 4.91 -1.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd oval
		(at 4.91 -2.2 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd oval
		(at 4.91 -2.6 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd oval
		(at 4.91 -3 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd oval
		(at 4.91 -3.4 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd oval
		(at 4.91 -3.8 90)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd oval
		(at 3.8 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd oval
		(at 3.4 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd oval
		(at 3 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd oval
		(at 2.6 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd oval
		(at 2.2 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd oval
		(at 1.8 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd oval
		(at 1.4 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd oval
		(at 1 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd oval
		(at 0.6 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd oval
		(at 0.2 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd oval
		(at -0.2 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd oval
		(at -0.6 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd oval
		(at -1 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd oval
		(at -1.4 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd oval
		(at -1.8 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd oval
		(at -2.2 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd oval
		(at -2.6 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd oval
		(at -3 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd oval
		(at -3.4 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd oval
		(at -3.8 -4.91)
		(size 0.22 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at -1.275 -1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at -1.275 -0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at -1.275 0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at -1.275 1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at -0.425 -1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at -0.425 -0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at -0.425 0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at -0.425 1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 0.425 -1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 0.425 -0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 0.425 0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 0.425 1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 1.275 -1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 1.275 -0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 1.275 0.425)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(pad "81" smd rect
		(at 1.275 1.275)
		(size 0.85 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.075)
	)
	(embedded_fonts no)
	(model "antmicro_rp2350b.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
