(footprint "QFN-32-1EP_4x4mm_P0.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-32-1EP_4x4mm_P0.4mm"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.851 6.688 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.851 7.888 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.851 9.088 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.005 -1.4)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "2" smd roundrect
		(at -2.005 -1)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "3" smd roundrect
		(at -2.005 -0.6)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "4" smd roundrect
		(at -2.005 -0.201)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "5" smd roundrect
		(at -2.005 0.2)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "6" smd roundrect
		(at -2.005 0.599)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "7" smd roundrect
		(at -2.005 0.999)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "8" smd roundrect
		(at -2.005 1.399)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "9" smd roundrect
		(at -1.4 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "10" smd roundrect
		(at -1 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "11" smd roundrect
		(at -0.6 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "12" smd roundrect
		(at -0.201 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "13" smd roundrect
		(at 0.2 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "14" smd roundrect
		(at 0.599 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "15" smd roundrect
		(at 0.999 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "16" smd roundrect
		(at 1.399 2.004)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "17" smd roundrect
		(at 2.004 1.399)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "18" smd roundrect
		(at 2.004 0.999)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "19" smd roundrect
		(at 2.004 0.599)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "20" smd roundrect
		(at 2.004 0.2)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "21" smd roundrect
		(at 2.004 -0.201)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "22" smd roundrect
		(at 2.004 -0.6)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "23" smd roundrect
		(at 2.004 -1)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "24" smd roundrect
		(at 2.004 -1.4)
		(size 0.71 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "25" smd roundrect
		(at 1.399 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "26" smd roundrect
		(at 0.999 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "27" smd roundrect
		(at 0.599 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "28" smd roundrect
		(at 0.2 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "29" smd roundrect
		(at -0.201 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "30" smd roundrect
		(at -0.6 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "31" smd roundrect
		(at -1 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "32" smd roundrect
		(at -1.4 -2.005)
		(size 0.22 0.71)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.03)
	)
	(pad "33" smd rect
		(at 0 0)
		(size 2.8 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_rtl8111h.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
