(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RTL8111H"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RTL8111H"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RTL8111H"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2108141930_Realtek-Semicon-RTL8111H-CG_C2761340.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "10/100/1000M Ethernet controller,  triple-speed IEEE 802.3 compatible MAC, triple-speed Ethernet transceiver, PCIe bus controller, embedded memory"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RTL8111H"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Realtek"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, ETHERNET, PCIE, SMT, TRANSCEIVER, PHY"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RTL8111H_1_1"
				(pin bidirectional line
					(at 27.94 -21.59 180)
					(length 2.54)
					(name "MDIP0")
					(number "1")
				)
				(pin bidirectional line
					(at 27.94 -19.05 180)
					(length 2.54)
					(name "MDIN0")
					(number "2")
				)
				(pin power_in line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "AVDD10")
					(number "3")
				)
				(pin bidirectional line
					(at 27.94 -26.67 180)
					(length 2.54)
					(name "MDIP1")
					(number "4")
				)
				(pin bidirectional line
					(at 27.94 -24.13 180)
					(length 2.54)
					(name "MDIN1")
					(number "5")
				)
				(pin bidirectional line
					(at 27.94 -31.75 180)
					(length 2.54)
					(name "MDIP2")
					(number "6")
				)
				(pin bidirectional line
					(at 27.94 -29.21 180)
					(length 2.54)
					(name "MDIN2")
					(number "7")
				)
				(pin power_in line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "AVDD10_1")
					(number "8")
				)
				(pin bidirectional line
					(at 27.94 -36.83 180)
					(length 2.54)
					(name "MDIP3")
					(number "9")
				)
				(pin bidirectional line
					(at 27.94 -34.29 180)
					(length 2.54)
					(name "MDIN3")
					(number "10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDD33_1")
					(number "11")
				)
				(pin open_collector line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLKREQB")
					(number "12")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "HSIP")
					(number "13")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "HSIN")
					(number "14")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "REFCLK_P")
					(number "15")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "REFCLK_N")
					(number "16")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 2.54)
					(name "HSOP")
					(number "17")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "HSON")
					(number "18")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PERSTB")
					(number "19")
				)
				(pin open_collector line
					(at 0 -43.18 0)
					(length 2.54)
					(name "ISOLATEB")
					(number "20")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "LANWAKEB")
					(number "21")
				)
				(pin power_in line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "DVDD10")
					(number "22")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDREG")
					(number "23")
				)
				(pin output line
					(at 27.94 0 180)
					(length 2.54)
					(name "REGOUT")
					(number "24")
				)
				(pin output line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "LED2")
					(number "25")
				)
				(pin output line
					(at 27.94 -45.72 180)
					(length 2.54)
					(name "LED1/GPO")
					(number "26")
				)
				(pin output line
					(at 27.94 -43.18 180)
					(length 2.54)
					(name "LED0")
					(number "27")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "CKXTAL1")
					(number "28")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "CKXTAL2")
					(number "29")
				)
				(pin power_in line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "AVD10_2")
					(number "30")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "RSET")
					(number "31")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVDD33_2")
					(number "32")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
