(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RTL8211FDI-CG"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RTL8211FDI-CG"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RTL8211FDI-CG"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/C692886.pdf"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Integrated 10/100/1000M Ethernet precision transceiver"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RTL8211FDI-CG"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Realtek"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, ETHERNET, PCIE, SMT, TRANSCEIVER, PHY"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RTL8211FDI-CG_0_1")
			(symbol "RTL8211FDI-CG_1_1"
				(text "RGMII"
					(at 12.7 -46.99 900)
				)
				(text "MDI"
					(at 20.32 -26.67 900)
				)
				(pin bidirectional line
					(at 31.75 -17.78 180)
					(length 2.54)
					(name "MDIP0")
					(number "1")
				)
				(pin bidirectional line
					(at 31.75 -20.32 180)
					(length 2.54)
					(name "MDIN0")
					(number "2")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "AVDD10")
					(number "3")
				)
				(pin bidirectional line
					(at 31.75 -22.86 180)
					(length 2.54)
					(name "MDIP1")
					(number "4")
				)
				(pin bidirectional line
					(at 31.75 -25.4 180)
					(length 2.54)
					(name "MDIN1")
					(number "5")
				)
				(pin bidirectional line
					(at 31.75 -27.94 180)
					(length 2.54)
					(name "MDIP2")
					(number "6")
				)
				(pin bidirectional line
					(at 31.75 -30.48 180)
					(length 2.54)
					(name "MDIN2")
					(number "7")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "AVDD10")
					(number "8")
				)
				(pin bidirectional line
					(at 31.75 -33.02 180)
					(length 2.54)
					(name "MDIP3")
					(number "9")
				)
				(pin bidirectional line
					(at 31.75 -35.56 180)
					(length 2.54)
					(name "MDIN3")
					(number "10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDD33")
					(number "11")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "~{PHYRST}")
					(number "12")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "MDC")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "MDIO")
					(number "14")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "TXD3")
					(number "15")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "TXD2")
					(number "16")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "TXD1")
					(number "17")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "TXD0")
					(number "18")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "TXCTL")
					(number "19")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TXC")
					(number "20")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DVDD10")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "RXD3")
					(number "22")
					(alternate "PHYAD0" passive line)
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "RXD2")
					(number "23")
					(alternate "PLLOFF" passive line)
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "RXD1")
					(number "24")
					(alternate "TXDLY" passive line)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "RXD0")
					(number "25")
					(alternate "RXDLY" passive line)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "RXCTL")
					(number "26")
					(alternate "PHYAD2" passive line)
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "RXC")
					(number "27")
					(alternate "PHYAD1" passive line)
				)
				(pin passive line
					(at 31.75 0 180)
					(length 2.54)
					(name "DVDD_RG")
					(number "28")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "DVDD33")
					(number "29")
				)
				(pin power_out line
					(at 31.75 -2.54 180)
					(length 2.54)
					(name "LDO_OUT")
					(number "30")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{INT}")
					(number "31")
					(alternate "~{PME}" passive line)
				)
				(pin bidirectional line
					(at 31.75 -40.64 180)
					(length 2.54)
					(name "LED0")
					(number "32")
					(alternate "CFG_EXT" passive line)
				)
				(pin bidirectional line
					(at 31.75 -43.18 180)
					(length 2.54)
					(name "LED1")
					(number "33")
					(alternate "CFG_LDO0" passive line)
				)
				(pin bidirectional line
					(at 31.75 -45.72 180)
					(length 2.54)
					(name "LED2")
					(number "34")
					(alternate "CFG_LDO1" passive line)
				)
				(pin output line
					(at 31.75 -50.8 180)
					(length 2.54)
					(name "CLKOUT")
					(number "35")
				)
				(pin input line
					(at 31.75 -53.34 180)
					(length 2.54)
					(name "XTAL_IN")
					(number "36")
				)
				(pin output line
					(at 31.75 -55.88 180)
					(length 2.54)
					(name "XTAL_OUT")
					(number "37")
					(alternate "EXT_CLK" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "AVDD10")
					(number "38")
				)
				(pin output line
					(at 31.75 -60.96 180)
					(length 2.54)
					(name "RSET")
					(number "39")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "AVDD33")
					(number "40")
				)
				(pin power_in line
					(at 31.75 -66.04 180)
					(length 2.54)
					(name "GND")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
