(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RTL8211FS-CG"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RTL8211FS-CG"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RTL8211FS-CG"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2207051600_Realtek-Semicon-RTL8211FS-CG_C2844012.pdf"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "INTEGRATED 10/100/1000M ETHERNET PRECISION TRANSCEIVER"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RTL8211FS-CG"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Realtek"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, ETHERNET, PCIE, SMT, TRANSCEIVER, PHY"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RTL8211FS-CG_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "AVDD33")
					(number "1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDD10")
					(number "4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "AVDD10")
					(number "9")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD33")
					(number "12")
				)
				(pin input line
					(at 31.75 -10.16 180)
					(length 2.54)
					(name "PHYRSTB")
					(number "13")
				)
				(pin input line
					(at 31.75 -12.7 180)
					(length 2.54)
					(name "MDC")
					(number "14")
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "MDIO")
					(number "15")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DVDD10")
					(number "22")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DVDD_RG")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD33")
					(number "30")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DVDD33")
					(number "30")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VDD_REG")
					(number "31")
				)
				(pin power_out line
					(at 31.75 0 180)
					(length 2.54)
					(name "REG_OUT")
					(number "32")
				)
				(pin bidirectional line
					(at 31.75 -30.48 180)
					(length 2.54)
					(name "PTP_CLKI_N")
					(number "33")
					(alternate "CFG_EXT" passive line)
					(alternate "GPIO0" passive line)
				)
				(pin bidirectional line
					(at 31.75 -33.02 180)
					(length 2.54)
					(name "INTB")
					(number "34")
					(alternate "CFG_EXT" passive line)
					(alternate "GPIO1" passive line)
					(alternate "PMEB" passive line)
				)
				(pin bidirectional line
					(at 31.75 -20.32 180)
					(length 2.54)
					(name "LED0")
					(number "35")
					(alternate "CFG_EXT" passive line)
				)
				(pin bidirectional line
					(at 31.75 -22.86 180)
					(length 2.54)
					(name "LED1")
					(number "36")
					(alternate "CFG_LDO0" passive line)
				)
				(pin bidirectional line
					(at 31.75 -25.4 180)
					(length 2.54)
					(name "LED2")
					(number "37")
					(alternate "CFG_LDO1" passive line)
				)
				(pin output line
					(at 31.75 -5.08 180)
					(length 2.54)
					(name "CLKOUT")
					(number "44")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "XTAL_IN")
					(number "45")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "XTAL_OUT")
					(number "46")
					(alternate "EXT_CLK" passive line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "AVDD10")
					(number "47")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RSET")
					(number "48")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 2.54)
					(name "GND")
					(number "49")
				)
			)
			(symbol "RTL8211FS-CG_2_1"
				(text "RGMII"
					(at 5.08 2.54 0)
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXD3")
					(number "16")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TXD2")
					(number "17")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "TXD1")
					(number "18")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "TXD0")
					(number "19")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TXCTL")
					(number "20")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "TXC")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RXD3")
					(number "23")
					(alternate "PHYAD0" passive line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RXD2")
					(number "24")
					(alternate "PLLOFF" passive line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "RXD1")
					(number "25")
					(alternate "TXDLY" passive line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RXD0")
					(number "26")
					(alternate "RXDLY" passive line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "RXCTL")
					(number "27")
					(alternate "PHYAD2" passive line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RXC")
					(number "28")
					(alternate "PHYAD1" passive line)
				)
			)
			(symbol "RTL8211FS-CG_3_1"
				(text "SGMII"
					(at 6.35 2.54 0)
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "HSIP")
					(number "38")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "HSIN")
					(number "39")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 2.54)
					(name "HSOP")
					(number "40")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "HSON")
					(number "41")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "HSOP_CLK")
					(number "42")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "HSON_CLK")
					(number "43")
				)
			)
			(symbol "RTL8211FS-CG_4_1"
				(text "MDI"
					(at 4.445 2.54 0)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "MDIP0")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "MDIN0")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "MDIP1")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "MDIN1")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "MDIP2")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "MDIN2")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "MDIP3")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "MDIN3")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
