(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "S25FL128LAGNFA010"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "S25FL128LAGNFA010"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "S25FL128LAGNFA010"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-S25FL256L_S25FL128L_256-MB_(32-MB)_128-MB_(16-MB)_3.0_V_FL-L_FLASH_MEMORY-DataSheet-v09_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ed40e335224"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FLASH - NOR Memory IC 128Mbit SPI - Quad I/O, QPI 133 MHz 8-WSON (5x6)"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Cypress Semiconductor"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "S25FL128LAGNFA010"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "S25FL128LAGNFA010_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "*CS")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SO/IO1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "*WP/IO2")
					(number "3")
				)
				(pin power_in line
					(at 19.05 -17.78 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SI/IO0")
					(number "5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SCK")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "*HOLD/IO3")
					(number "7")
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin unspecified line
					(at 0 -12.7 0)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
