(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "S25FL128SAGNFI000"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "S25FL128SAGNFI000"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "S25FL128SAGNFI000"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/2309615.pdf"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Flash Memory, MirrorBit Eclipse Architecture, Serial NOR, 128 Mbit, 16M x 8bit, SPI, WSON, 8 Pins"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "S25FL128SAGNFI000"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Cypress Semiconductor"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, FLASH, SPI, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "S25FL128SAGNFI000_1_1"
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SO/IO1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{WP}/IO2")
					(number "3")
				)
				(pin power_in line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "V_{SS}")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SI/IO0")
					(number "5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCK")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{HOLD}/IO3")
					(number "7")
				)
				(pin power_in line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "V_{CC}")
					(number "8")
				)
				(pin no_connect line
					(at 17.78 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
