(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "S25FL256SAG_SOIC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "S25FL256SAG_SOIC"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "S25FL256SAG_SOIC"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/196/Infineon_S25FL512S_512_Mb__64_MB__3_0_V_SPI_Flash_-3107475.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NOR Flash"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "S25FL512SAGMFVR10"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, FLASH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "S25FL256SAG_SOIC_1_1"
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "~{HOLD/IO3}")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin passive line
					(at 19.05 -6.35 180)
					(length 2.54)
					(hide yes)
					(name "DNU")
					(number "4")
				)
				(pin passive line
					(at 19.05 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "DNU")
					(number "5")
				)
				(pin no_connect line
					(at 19.05 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "6")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "~{CS}")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "SO/IO1")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "~{WP/IO2}")
					(number "9")
				)
				(pin power_in line
					(at 21.59 -19.05 180)
					(length 2.54)
					(name "VSS")
					(number "10")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "DNU")
					(number "11")
				)
				(pin passive line
					(at 19.05 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "DNU")
					(number "12")
				)
				(pin no_connect line
					(at 19.05 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin bidirectional line
					(at 21.59 0 180)
					(length 2.54)
					(name "VIO")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SI/IO0")
					(number "15")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SCK")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
