(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "S28HS512TGABHM010"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "S28HS512TGABHM010"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "S28HS512TGABHM010"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/3/70/1/8HS01GT_S28HL512T_S28HL01GT_512MB_1GB_SEMPER_TM_FLASH_OCTAL_INTERFACE_1_8V_3-DataSheet-v68_00-EN.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NOR Flash 512Mb, 64M x 8bit, 1.8V, 200MHz, 24-ball TFBGA, RoHS"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Infineon"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "S28HS512TGABHM010"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, FLASH, HYPERBUS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "S28HS512TGABHM010_1_1"
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RFU1")
					(number "A2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RFU4")
					(number "A3")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{RESET}")
					(number "A4")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{INT}")
					(number "A5")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RFU5")
					(number "B1")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "CLK")
					(number "B2")
				)
				(pin power_in line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "VSS")
					(number "B3")
				)
				(pin power_in line
					(at 30.48 0 180)
					(length 2.54)
					(name "VCC")
					(number "B4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RFU2")
					(number "B5")
				)
				(pin power_in line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "VSSQ")
					(number "C1")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{CS}")
					(number "C2")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DS")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DQ2")
					(number "C4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RFU3")
					(number "C5")
				)
				(pin power_in line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "VCCQ")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DQ1")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DQ0")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "DQ3")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "DQ4")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "DQ7")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "DQ6")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "DQ5")
					(number "E3")
				)
				(pin power_in line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "VCCQ")
					(number "E4")
				)
				(pin power_in line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "VSSQ")
					(number "E5")
				)
			)
			(embedded_fonts no)
		)
)
