(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SC18IS602BIPW"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SC18IS602BIPW"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SC18IS602BIPW"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC18IS602B.pdf"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I²C Controller SPI Interface 16-TSSOP"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SC18IS602BIPW"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, I2C, SPI, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SC18IS602BIPW_1_1"
				(pin bidirectional line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "GPIO0/~{SS0}")
					(number "1")
				)
				(pin bidirectional line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "GPIO1/~{SS1}")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "V_{SS}")
					(number "4")
				)
				(pin input line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "MISO")
					(number "5")
				)
				(pin output line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "MOSI")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SDA")
					(number "7")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCL")
					(number "8")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{INT}")
					(number "9")
				)
				(pin bidirectional line
					(at 27.94 -20.32 180)
					(length 2.54)
					(name "GPIO2/~{SS2}")
					(number "10")
				)
				(pin output line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "SCLK")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD}")
					(number "12")
				)
				(pin bidirectional line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "GPIO3/~{SS3}")
					(number "13")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A0")
					(number "14")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A1")
					(number "15")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A2")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
