(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SC606T"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 69.85 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SC606T"
				(at 69.85 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SC606T"
				(at 69.85 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.quectel.com/product/lte-sc606t-smart-module-series"
				(at 69.85 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Qualcomm® octa-core ARM Cortex-A53 64-bit CPU + AdrenoTM 506 GPU"
				(at 69.85 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Quectel"
				(at 69.85 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SC606T-WF"
				(at 69.85 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 69.85 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 69.85 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SC606T_1_0"
				(pin input clock
					(at 0 0 0)
					(length 3.81)
					(name "CSI2_CLK_P")
					(number "77")
				)
				(pin input inverted_clock
					(at 0 -2.54 0)
					(length 3.81)
					(name "CSI2_CLK_N")
					(number "78")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "CSI2_LN0_P")
					(number "79")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "CSI2_LN0_N")
					(number "80")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "CSI2_LN1_P")
					(number "81")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "CSI2_LN1_N")
					(number "82")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "CSI2_LN2_P")
					(number "83")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "CSI2_LN2_N")
					(number "84")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "CSI2_LN3_P")
					(number "85")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "CSI2_LN3_N")
					(number "86")
				)
				(pin input clock
					(at 0 -27.94 0)
					(length 3.81)
					(name "CSI0_CLK_P")
					(number "88")
				)
				(pin input inverted_clock
					(at 0 -30.48 0)
					(length 3.81)
					(name "CSI0_CLK_N")
					(number "89")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "CSI0_LN0_P")
					(number "90")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "CSI0_LN0_N")
					(number "91")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "CSI0_LN1_P")
					(number "92")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "CSI0_LN1_N")
					(number "93")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "CSI0_LN2_P")
					(number "94")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "CSI0_LN2_N")
					(number "95")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "CSI0_LN3_P")
					(number "96")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 3.81)
					(name "CSI0_LN3_N")
					(number "97")
				)
				(pin output clock
					(at 43.18 -27.94 180)
					(length 3.81)
					(name "DSI1_CLK_P")
					(number "102")
				)
				(pin output inverted_clock
					(at 43.18 -30.48 180)
					(length 3.81)
					(name "DSI1_CLK_N")
					(number "103")
				)
				(pin output line
					(at 43.18 -33.02 180)
					(length 3.81)
					(name "DSI1_LN0_P")
					(number "104")
				)
				(pin output line
					(at 43.18 -35.56 180)
					(length 3.81)
					(name "DSI1_LN0_N")
					(number "105")
				)
				(pin output line
					(at 43.18 -38.1 180)
					(length 3.81)
					(name "DSI1_LN1_P")
					(number "106")
				)
				(pin output line
					(at 43.18 -40.64 180)
					(length 3.81)
					(name "DSI1_LN1_N")
					(number "107")
				)
				(pin output line
					(at 43.18 -43.18 180)
					(length 3.81)
					(name "DSI1_LN2_P")
					(number "108")
				)
				(pin output line
					(at 43.18 -45.72 180)
					(length 3.81)
					(name "DSI1_LN2_N")
					(number "109")
				)
				(pin output line
					(at 43.18 -48.26 180)
					(length 3.81)
					(name "DSI1_LN3_P")
					(number "110")
				)
				(pin output line
					(at 43.18 -50.8 180)
					(length 3.81)
					(name "DSI1_LN3_N")
					(number "111")
				)
				(pin output clock
					(at 43.18 0 180)
					(length 3.81)
					(name "DSI0_CLK_P")
					(number "115")
				)
				(pin output inverted_clock
					(at 43.18 -2.54 180)
					(length 3.81)
					(name "DSI0_CLK_N")
					(number "116")
				)
				(pin output line
					(at 43.18 -5.08 180)
					(length 3.81)
					(name "DSI0_LN0_P")
					(number "117")
				)
				(pin output line
					(at 43.18 -7.62 180)
					(length 3.81)
					(name "DSI0_LN0_N")
					(number "118")
				)
				(pin output line
					(at 43.18 -10.16 180)
					(length 3.81)
					(name "DSI0_LN1_P")
					(number "119")
				)
				(pin output line
					(at 43.18 -12.7 180)
					(length 3.81)
					(name "DSI0_LN1_N")
					(number "120")
				)
				(pin output line
					(at 43.18 -15.24 180)
					(length 3.81)
					(name "DSI0_LN2_P")
					(number "121")
				)
				(pin output line
					(at 43.18 -17.78 180)
					(length 3.81)
					(name "DSI0_LN2_N")
					(number "122")
				)
				(pin output line
					(at 43.18 -20.32 180)
					(length 3.81)
					(name "DSI0_LN3_P")
					(number "123")
				)
				(pin output line
					(at 43.18 -22.86 180)
					(length 3.81)
					(name "DSI0_LN3_N")
					(number "124")
				)
				(pin input clock
					(at 0 -55.88 0)
					(length 3.81)
					(name "CSI1_CLK_P")
					(number "183")
				)
				(pin input inverted_clock
					(at 0 -58.42 0)
					(length 3.81)
					(name "CSI1_CLK_N")
					(number "184")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 3.81)
					(name "CSI1_LN0_P")
					(number "185")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 3.81)
					(name "CSI1_LN0_N")
					(number "186")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "CSI1_LN1_P")
					(number "187")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 3.81)
					(name "CSI1_LN1_N")
					(number "188")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 3.81)
					(name "CSI1_LN2_P")
					(number "189")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "CSI1_LN2_N")
					(number "190")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 3.81)
					(name "CSI1_LN3_P")
					(number "191")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 3.81)
					(name "CSI1_LN3_N")
					(number "192")
				)
			)
			(symbol "SC606T_2_0"
				(text "Earpiece"
					(at 16.51 -31.75 0)
				)
				(text "Speaker"
					(at 16.51 -39.37 0)
				)
				(text "Microphone"
					(at 19.05 -6.35 900)
				)
				(text "Headphone"
					(at 19.05 -21.59 900)
				)
				(text "Line"
					(at 19.05 -46.99 900)
				)
				(text "(U)SIM1"
					(at 19.05 -58.42 900)
				)
				(text "(U)SIM2"
					(at 19.05 -73.66 900)
				)
				(text "SDIO/SD"
					(at 19.05 -93.98 900)
				)
				(text "SPI"
					(at 19.05 -113.03 0)
				)
				(text "LCD"
					(at 22.86 -32.385 0)
				)
				(text "CAM"
					(at 22.86 -54.61 0)
				)
				(text "Others"
					(at 22.86 -81.28 0)
				)
				(text "Key"
					(at 22.86 -99.06 0)
				)
				(text "Sensor I^{2}C"
					(at 22.86 -106.68 0)
				)
				(text "FP"
					(at 24.13 -3.81 0)
				)
				(text "RF"
					(at 24.13 -17.78 0)
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 3.81)
					(name "ANT_MAIN")
					(number "19")
				)
				(pin input line
					(at 43.18 -101.6 180)
					(length 3.81)
					(name "PWRKEY")
					(number "39")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "MIC1_P")
					(number "44")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "MIC1_N")
					(number "45")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "MIC2_P")
					(number "46")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "HS_DET")
					(number "48")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 3.81)
					(name "HPH_L")
					(number "49")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "HPH_REF")
					(number "50")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 3.81)
					(name "HPH_R")
					(number "51")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "EAR_N")
					(number "52")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 3.81)
					(name "EAR_P")
					(number "53")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "SPK_N")
					(number "54")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 3.81)
					(name "SPK_P")
					(number "55")
				)
				(pin input line
					(at 43.18 -88.9 180)
					(length 3.81)
					(name "USB_BOOT")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 3.81)
					(name "SPI_CS")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 3.81)
					(name "SPI_CLK")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 3.81)
					(name "SPI_MOSI")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 3.81)
					(name "SPI_MISO")
					(number "61")
				)
				(pin power_out line
					(at 0 -83.82 0)
					(length 3.81)
					(name "SD_LDO11")
					(number "63")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "SD_DET")
					(number "64")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "SD_DATA3")
					(number "65")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "SD_DATA2")
					(number "66")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "SD_DATA1")
					(number "67")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 3.81)
					(name "SD_DATA0")
					(number "68")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 3.81)
					(name "SD_CMD")
					(number "69")
				)
				(pin output clock
					(at 0 -104.14 0)
					(length 3.81)
					(name "SD_CLK")
					(number "70")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 3.81)
					(name "SCAM_PWDN")
					(number "71")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 3.81)
					(name "SCAM_RST")
					(number "72")
				)
				(pin bidirectional line
					(at 43.18 -44.45 180)
					(length 3.81)
					(name "MCAM_PWDN")
					(number "73")
				)
				(pin bidirectional line
					(at 43.18 -46.99 180)
					(length 3.81)
					(name "MCAM_RST")
					(number "74")
				)
				(pin bidirectional line
					(at 43.18 -41.91 180)
					(length 3.81)
					(name "MCAM_MCLK")
					(number "99")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 3.81)
					(name "SCAM_MCLK")
					(number "100")
				)
				(pin output line
					(at 43.18 -36.83 180)
					(length 3.81)
					(name "LCD1_RST")
					(number "113")
				)
				(pin input line
					(at 43.18 -34.29 180)
					(length 3.81)
					(name "LCD1_TE")
					(number "114")
				)
				(pin input line
					(at 43.18 -27.94 180)
					(length 3.81)
					(name "LCD0_TE")
					(number "126")
				)
				(pin output line
					(at 43.18 -30.48 180)
					(length 3.81)
					(name "LCD0_RST")
					(number "127")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 3.81)
					(name "ANT_WIFI/BT")
					(number "129")
				)
				(pin open_collector clock
					(at 43.18 -113.03 180)
					(length 3.81)
					(name "SENSOR_I2C_SCL")
					(number "131")
				)
				(pin open_collector line
					(at 43.18 -110.49 180)
					(length 3.81)
					(name "SENSOR_I2C_SDA")
					(number "132")
				)
				(pin input line
					(at 43.18 -15.24 180)
					(length 3.81)
					(name "ANT_GNSS")
					(number "134")
				)
				(pin power_out line
					(at 0 -53.34 0)
					(length 3.81)
					(name "USIM1_VDD")
					(number "141")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "USIM1_DATA")
					(number "142")
				)
				(pin output clock
					(at 0 -58.42 0)
					(length 3.81)
					(name "USIM1_CLK")
					(number "143")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 3.81)
					(name "USIM1_RST")
					(number "144")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 3.81)
					(name "USIM1_DET")
					(number "145")
				)
				(pin input line
					(at 43.18 -96.52 180)
					(length 3.81)
					(name "VOL_UP")
					(number "146")
				)
				(pin input line
					(at 43.18 -99.06 180)
					(length 3.81)
					(name "VOL_DOWN")
					(number "147")
				)
				(pin input line
					(at 43.18 -17.78 180)
					(length 3.81)
					(name "ANT_DRX")
					(number "149")
				)
				(pin input line
					(at 43.18 -74.93 180)
					(length 3.81)
					(name "PMU_MPP2")
					(number "151")
				)
				(pin output line
					(at 43.18 -72.39 180)
					(length 3.81)
					(name "PMU_MPP4")
					(number "152")
				)
				(pin power_out line
					(at 0 -10.16 0)
					(length 3.81)
					(name "MIC_BIAS")
					(number "167")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "MIC_GND")
					(number "168")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "MIC3_P")
					(number "169")
				)
				(pin power_out line
					(at 0 -86.36 0)
					(length 3.81)
					(name "SD_LDO12")
					(number "179")
				)
				(pin bidirectional line
					(at 43.18 -62.23 180)
					(length 3.81)
					(name "DCAM_RST")
					(number "180")
				)
				(pin bidirectional line
					(at 43.18 -64.77 180)
					(length 3.81)
					(name "DCAM_PWDN")
					(number "181")
				)
				(pin bidirectional line
					(at 43.18 -59.69 180)
					(length 3.81)
					(name "DCAM_MCLK")
					(number "194")
				)
				(pin output line
					(at 43.18 -91.44 180)
					(length 3.81)
					(name "GNSS_LNA_EN")
					(number "202")
				)
				(pin bidirectional line
					(at 43.18 0 180)
					(length 3.81)
					(name "FP_SPI_CS")
					(number "203")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 3.81)
					(name "USIM2_RST")
					(number "207")
				)
				(pin output clock
					(at 0 -73.66 0)
					(length 3.81)
					(name "USIM2_CLK")
					(number "208")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "USIM2_DATA")
					(number "209")
				)
				(pin power_out line
					(at 0 -68.58 0)
					(length 3.81)
					(name "USIM2_VDD")
					(number "210")
				)
				(pin bidirectional line
					(at 43.18 -82.55 180)
					(length 3.81)
					(name "S2A")
					(number "211")
				)
				(pin bidirectional line
					(at 43.18 -77.47 180)
					(length 3.81)
					(name "S1A")
					(number "215")
				)
				(pin bidirectional line
					(at 43.18 -80.01 180)
					(length 3.81)
					(name "S1B")
					(number "216")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 3.81)
					(name "LINE_OUT_P")
					(number "227")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 3.81)
					(name "LINE_OUT_N")
					(number "228")
				)
				(pin bidirectional line
					(at 43.18 -85.09 180)
					(length 3.81)
					(name "S2B")
					(number "233")
				)
				(pin bidirectional line
					(at 43.18 -67.31 180)
					(length 3.81)
					(name "CAM4_MCLK")
					(number "236")
				)
				(pin input line
					(at 43.18 -22.86 180)
					(length 3.81)
					(name "FM_ANT")
					(number "244")
				)
			)
			(symbol "SC606T_2_1"
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 3.81)
					(name "FP_SPI_MOSI")
					(number "249")
				)
				(pin bidirectional clock
					(at 43.18 -5.08 180)
					(length 3.81)
					(name "FP_SPI_CLK")
					(number "250")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 3.81)
					(name "FP_SPI_MISO")
					(number "251")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "USIM2_DET")
					(number "256")
				)
			)
			(symbol "SC606T_3_0"
				(text "TP0"
					(at 20.32 -3.81 900)
				)
				(text "TP1"
					(at 20.32 -16.51 900)
				)
				(text "UART"
					(at 20.32 -34.29 900)
				)
				(text "Camera I^{2}C"
					(at 22.86 1.27 0)
				)
				(text "USB"
					(at 22.86 -15.24 0)
				)
				(pin output line
					(at 0 -25.4 0)
					(length 3.81)
					(name "UART2_TXD")
					(number "5")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "UART2_RXD")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "UART4_TXD")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "UART4_RXD")
					(number "8")
				)
				(pin output line
					(at 43.18 -25.4 180)
					(length 3.81)
					(name "USB_ID")
					(number "30")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 3.81)
					(name "USB_DP")
					(number "32")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 3.81)
					(name "USB_DM")
					(number "33")
				)
				(pin input line
					(at 43.18 -17.78 180)
					(length 3.81)
					(name "USB_VBUS")
					(number "41")
				)
				(pin passive line
					(at 43.18 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "USB_VBUS")
					(number "42")
				)
				(pin open_collector clock
					(at 43.18 -2.54 180)
					(length 3.81)
					(name "CAM_I2C_SCL")
					(number "75")
				)
				(pin open_collector line
					(at 43.18 -5.08 180)
					(length 3.81)
					(name "CAM_I2C_SDA")
					(number "76")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "TP1_RST")
					(number "136")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "TP1_INT")
					(number "137")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "TP0_RST")
					(number "138")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "TP0_INT")
					(number "139")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 3.81)
					(name "TP0_I2C_SCL")
					(number "140")
				)
				(pin input line
					(at 43.18 -27.94 180)
					(length 3.81)
					(name "USB_SS_RX_P")
					(number "171")
				)
				(pin input line
					(at 43.18 -30.48 180)
					(length 3.81)
					(name "USB_SS_RX_M")
					(number "172")
				)
				(pin output line
					(at 43.18 -33.02 180)
					(length 3.81)
					(name "USB_SS_TX_P")
					(number "174")
				)
				(pin output line
					(at 43.18 -35.56 180)
					(length 3.81)
					(name "USB_SS_TX_M")
					(number "175")
				)
				(pin open_collector clock
					(at 43.18 -8.89 180)
					(length 3.81)
					(name "DCAM_I2C_SCL")
					(number "196")
				)
				(pin open_collector line
					(at 43.18 -11.43 180)
					(length 3.81)
					(name "DCAM_I2C_SDA")
					(number "197")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "UART5_RXD")
					(number "198")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "UART5_TXD")
					(number "199")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TP1_I2C_SDA")
					(number "204")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 3.81)
					(name "TP1_I2C_SCL")
					(number "205")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "TP0_I2C_SDA")
					(number "206")
				)
				(pin input line
					(at 43.18 -38.1 180)
					(length 3.81)
					(name "USBC_CC2")
					(number "223")
				)
				(pin input line
					(at 43.18 -40.64 180)
					(length 3.81)
					(name "USBC_CC1")
					(number "224")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 3.81)
					(name "USB_SS_SEL")
					(number "226")
				)
			)
			(symbol "SC606T_3_1"
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "UART5_RTS")
					(number "245")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "UART5_CTS")
					(number "246")
				)
			)
			(symbol "SC606T_4_0"
				(text "GPIO"
					(at 16.51 -20.32 0)
				)
				(text "GRFC"
					(at 16.51 -46.99 0)
				)
				(pin no_connect line
					(at 20.32 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "17")
				)
				(pin no_connect line
					(at 20.32 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "21")
				)
				(pin no_connect line
					(at 20.32 -34.29 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "22")
				)
				(pin no_connect line
					(at 20.32 -33.02 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "23")
				)
				(pin no_connect line
					(at 20.32 -31.75 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "24")
				)
				(pin no_connect line
					(at 20.32 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "25")
				)
				(pin no_connect line
					(at 20.32 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "26")
				)
				(pin no_connect line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "27")
				)
				(pin no_connect line
					(at 20.32 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "28")
				)
				(pin no_connect line
					(at 20.32 -25.4 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "29")
				)
				(pin no_connect line
					(at 20.32 -24.13 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "153")
				)
				(pin no_connect line
					(at 20.32 -22.86 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "154")
				)
				(pin no_connect line
					(at 20.32 -21.59 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "155")
				)
				(pin no_connect line
					(at 20.32 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "156")
				)
				(pin no_connect line
					(at 20.32 -19.05 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "157")
				)
				(pin no_connect line
					(at 20.32 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "158")
				)
				(pin no_connect line
					(at 20.32 -16.51 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "161")
				)
				(pin no_connect line
					(at 20.32 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "162")
				)
				(pin no_connect line
					(at 20.32 -13.97 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "164")
				)
				(pin no_connect line
					(at 20.32 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "165")
				)
				(pin no_connect line
					(at 20.32 -11.43 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "166")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "GPIO_98")
					(number "177")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "GPIO_99")
					(number "178")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "GPIO_3")
					(number "200")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "GPIO_2")
					(number "201")
				)
				(pin no_connect line
					(at 20.32 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "212")
				)
				(pin no_connect line
					(at 20.32 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "213")
				)
				(pin no_connect line
					(at 20.32 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "214")
				)
				(pin no_connect line
					(at 20.32 -6.35 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "217")
				)
				(pin no_connect line
					(at 20.32 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "218")
				)
				(pin no_connect line
					(at 20.32 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "222")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "GPIO_97")
					(number "229")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "GPIO_96")
					(number "230")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "GPIO_90")
					(number "231")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "GPIO_89")
					(number "232")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "GPIO_66")
					(number "234")
				)
				(pin no_connect line
					(at 20.32 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "235")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "GPIO_36")
					(number "237")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "GPIO_33")
					(number "238")
				)
				(pin no_connect line
					(at 20.32 -1.27 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "239")
				)
				(pin no_connect line
					(at 20.32 0 180)
					(length 3.81)
					(hide yes)
					(name "RESERVED")
					(number "240")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "GRFC_7")
					(number "241")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "GRFC_5")
					(number "242")
				)
			)
			(symbol "SC606T_4_1"
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "GPIO_1")
					(number "247")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "GPIO_0")
					(number "248")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "GPIO_42")
					(number "252")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "GPIO_43")
					(number "253")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "GPIO_44")
					(number "254")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "GPIO_45")
					(number "255")
				)
			)
			(symbol "SC606T_5_0"
				(pin power_out line
					(at 43.18 -10.16 180)
					(length 3.81)
					(name "VDD_RF")
					(number "1")
				)
				(pin passive line
					(at 43.18 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "VDD_RF")
					(number "2")
				)
				(pin power_in line
					(at 43.18 -35.56 180)
					(length 3.81)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin power_out line
					(at 0 0 0)
					(length 3.81)
					(name "LDO5_1P8")
					(number "9")
				)
				(pin power_out line
					(at 0 -5.08 0)
					(length 3.81)
					(name "LDO6_1P8")
					(number "10")
				)
				(pin power_out line
					(at 0 -10.16 0)
					(length 3.81)
					(name "LDO10_2P8")
					(number "11")
				)
				(pin power_out line
					(at 0 -15.24 0)
					(length 3.81)
					(name "LDO17_2P85")
					(number "12")
				)
				(pin power_out line
					(at 0 -20.32 0)
					(length 3.81)
					(name "LDO2_1P1")
					(number "13")
				)
				(pin power_out line
					(at 0 -25.4 0)
					(length 3.81)
					(name "LDO22_2P8")
					(number "14")
				)
				(pin power_out line
					(at 0 -30.48 0)
					(length 3.81)
					(name "LDO23_1P2")
					(number "15")
				)
				(pin power_in line
					(at 43.18 -30.48 180)
					(length 3.81)
					(name "VRTC")
					(number "16")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "18")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "20")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "31")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "34")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "35")
				)
				(pin power_in line
					(at 43.18 -20.32 180)
					(length 3.81)
					(name "VBAT")
					(number "36")
				)
				(pin passive line
					(at 43.18 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "VBAT")
					(number "37")
				)
				(pin passive line
					(at 43.18 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "VBAT")
					(number "38")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "40")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "43")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "56")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "62")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "87")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "98")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "101")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "112")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "125")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "128")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "130")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "133")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "135")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "148")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "150")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "159")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "160")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "163")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "170")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "173")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "176")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "182")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "193")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "195")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "219")
				)
				(pin power_out line
					(at 43.18 0 180)
					(length 3.81)
					(name "VPH_PWR")
					(number "220")
				)
				(pin passive line
					(at 43.18 0 180)
					(length 3.81)
					(hide yes)
					(name "VPH_PWR")
					(number "221")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "225")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "243")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "257")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "258")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "259")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "260")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "261")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "262")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "263")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "264")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "265")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "266")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "267")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "268")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "269")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "270")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "271")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "272")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "273")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "274")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "275")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "276")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "277")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "278")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "279")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "280")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "281")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "282")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "283")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "284")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "285")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "286")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "287")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "288")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "289")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "290")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "291")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "292")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "293")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "294")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "295")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "296")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "297")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "298")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "299")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "300")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "301")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "302")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "303")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "304")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "305")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "306")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "307")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "308")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "309")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "310")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "311")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "312")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "313")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "314")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "315")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "316")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "317")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "318")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "319")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "320")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "321")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "322")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "323")
				)
			)
			(embedded_fonts no)
		)
)
