(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SCANSTA112VS"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 49.53 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SCANSTA112VS"
				(at 49.53 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SCANSTA112VS"
				(at 49.53 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/SCANSTA112"
				(at 49.53 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Texas Instruments SCANSTA112VS/NOPB, Multiplexer Single 8 x 1 Multiplexer, 3  3.6 V, 100-Pin TQFP"
				(at 49.53 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SCANSTA112VS/NOPB"
				(at 49.53 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 49.53 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 49.53 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 49.53 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, JTAG, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SCANSTA112VS_1_1"
				(pin input line
					(at 0 -41.91 0)
					(length 3.81)
					(name "S_{0}")
					(number "1")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 3.81)
					(name "S_{1}")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "V_{CC}")
					(number "3")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 3.81)
					(name "S_{2}")
					(number "4")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 3.81)
					(name "S_{3}")
					(number "5")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 3.81)
					(name "S_{4}")
					(number "6")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 3.81)
					(name "S_{5}")
					(number "7")
				)
				(pin power_in line
					(at 30.48 -110.49 180)
					(length 3.81)
					(name "GND")
					(number "8")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 3.81)
					(name "S_{6}")
					(number "9")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 3.81)
					(name "S_{7}")
					(number "10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "ADDMASK")
					(number "11")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "TRANS")
					(number "12")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "13")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "~{OE}")
					(number "14")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 3.81)
					(name "LSP_{SEL0}")
					(number "15")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "LSP_{SEL1}")
					(number "16")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "LSP_{SEL2}")
					(number "17")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "18")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 3.81)
					(name "LSP_{SEL3}")
					(number "19")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 3.81)
					(name "LSP_{SEL4}")
					(number "20")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 3.81)
					(name "LSP_{SEL5}")
					(number "21")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 3.81)
					(name "LSP_{SEL6}")
					(number "22")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "23")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 3.81)
					(name "MPSEL_{B1/~{B0}}")
					(number "24")
					(alternate "MPSEL_{~{B0}}" input line)
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SB/~{S}")
					(number "25")
					(alternate "~{S}" input line)
				)
				(pin input line
					(at 0 -86.36 0)
					(length 3.81)
					(name "TDI_{B0}")
					(number "26")
				)
				(pin output line
					(at 0 -88.9 0)
					(length 3.81)
					(name "TDO_{B0}")
					(number "27")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin input line
					(at 0 -74.93 0)
					(length 3.81)
					(name "A0_{B0}")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "TCK_{B0}")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "~{TRST}_{B0}")
					(number "31")
				)
				(pin output line
					(at 0 -91.44 0)
					(length 3.81)
					(name "TMS_{B0}")
					(number "32")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "33")
				)
				(pin input line
					(at 0 -80.01 0)
					(length 3.81)
					(name "A1_{B0}")
					(number "34")
				)
				(pin output line
					(at 30.48 0 180)
					(length 3.81)
					(name "TRIST_{B0}")
					(number "35")
				)
				(pin output line
					(at 30.48 -13.97 180)
					(length 3.81)
					(name "Y0_{B0}")
					(number "36")
				)
				(pin output line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "Y1_{B0}")
					(number "37")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "38")
				)
				(pin input line
					(at 0 -100.33 0)
					(length 3.81)
					(name "TDI_{B1}")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 3.81)
					(name "TDO_{B1}")
					(number "40")
				)
				(pin input line
					(at 0 -77.47 0)
					(length 3.81)
					(name "A0_{B1}")
					(number "41")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 3.81)
					(name "TCK_{B1}")
					(number "42")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 3.81)
					(name "~{TRST}_{B1}")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 3.81)
					(name "TMS_{B1}")
					(number "45")
				)
				(pin output line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "Y1_{B1}")
					(number "46")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "TRIST_{B1}")
					(number "47")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "48")
				)
				(pin output line
					(at 30.48 -16.51 180)
					(length 3.81)
					(name "Y0_{B1}")
					(number "49")
				)
				(pin input line
					(at 0 -82.55 0)
					(length 3.81)
					(name "A1_{B1}")
					(number "50")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 3.81)
					(name "TLR_TRST")
					(number "51")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 3.81)
					(name "TLR_TRST_{6}")
					(number "52")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "53")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "~{RESET}")
					(number "54")
				)
				(pin input line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "TDI_{01}")
					(number "55")
				)
				(pin output line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "TDO_{01}")
					(number "56")
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 3.81)
					(name "TMS_{01}")
					(number "57")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "58")
				)
				(pin output line
					(at 30.48 -33.02 180)
					(length 3.81)
					(name "TCK_{01}")
					(number "59")
				)
				(pin output line
					(at 30.48 -35.56 180)
					(length 3.81)
					(name "~{TRST}_{01}")
					(number "60")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "TRIST_{01}")
					(number "61")
				)
				(pin output line
					(at 0 -71.12 0)
					(length 3.81)
					(name "Y1_{01}")
					(number "62")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "63")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "A1_{01}")
					(number "64")
				)
				(pin output line
					(at 0 -68.58 0)
					(length 3.81)
					(name "Y0_{01}")
					(number "65")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 3.81)
					(name "A0_{01}")
					(number "66")
				)
				(pin input line
					(at 30.48 -39.37 180)
					(length 3.81)
					(name "TDI_{02}")
					(number "67")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "68")
				)
				(pin output line
					(at 30.48 -41.91 180)
					(length 3.81)
					(name "TDO_{02}")
					(number "69")
				)
				(pin output line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "TMS_{02}")
					(number "70")
				)
				(pin output line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "TCK_{02}")
					(number "71")
				)
				(pin output line
					(at 30.48 -49.53 180)
					(length 3.81)
					(name "~{TRST}_{02}")
					(number "72")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "73")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "TRIST_{02}")
					(number "74")
				)
				(pin input line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "TDI_{03}")
					(number "75")
				)
				(pin output line
					(at 30.48 -55.88 180)
					(length 3.81)
					(name "TDO_{03}")
					(number "76")
				)
				(pin output line
					(at 30.48 -58.42 180)
					(length 3.81)
					(name "TMS_{03}")
					(number "77")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "78")
				)
				(pin output line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "~{TRST}_{03}")
					(number "79")
				)
				(pin output line
					(at 30.48 -60.96 180)
					(length 3.81)
					(name "TCK_{03}")
					(number "80")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "TRIST_{03}")
					(number "81")
				)
				(pin input line
					(at 30.48 -67.31 180)
					(length 3.81)
					(name "TDI_{04}")
					(number "82")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "83")
				)
				(pin output line
					(at 30.48 -69.85 180)
					(length 3.81)
					(name "TDO_{04}")
					(number "84")
				)
				(pin output line
					(at 30.48 -72.39 180)
					(length 3.81)
					(name "TMS_{04}")
					(number "85")
				)
				(pin output line
					(at 30.48 -74.93 180)
					(length 3.81)
					(name "TCK_{04}")
					(number "86")
				)
				(pin output line
					(at 30.48 -77.47 180)
					(length 3.81)
					(name "~{TRST}_{04}")
					(number "87")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "88")
				)
				(pin output line
					(at 30.48 -86.36 180)
					(length 3.81)
					(name "TMS_{05}")
					(number "89")
				)
				(pin output line
					(at 30.48 -83.82 180)
					(length 3.81)
					(name "TDO_{05}")
					(number "90")
				)
				(pin input line
					(at 30.48 -81.28 180)
					(length 3.81)
					(name "TDI_{05}")
					(number "91")
				)
				(pin output line
					(at 30.48 -88.9 180)
					(length 3.81)
					(name "TCK_{05}")
					(number "92")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "V_{CC}")
					(number "93")
				)
				(pin output line
					(at 30.48 -91.44 180)
					(length 3.81)
					(name "~{TRST}_{05}")
					(number "94")
				)
				(pin input line
					(at 30.48 -95.25 180)
					(length 3.81)
					(name "TDI_{06}")
					(number "95")
				)
				(pin output line
					(at 30.48 -97.79 180)
					(length 3.81)
					(name "TDO_{06}")
					(number "96")
				)
				(pin output line
					(at 30.48 -100.33 180)
					(length 3.81)
					(name "TMS_{06}")
					(number "97")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "98")
				)
				(pin output line
					(at 30.48 -102.87 180)
					(length 3.81)
					(name "TCK_{06}")
					(number "99")
				)
				(pin output line
					(at 30.48 -105.41 180)
					(length 3.81)
					(name "~{TRST}_{06}")
					(number "100")
				)
			)
			(embedded_fonts no)
		)
)
