(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SE050C1HQ1_Z01SCZ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SE050C1HQ1_Z01SCZ"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SE050C1HQ1_Z01SCZ"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/3/118/1/SE050-DATASHEET.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Security ICs / Authentication ICs"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SE050C1HQ1/Z01SCZ"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SE050C1HQ1_Z01SCZ_1_1"
				(pin passive line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "ISO_14443_LB")
					(number "1")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin bidirectional line
					(at 25.4 -11.43 180)
					(length 2.54)
					(name "ISO_7816_IO1")
					(number "3")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin open_collector line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SDA")
					(number "9")
				)
				(pin open_collector line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCL")
					(number "10")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "ENA")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{IN}")
					(number "12")
				)
				(pin input line
					(at 25.4 -8.89 180)
					(length 2.54)
					(name "ISO_7816_CLK")
					(number "13")
				)
				(pin input line
					(at 25.4 -6.35 180)
					(length 2.54)
					(name "~{ISO_7816_RST}")
					(number "14")
				)
				(pin power_out line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{OUT}")
					(number "15")
				)
				(pin input line
					(at 25.4 -13.97 180)
					(length 2.54)
					(name "ISO_7816_IO2")
					(number "16")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "ISO_14443_LA")
					(number "17")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "V_{CC}")
					(number "18")
				)
				(pin power_in line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "V_{SS}")
					(number "19")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin passive line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "EP")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
