(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RF_SI4703-C19-GM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RF_SI4703-C19-GM"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RF_SI4703-C19-GM"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si4702-03-C19.pdf"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF Receiver, MP3 Players, Notebook PCs, FM Radio, 76MHz to 108MHz, FM, 2.7V to 5.5V Supply, QFN-20"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI4703-C19-GM"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Silicon Labs"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RF_SI4703-C19-GM_1_1"
				(pin no_connect line
					(at 16.51 -13.97 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "FMIP")
					(number "2")
				)
				(pin power_in line
					(at 19.05 -17.78 180)
					(length 2.54)
					(name "RFGND")
					(number "3")
				)
				(pin passive line
					(at 19.05 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{RST}")
					(number "5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{SEN}")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SCLK")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SDIO")
					(number "8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RCLK")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIO")
					(number "10")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VD")
					(number "11")
				)
				(pin power_in line
					(at 19.05 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "12")
				)
				(pin output line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "ROUT")
					(number "13")
				)
				(pin output line
					(at 19.05 -10.16 180)
					(length 2.54)
					(name "LOUT")
					(number "14")
				)
				(pin passive line
					(at 19.05 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "15")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VA")
					(number "16")
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "GPIO3")
					(number "17")
				)
				(pin output line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "GPIO2")
					(number "18")
				)
				(pin output line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "GPIO1")
					(number "19")
				)
				(pin no_connect line
					(at 16.51 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin passive line
					(at 19.05 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
