(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SI52112-B6-GT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SI52112-B6-GT"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SI52112-B6-GT"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si52112-B5-B6.pdf"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Clock Generator, 100MHz, 2.97V to 3.63V, 2 Outputs, TSSOP-8"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI52112-B6-GT"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Skyworks Solutions"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SI52112-B6-GT_0_1")
			(symbol "SI52112-B6-GT_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "XOUT")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "XIN/CLKIN")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin output line
					(at 24.13 0 180)
					(length 2.54)
					(name "DIFF1")
					(number "5")
				)
				(pin output line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "~{DIFF1}")
					(number "6")
				)
				(pin output line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "DIFF2")
					(number "7")
				)
				(pin output line
					(at 24.13 -7.62 180)
					(length 2.54)
					(name "~{DIFF2}")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
