(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SI5338B-B-GM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 36.83 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SI5338B-B-GM"
				(at 36.83 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SI5338B-B-GM"
				(at 36.83 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.skyworksinc.com/en/application-pages/-/media/SkyWorks/SL/documents/public/data-sheets/Si5338.pdf"
				(at 36.83 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PLL Clock Generator 0.16MHz to 350MHz 24-Pin QFN EP"
				(at 36.83 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI5338B-B-GM"
				(at 36.83 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Skyworks Solutions"
				(at 36.83 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.83 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, CLOCK, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SI5338B-B-GM_0_0"
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "IN1/CLKIN")
					(number "1")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "IN2/CLKINB")
					(number "2")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "IN5/FDBK")
					(number "5")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "IN6/FDBKB")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "7")
				)
				(pin output line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "CLK3B")
					(number "9")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "CLK3A")
					(number "10")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDDO3")
					(number "11")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SCL")
					(number "12")
				)
				(pin output line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "CLK2B")
					(number "13")
				)
				(pin output line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "CLK2A")
					(number "14")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDO2")
					(number "15")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDO1")
					(number "16")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "CLK1B")
					(number "17")
				)
				(pin output line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "CLK1A")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SDA")
					(number "19")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDO0")
					(number "20")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "CLK0B")
					(number "21")
				)
				(pin output line
					(at 25.4 0 180)
					(length 2.54)
					(name "CLK0A")
					(number "22")
				)
				(pin power_in line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "RSVD_GND")
					(number "23")
				)
				(pin power_in line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "GND")
					(number "25")
				)
			)
			(symbol "SI5338B-B-GM_1_0"
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "IN3/CLKIN")
					(number "3")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "IN4/I2C_LSB")
					(number "4")
				)
				(pin open_collector line
					(at 0 -38.1 0)
					(length 2.54)
					(name "INTR")
					(number "8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
