(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SI5391A-A-GM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SI5391A-A-GM"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SI5391A-A-GM"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/472/si5391_datasheet-2507418.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Clock Generator IC 1GHz 1 64-VFQFN Exposed Pad"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI5391A-A-GM"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Skyworks Solutions"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, CLOCK, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SI5391A-A-GM_1_1"
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "IN1")
					(number "1")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "IN1B")
					(number "2")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "IN_SEL0")
					(number "3")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 2.54)
					(name "IN_SEL1")
					(number "4")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 2.54)
					(name "SYNCB")
					(number "5")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "RSTB")
					(number "6")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(name "X1")
					(number "7")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 2.54)
					(name "XA")
					(number "8")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 2.54)
					(name "XB")
					(number "9")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 2.54)
					(name "X2")
					(number "10")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 2.54)
					(name "OEB")
					(number "11")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "INTRB")
					(number "12")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDDA")
					(number "13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "IN2")
					(number "14")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "IN2B")
					(number "15")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "SCLK")
					(number "16")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "A1/SDO")
					(number "17")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "SDA/SDIO")
					(number "18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "A0/CSB")
					(number "19")
				)
				(pin passive line
					(at 22.86 -34.29 180)
					(length 2.54)
					(name "OUT0AB")
					(number "20")
				)
				(pin passive line
					(at 22.86 -31.75 180)
					(length 2.54)
					(name "OUT0A")
					(number "21")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(name "VDDO0")
					(number "22")
				)
				(pin passive line
					(at 22.86 -29.21 180)
					(length 2.54)
					(name "OUT0B")
					(number "23")
				)
				(pin passive line
					(at 22.86 -26.67 180)
					(length 2.54)
					(name "OUT0")
					(number "24")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(name "FDEC")
					(number "25")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "VDDO1")
					(number "26")
				)
				(pin passive line
					(at 22.86 -39.37 180)
					(length 2.54)
					(name "OUT1B")
					(number "27")
				)
				(pin passive line
					(at 22.86 -36.83 180)
					(length 2.54)
					(name "OUT1")
					(number "28")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "VDDO2")
					(number "29")
				)
				(pin passive line
					(at 22.86 -44.45 180)
					(length 2.54)
					(name "OUT2B")
					(number "30")
				)
				(pin passive line
					(at 22.86 -41.91 180)
					(length 2.54)
					(name "OUT2")
					(number "31")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "32")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "VDDO3")
					(number "33")
				)
				(pin passive line
					(at 22.86 -49.53 180)
					(length 2.54)
					(name "OUT3B")
					(number "34")
				)
				(pin passive line
					(at 22.86 -46.99 180)
					(length 2.54)
					(name "OUT3")
					(number "35")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "VDDO4")
					(number "36")
				)
				(pin passive line
					(at 22.86 -54.61 180)
					(length 2.54)
					(name "OUT4B")
					(number "37")
				)
				(pin passive line
					(at 22.86 -52.07 180)
					(length 2.54)
					(name "OUT4")
					(number "38")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "I2C_SEL")
					(number "39")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "VDDO5")
					(number "40")
				)
				(pin passive line
					(at 22.86 -59.69 180)
					(length 2.54)
					(name "OUT5B")
					(number "41")
				)
				(pin passive line
					(at 22.86 -57.15 180)
					(length 2.54)
					(name "OUT5")
					(number "42")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "VDDO6")
					(number "43")
				)
				(pin passive line
					(at 22.86 -64.77 180)
					(length 2.54)
					(name "OUT6B")
					(number "44")
				)
				(pin passive line
					(at 22.86 -62.23 180)
					(length 2.54)
					(name "OUT_6")
					(number "45")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "46")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 2.54)
					(name "LOLB")
					(number "47")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 2.54)
					(name "FINC")
					(number "48")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "VDDO7")
					(number "49")
				)
				(pin passive line
					(at 22.86 -69.85 180)
					(length 2.54)
					(name "OUT7B")
					(number "50")
				)
				(pin passive line
					(at 22.86 -67.31 180)
					(length 2.54)
					(name "OUT7")
					(number "51")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "VDDO8")
					(number "52")
				)
				(pin passive line
					(at 22.86 -74.93 180)
					(length 2.54)
					(name "OUT8B")
					(number "53")
				)
				(pin passive line
					(at 22.86 -72.39 180)
					(length 2.54)
					(name "OUT8")
					(number "54")
				)
				(pin passive line
					(at 22.86 -80.01 180)
					(length 2.54)
					(name "OUT9B")
					(number "55")
				)
				(pin passive line
					(at 22.86 -77.47 180)
					(length 2.54)
					(name "OUT9")
					(number "56")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "VDDO9")
					(number "57")
				)
				(pin passive line
					(at 22.86 -85.09 180)
					(length 2.54)
					(name "OUT9AB")
					(number "58")
				)
				(pin passive line
					(at 22.86 -82.55 180)
					(length 2.54)
					(name "OUT9A")
					(number "59")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "60")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 2.54)
					(name "FB_IN")
					(number "61")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 2.54)
					(name "FB_INB")
					(number "62")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "IN0")
					(number "63")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "IN0B")
					(number "64")
				)
				(pin passive line
					(at 0 -85.09 0)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
