(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SLB9645TT12"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SLB9645TT12"
				(at 34.29 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SLB9645TT12"
				(at 34.29 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-Data-sheet-SLB9645_1.2_Rev1.2-DS-v01_02-EN.pdf?fileId=5546d462689a790c016929d1c4074fdf"
				(at 34.29 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Security ICs / Authentication ICs"
				(at 34.29 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SLB9645TT12"
				(at 34.29 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 34.29 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SLB9645TT12_1_1"
				(pin open_collector line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SDA")
					(number "1")
				)
				(pin open_collector line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SCL")
					(number "2")
				)
				(pin no_connect line
					(at 17.78 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin passive line
					(at 20.32 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "5")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "~{DAVINT}")
					(number "6")
				)
				(pin input line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "PP")
					(number "7")
				)
				(pin no_connect line
					(at 17.78 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{RESET}")
					(number "9")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "10")
				)
				(pin power_in line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin no_connect line
					(at 17.78 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin no_connect line
					(at 17.78 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin no_connect line
					(at 17.78 -13.97 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin no_connect line
					(at 17.78 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin no_connect line
					(at 17.78 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin no_connect line
					(at 17.78 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "17")
				)
				(pin passive line
					(at 20.32 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "18")
				)
				(pin no_connect line
					(at 17.78 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "19")
				)
				(pin no_connect line
					(at 17.78 -6.35 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin no_connect line
					(at 17.78 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "21")
				)
				(pin no_connect line
					(at 17.78 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "22")
				)
				(pin no_connect line
					(at 12.7 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "23")
				)
				(pin no_connect line
					(at 11.43 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "24")
				)
				(pin passive line
					(at 20.32 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
				(pin no_connect line
					(at 10.16 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "26")
				)
				(pin no_connect line
					(at 8.89 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "27")
				)
				(pin no_connect line
					(at 7.62 0 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "28")
				)
			)
			(embedded_fonts no)
		)
)
